(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CrossLink_LIFCL-40-9BG256C"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CrossLink_LIFCL-40-9BG256C"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CrossLink_LIFCL-40-9BG256C"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.latticesemi.com/-/media/LatticeSemi/Documents/DataSheets/CrossLink/FPGA-DS-02007-2-1-CrossLink-Family-Data-Sheet.ashx?document_id=51662"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "CrossLink-NX™ Field Programmable Gate Array 256-LFBGA"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LIFCL-40-9BG256C"
				(at 53.34 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Lattice Semiconductor"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, FPGA, IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CrossLink_LIFCL-40-9BG256C_1_1"
				(text "BANK0"
					(at 40.64 -31.75 0)
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PT76B/DONE\n")
					(number "B16")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PT74B/PROGRAMN")
					(number "C12")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PT82B/MCSNO/MSDO")
					(number "C13")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PT78B/MOSI/MD0")
					(number "C14")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PT78A/MCSN/PCLKT0_1")
					(number "C15")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PT76A/MCLK/PCLKT0_0")
					(number "C16")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PT74A/INITN\n")
					(number "D11")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PT82A/MD3")
					(number "D12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VCCIO0")
					(number "D13")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PT80B/MD2")
					(number "D15")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PT80A/MISO/MD1")
					(number "D16")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PT84A")
					(number "E15")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PT84B")
					(number "E16")
				)
			)
			(symbol "CrossLink_LIFCL-40-9BG256C_2_1"
				(text "BANK1"
					(at 40.64 -54.61 0)
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "JTAG_EN")
					(number "D10")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PR4A")
					(number "E9")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PR4B")
					(number "E10")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PR6B/TMS/SCSN")
					(number "E11")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PR6A")
					(number "E12")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PR10A")
					(number "E13")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PR10B/TDO/SSO")
					(number "E14")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PR3B")
					(number "F9")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PR8A")
					(number "F10")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PR8B/TDI/SSI")
					(number "F11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VCCIO1")
					(number "F13")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PR13A/TCK/SCLK")
					(number "F14")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PR13B")
					(number "F15")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PR19A/PCLKT1_1")
					(number "F16")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PR11A/SDA/USER_SDA")
					(number "G9")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PR11B/SCL/USER_SCL")
					(number "G10")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PR15A")
					(number "G11")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PR15B")
					(number "G12")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PR17A/PCLKT1_2")
					(number "G13")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PR17B")
					(number "G14")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PR20A/PCLKT1_0\n")
					(number "G15")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "PR19B")
					(number "G16")
				)
			)
			(symbol "CrossLink_LIFCL-40-9BG256C_3_1"
				(text "BANK2"
					(at 40.64 -34.29 0)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PR30B")
					(number "H10")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PR30A/PCLKT2_0")
					(number "H11")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PR32B")
					(number "H12")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PR32A/PCLKT2_1")
					(number "H13")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PR27B")
					(number "H14")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PR27A")
					(number "H15")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PR26A")
					(number "H16")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PR36A")
					(number "J11")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PR36B")
					(number "J12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VCCIO2")
					(number "J13")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PR34B")
					(number "J15")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PR34A/PCLKT2_2")
					(number "J16")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PR38A")
					(number "K11")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PR38B")
					(number "K12")
				)
			)
			(symbol "CrossLink_LIFCL-40-9BG256C_4_1"
				(text "BANK3"
					(at 40.64 -77.47 0)
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 3.81)
					(name "PB80B/ADC_CN12")
					(number "L10")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 3.81)
					(name "PB80A/ADC_CP12")
					(number "L11")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 3.81)
					(name "PB82B/ADC_CN15")
					(number "L12")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 3.81)
					(name "PB78B/ADC_CN11")
					(number "M11")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 3.81)
					(name "PB78A/ADC_CP11")
					(number "M12")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 3.81)
					(name "PB82A/ADC_CP15")
					(number "M13")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PB74A/PCLKT3_3/ADC_CP14")
					(number "M14")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 3.81)
					(name "PB84B/LRC_GPLL0C_IN/VREF3_2")
					(number "M15")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 3.81)
					(name "PB84A/LRC_GPLL0T_IN")
					(number "M16")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PB64B/ADC_CN4")
					(number "N11")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PB64A/ADC_CP4")
					(number "N12")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PB70B/COMP2IN\n")
					(number "N13")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "PB74B/PCLKC3_3/ADC_CN14")
					(number "N14")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "PB76B/COMP3IN")
					(number "N15")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "PB76A/COMP3IP")
					(number "N16")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PB56A/ADC_CP7\n")
					(number "P10")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PB54B/PCLKC3_0/ADC_CN5\n")
					(number "P11")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "VCCIO3")
					(number "P12")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PB70A/COMP2IP")
					(number "P14")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PB72A/PCLKT3_2/ADC_CP13")
					(number "P15")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "PB72B/PCLKC3_2/ADC_CN13")
					(number "P16")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PB56B/ADC_CN7\n")
					(number "R10")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PB54A/PCLKT3_0/VREF3_1/ADC_CP5")
					(number "R11")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PB60A/ADC_CP9")
					(number "R12")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PB62A/ADC_CP10")
					(number "R13")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PB62B/ADC_CN10")
					(number "R14")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PB68B/ADC_CN8")
					(number "R15")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PB68A/ADC_CP8")
					(number "R16")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PB58B/PCLKC3_1/ADC_CN6\n")
					(number "T11")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PB58A/PCLKT3_1/ADC_CP6\n")
					(number "T12")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PB60B/ADC_CN9")
					(number "T13")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PB66A/COMP1IP")
					(number "T14")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PB66B/COMP1IN")
					(number "T15")
				)
			)
			(symbol "CrossLink_LIFCL-40-9BG256C_5_1"
				(text "BANK4"
					(at 40.64 -82.55 0)
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PB34A")
					(number "L8")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "PB34B")
					(number "L9")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "PB38B")
					(number "M8")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "PB38A")
					(number "M9")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 3.81)
					(name "PB46A")
					(number "M10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VCCIO4")
					(number "N6")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PB36A")
					(number "N8")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "PB36B")
					(number "N9")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 3.81)
					(name "PB46B/VREF4_2")
					(number "N10")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PB24B/PCLKC4_2\n")
					(number "P4")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PB22B")
					(number "P5")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PB32A")
					(number "P6")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PB32B")
					(number "P7")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 3.81)
					(name "PB42B")
					(number "P8")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 3.81)
					(name "PB44B/PCLKC4_0")
					(number "P9")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PB16A/VREF4_1")
					(number "R1")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PB16B")
					(number "R2")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PB18A/PCLKT4_3\n")
					(number "R3")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PB24A/PCLKT4_2")
					(number "R4")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PB22A")
					(number "R5")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PB26B")
					(number "R6")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PB28B")
					(number "R7")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 3.81)
					(name "PB42A")
					(number "R8")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 3.81)
					(name "PB44A/PCLKT4_0")
					(number "R9")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PB18B/PCLKC4_3\n")
					(number "T2")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PB20A")
					(number "T3")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PB20B")
					(number "T4")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PB26A")
					(number "T5")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PB28A")
					(number "T6")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PB30A")
					(number "T7")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PB30B")
					(number "T8")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 3.81)
					(name "PB40A/PCLKT4_1")
					(number "T9")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 3.81)
					(name "PB40B/PCLKC4_1")
					(number "T10")
				)
			)
			(symbol "CrossLink_LIFCL-40-9BG256C_6_1"
				(text "BANK5"
					(at 50.8 -26.67 0)
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PB10B/PCLKC5_2/ADC_CN2/COMP3N")
					(number "K7")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PB10A/PCLKT5_2/ADC_CP2/COMP3P")
					(number "L6")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PB8A/PCLKT5_1/LLC_GPLL0T_IN/ADC_CP3")
					(number "L7")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PB6B/PCLKC5_0/CDR_RXN1/ADC_CN1/COMP2N")
					(number "M4")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PB8B/PCLKC5_1/LLC_GPLL0C_IN/ADC_CN3")
					(number "M7")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PB4B/CDR_RXN0/ADC_CN0/COMP1N")
					(number "N3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PB6A/PCLKT5_0/CDR_RXP1/ADC_CP1/COMP2P")
					(number "N4")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VCCIO5")
					(number "N5")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PB12A/PCLKT5_3")
					(number "P1")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PB12B/PCLKC5_3/VREF5_2")
					(number "P2")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PB4A/CDR_RXP0/VREF5_1/ADC_CP0/COMP1P\n")
					(number "P3")
				)
			)
			(symbol "CrossLink_LIFCL-40-9BG256C_7_1"
				(text "BANK6"
					(at 39.37 -67.31 0)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PL27A")
					(number "H1")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PL27B")
					(number "H2")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PL26B")
					(number "H3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PL26A")
					(number "H4")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PL24B")
					(number "H5")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PL24A")
					(number "H6")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PL32A/PCLKT6_1")
					(number "J1")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PL32B")
					(number "J2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VCCIO6")
					(number "J4")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PL30B")
					(number "J5")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PL30A/PCLKT6_0")
					(number "J6")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PL34A/PCLKT6_2")
					(number "K1")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PL34B")
					(number "K2")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PL36B")
					(number "K3")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PL36A")
					(number "K4")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PL38B")
					(number "K5")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PL38A")
					(number "K6")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PL40A")
					(number "L1")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PL40B")
					(number "L2")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "PL47B")
					(number "L3")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PL46A")
					(number "L4")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "PL46B")
					(number "L5")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PL42A")
					(number "M1")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "PL42B")
					(number "M2")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "PL47A")
					(number "M3")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 3.81)
					(name "PL49B")
					(number "N1")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 3.81)
					(name "PL49A")
					(number "N2")
				)
			)
			(symbol "CrossLink_LIFCL-40-9BG256C_8_1"
				(text "BANK7"
					(at 40.64 -29.21 0)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PL3A/ULC_GPLL0T_IN")
					(number "D4")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PL3B/ULC_GPLL0C_IN")
					(number "D5")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PL4A")
					(number "D6")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PL6A")
					(number "E4")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PL6B")
					(number "E5")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PL4B")
					(number "E6")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PL19A/PCLKT7_1")
					(number "F4")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VCCIO7")
					(number "F5")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PL17A/PCLKT7_2")
					(number "F6")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PL20A/PCLKT7_0")
					(number "G3")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PL19B")
					(number "G4")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PL17B")
					(number "G6")
				)
			)
			(symbol "CrossLink_LIFCL-40-9BG256C_9_1"
				(text "PHY0"
					(at 24.13 -29.21 0)
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "DPHY0_D3+")
					(number "B1")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "DPHY0_D3-")
					(number "B2")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "DPHY0_D1+")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "DPHY0_D1-")
					(number "C2")
				)
				(pin bidirectional clock
					(at 0 0 0)
					(length 3.81)
					(name "DPHY0_CK+")
					(number "D1")
				)
				(pin bidirectional clock
					(at 0 -2.54 0)
					(length 3.81)
					(name "DPHY0_CK-")
					(number "D2")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 3.81)
					(name "DPHY0_D0+")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 3.81)
					(name "DPHY0_D0-")
					(number "E2")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 3.81)
					(name "DPHY0_D2+")
					(number "F1")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 3.81)
					(name "DPHY0_D2-")
					(number "F2")
				)
			)
			(symbol "CrossLink_LIFCL-40-9BG256C_10_1"
				(text "PHY1"
					(at 24.13 -29.21 0)
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 3.81)
					(name "DPHY1_D2+")
					(number "A3")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 3.81)
					(name "DPHY1_D0+")
					(number "A4")
				)
				(pin bidirectional clock
					(at 0 0 0)
					(length 3.81)
					(name "DPHY1_CK+")
					(number "A5")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "DPHY1_D1+")
					(number "A6")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "DPHY1_D3+")
					(number "A7")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 3.81)
					(name "DPHY1_D2-")
					(number "B3")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 3.81)
					(name "DPHY1_D0-")
					(number "B4")
				)
				(pin bidirectional clock
					(at 0 -2.54 0)
					(length 3.81)
					(name "DPHY1_CK-")
					(number "B5")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "DPHY1_D1-")
					(number "B6")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "DPHY1_D3-")
					(number "B7")
				)
			)
			(symbol "CrossLink_LIFCL-40-9BG256C_11_1"
				(text "ADC"
					(at 24.13 -24.13 0)
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 3.81)
					(name "ADC_D0-")
					(number "K13")
				)
				(pin passive line
					(at 0 -3.81 0)
					(length 3.81)
					(name "ADC_D0+")
					(number "K14")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "ADC_D1+")
					(number "K15")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "ADC_D1-")
					(number "K16")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 3.81)
					(name "VSSADC")
					(number "L13")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VCCADC18")
					(number "L14")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 3.81)
					(name "ADC_REFP0")
					(number "L15")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(name "ADC_REFP1")
					(number "L16")
				)
			)
			(symbol "CrossLink_LIFCL-40-9BG256C_12_1"
				(text "SDO"
					(at 24.13 -22.86 0)
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "SD_REFCLK+")
					(number "A9")
				)
				(pin output line
					(at 0 -8.89 0)
					(length 3.81)
					(name "SD0_TXD-")
					(number "A11")
				)
				(pin output line
					(at 0 -6.35 0)
					(length 3.81)
					(name "SD0_TXD+")
					(number "A12")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "SD0_RXD-")
					(number "A14")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "SD0_RXD+")
					(number "A15")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "SD_REFCLK-")
					(number "B9")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 3.81)
					(name "SD0_REFRET")
					(number "B12")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 3.81)
					(name "SD0_REXT")
					(number "C11")
				)
			)
			(symbol "CrossLink_LIFCL-40-9BG256C_13_1"
				(pin power_in line
					(at 33.02 0 180)
					(length 3.81)
					(name "VSSADPHY")
					(number "A1")
				)
				(pin power_in line
					(at 0 -34.29 0)
					(length 3.81)
					(name "VCCPLLDPHY0")
					(number "A2")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(hide yes)
					(name "VSSADPHY")
					(number "A8")
				)
				(pin power_in line
					(at 33.02 -3.81 180)
					(length 3.81)
					(name "VSSSD")
					(number "A10")
				)
				(pin passive line
					(at 33.02 -3.81 180)
					(length 3.81)
					(hide yes)
					(name "VSSSD")
					(number "A13")
				)
				(pin passive line
					(at 33.02 -3.81 180)
					(length 3.81)
					(hide yes)
					(name "VSSSD")
					(number "A16")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(hide yes)
					(name "VSSADPHY")
					(number "B8")
				)
				(pin passive line
					(at 33.02 -3.81 180)
					(length 3.81)
					(hide yes)
					(name "VSSSD")
					(number "B10")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 3.81)
					(name "VCCAUXSD")
					(number "B11")
				)
				(pin power_in line
					(at 0 -45.72 0)
					(length 3.81)
					(name "VCCPLLSD0")
					(number "B13")
				)
				(pin passive line
					(at 33.02 -3.81 180)
					(length 3.81)
					(hide yes)
					(name "VSSSD")
					(number "B14")
				)
				(pin power_in line
					(at 0 -43.18 0)
					(length 3.81)
					(name "VCCSD0")
					(number "B15")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(hide yes)
					(name "VSSADPHY")
					(number "C3")
				)
				(pin power_in line
					(at 0 -21.59 0)
					(length 3.81)
					(name "VCCDPHY0")
					(number "C4")
				)
				(pin power_in line
					(at 0 -36.83 0)
					(length 3.81)
					(name "VCCPLLDPHY1")
					(number "C5")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(hide yes)
					(name "VSSADPHY")
					(number "C6")
				)
				(pin power_in line
					(at 0 -24.13 0)
					(length 3.81)
					(name "VCCDPHY1")
					(number "C7")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 3.81)
					(name "VCCADPHY1")
					(number "C8")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "C9")
				)
				(pin power_in line
					(at 33.02 -7.62 180)
					(length 3.81)
					(name "VSS")
					(number "C10")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(hide yes)
					(name "VSSADPHY")
					(number "D3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VCC")
					(number "D7")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D8")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "D9")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D14")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 3.81)
					(name "VCCADPHY0")
					(number "E3")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E7")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E8")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(hide yes)
					(name "VSSADPHY")
					(number "F3")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VCCAUXA")
					(number "F7")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VCCAUX")
					(number "F8")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F12")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(hide yes)
					(name "VSSADPHY")
					(number "G1")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G2")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G5")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "VCCAUX")
					(number "G7")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G8")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "H7")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H8")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H9")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J3")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J7")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J8")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J9")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "J10")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J14")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 3.81)
					(name "VCCAUXH4")
					(number "K8")
				)
				(pin power_in line
					(at 0 -3.81 0)
					(length 3.81)
					(name "VCCECLK")
					(number "K9")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VCCAUXH3")
					(number "K10")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "M5")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 3.81)
					(name "VCCAUXH5")
					(number "M6")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "N7")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "P13")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "T1")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "T16")
				)
			)
			(embedded_fonts no)
		)
)
