(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CrossLink_LIFCL-40-9MG121I"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 81.28 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CrossLink_LIFCL-40-9MG121I"
				(at 81.28 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CrossLink_LIFCL-40-9MG121I"
				(at 81.28 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/225/Lattice_FPGA_DS_02049_1_3_CrossLink_NX_Family-2940960.pdf"
				(at 81.28 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Lattice CrossLink-NX Embedded Vision Bridging & Processing FPGA with 2.5G MIPI D-PHY"
				(at 81.28 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LIFCL-40-9MG121I"
				(at 81.28 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Lattice Semiconductor"
				(at 81.28 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 81.28 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 81.28 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "IC, FPGA, BGA"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CrossLink_LIFCL-40-9MG121I_1_1"
				(text "Bank 1"
					(at 16.51 0 0)
				)
				(text "Bank 5"
					(at 27.94 -19.05 900)
				)
				(text "Bank 1"
					(at 30.48 -82.55 900)
				)
				(text "Bank 0"
					(at 30.48 -134.62 900)
				)
				(text "Bank 3"
					(at 33.02 -152.4 900)
				)
				(text "Bank 4"
					(at 41.91 -80.01 900)
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "JTAG_EN")
					(number "A1")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 3.81)
					(name "PR10B/TDO/SSO")
					(number "A2")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 3.81)
					(name "PR8B/TDI/SSI")
					(number "A3")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "DPHY1_DP3")
					(number "A5")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "DPHY1_DP1")
					(number "A6")
				)
				(pin input clock
					(at 0 -35.56 0)
					(length 3.81)
					(name "DPHY1_CKP")
					(number "A7")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "DPHY1_DP0")
					(number "A8")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "DPHY1_DP2")
					(number "A9")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "DPHY0_DN3")
					(number "A10")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "DPHY0_DP3")
					(number "A11")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "PR6B/TMS/SCSN")
					(number "B1")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 3.81)
					(name "PR11A/SDA/USER_SDA")
					(number "B2")
				)
				(pin bidirectional line
					(at 0 -152.4 0)
					(length 3.81)
					(name "PT84A")
					(number "B3")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "DPHY1_DN3")
					(number "B5")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "DPHY1_DN1")
					(number "B6")
				)
				(pin input clock
					(at 0 -33.02 0)
					(length 3.81)
					(name "DPHY1_CKN")
					(number "B7")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "DPHY1_DN0")
					(number "B8")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "DPHY1_DN2")
					(number "B9")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "DPHY0_DN1")
					(number "B10")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "DPHY0_DP1")
					(number "B11")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 3.81)
					(name "PR13A/TCK/SCLK")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 3.81)
					(name "PR11B/SCL/USER_SCL")
					(number "C2")
				)
				(pin bidirectional line
					(at 0 -154.94 0)
					(length 3.81)
					(name "PT84B")
					(number "C3")
				)
				(pin input clock
					(at 0 -5.08 0)
					(length 3.81)
					(name "DPHY0_CKN")
					(number "C10")
				)
				(pin input clock
					(at 0 -7.62 0)
					(length 3.81)
					(name "DPHY0_CKP")
					(number "C11")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 3.81)
					(name "PR13B")
					(number "D1")
				)
				(pin bidirectional line
					(at 0 -139.7 0)
					(length 3.81)
					(name "PT80B/MD2")
					(number "D5")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 3.81)
					(name "PT78B/MOSI/MD0")
					(number "D6")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 3.81)
					(name "PT76B/DONE")
					(number "D7")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 3.81)
					(name "PT74B/PROGRAMN")
					(number "D8")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "DPHY0_DN0")
					(number "D10")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "DPHY0_DP0")
					(number "D11")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 3.81)
					(name "PR17A/PCLKT1_2")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 3.81)
					(name "PR15A")
					(number "E2")
				)
				(pin bidirectional line
					(at 0 -147.32 0)
					(length 3.81)
					(name "PT82B/MCSNO/MSDO")
					(number "E3")
				)
				(pin bidirectional line
					(at 0 -144.78 0)
					(length 3.81)
					(name "PT82A/MD3")
					(number "E4")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 3.81)
					(name "PT80A/MISO/MD1")
					(number "E5")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 3.81)
					(name "PT78A/MCSN/PCLKT0_1")
					(number "E6")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 3.81)
					(name "PT76A/MCLK/PCLKT0_0")
					(number "E7")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 3.81)
					(name "PT74A/INITN")
					(number "E8")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "DPHY0_DN2")
					(number "E10")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "DPHY0_DP2")
					(number "E11")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 3.81)
					(name "PR20A/PCLKT1_0")
					(number "F1")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 3.81)
					(name "PR19A/PCLKT1_1")
					(number "F2")
				)
				(pin bidirectional line
					(at 66.04 -100.33 180)
					(length 3.81)
					(name "PB32A")
					(number "F5")
				)
				(pin bidirectional line
					(at 66.04 -72.39 180)
					(length 3.81)
					(name "PB24B/PCLKC4_2")
					(number "F6")
				)
				(pin bidirectional line
					(at 66.04 -69.85 180)
					(length 3.81)
					(name "PB24A/PCLKT4_2")
					(number "F7")
				)
				(pin bidirectional line
					(at 66.04 -179.07 180)
					(length 3.81)
					(name "PB84B/VREF3_2")
					(number "G1")
				)
				(pin bidirectional line
					(at 66.04 -176.53 180)
					(length 3.81)
					(name "PB84A/LRC_GPLL0T_IN")
					(number "G2")
				)
				(pin bidirectional line
					(at 66.04 -138.43 180)
					(length 3.81)
					(name "PB58A/PCLKT3_1")
					(number "G4")
				)
				(pin bidirectional line
					(at 66.04 -102.87 180)
					(length 3.81)
					(name "PB32B")
					(number "G5")
				)
				(pin bidirectional line
					(at 66.04 -62.23 180)
					(length 3.81)
					(name "PB22A")
					(number "G7")
				)
				(pin bidirectional line
					(at 66.04 -64.77 180)
					(length 3.81)
					(name "PB22B")
					(number "G8")
				)
				(pin bidirectional line
					(at 66.04 -3.81 180)
					(length 3.81)
					(name "PB4B/CDR_RXN0")
					(number "G10")
				)
				(pin bidirectional line
					(at 66.04 -1.27 180)
					(length 3.81)
					(name "PB4A/CDR_RXP0/VREF5_1")
					(number "G11")
				)
				(pin bidirectional line
					(at 66.04 -168.91 180)
					(length 3.81)
					(name "PB74A/PCLKT3_3")
					(number "H1")
				)
				(pin bidirectional line
					(at 66.04 -171.45 180)
					(length 3.81)
					(name "PB74B/PCLKC3_3")
					(number "H2")
				)
				(pin bidirectional line
					(at 66.04 -140.97 180)
					(length 3.81)
					(name "PB58B/PCLKC3_1")
					(number "H4")
				)
				(pin bidirectional line
					(at 66.04 -107.95 180)
					(length 3.81)
					(name "PB40A/PCLKT4_1")
					(number "H5")
				)
				(pin bidirectional line
					(at 66.04 -57.15 180)
					(length 3.81)
					(name "PB20B")
					(number "H7")
				)
				(pin bidirectional line
					(at 66.04 -54.61 180)
					(length 3.81)
					(name "PB20A")
					(number "H8")
				)
				(pin bidirectional line
					(at 66.04 -11.43 180)
					(length 3.81)
					(name "PB6B/PCLKC5_0/CDR_RXN1")
					(number "H10")
				)
				(pin bidirectional line
					(at 66.04 -8.89 180)
					(length 3.81)
					(name "PB6A/PCLKT5_0/CDR_RXP1")
					(number "H11")
				)
				(pin bidirectional line
					(at 66.04 -161.29 180)
					(length 3.81)
					(name "PB72A/PCLKT3_2")
					(number "J1")
				)
				(pin bidirectional line
					(at 66.04 -163.83 180)
					(length 3.81)
					(name "PB72B/PCLKC3_2")
					(number "J2")
				)
				(pin bidirectional line
					(at 66.04 -130.81 180)
					(length 3.81)
					(name "PB56A")
					(number "J4")
				)
				(pin bidirectional line
					(at 66.04 -110.49 180)
					(length 3.81)
					(name "PB40B/PCLKC4_1")
					(number "J5")
				)
				(pin bidirectional line
					(at 66.04 -87.63 180)
					(length 3.81)
					(name "PB28B")
					(number "J7")
				)
				(pin bidirectional line
					(at 66.04 -46.99 180)
					(length 3.81)
					(name "PB18A/PCLKT4_3")
					(number "J8")
				)
				(pin bidirectional line
					(at 66.04 -19.05 180)
					(length 3.81)
					(name "PB8B/PCLKC5_1/LLC_GPLL0C_IN")
					(number "J10")
				)
				(pin bidirectional line
					(at 66.04 -16.51 180)
					(length 3.81)
					(name "PB8A/PCLKT5_1/LLC_GPLL0T_IN")
					(number "J11")
				)
				(pin bidirectional line
					(at 66.04 -153.67 180)
					(length 3.81)
					(name "PB68A")
					(number "K1")
				)
				(pin bidirectional line
					(at 66.04 -156.21 180)
					(length 3.81)
					(name "PB68B")
					(number "K2")
				)
				(pin bidirectional line
					(at 66.04 -133.35 180)
					(length 3.81)
					(name "PB56B")
					(number "K4")
				)
				(pin bidirectional line
					(at 66.04 -118.11 180)
					(length 3.81)
					(name "PB44B/PCLKC4_0")
					(number "K5")
				)
				(pin bidirectional line
					(at 66.04 -95.25 180)
					(length 3.81)
					(name "PB30B")
					(number "K6")
				)
				(pin bidirectional line
					(at 66.04 -85.09 180)
					(length 3.81)
					(name "PB28A")
					(number "K7")
				)
				(pin bidirectional line
					(at 66.04 -49.53 180)
					(length 3.81)
					(name "PB18B/PCLKC4_3")
					(number "K8")
				)
				(pin bidirectional line
					(at 66.04 -41.91 180)
					(length 3.81)
					(name "PB16B")
					(number "K9")
				)
				(pin bidirectional line
					(at 66.04 -34.29 180)
					(length 3.81)
					(name "PB12B/PCLKC5_3/VREF5_2")
					(number "K10")
				)
				(pin bidirectional line
					(at 66.04 -24.13 180)
					(length 3.81)
					(name "PB10A/PCLKT5_2")
					(number "K11")
				)
				(pin bidirectional line
					(at 66.04 -148.59 180)
					(length 3.81)
					(name "PB60B")
					(number "L1")
				)
				(pin bidirectional line
					(at 66.04 -146.05 180)
					(length 3.81)
					(name "PB60A")
					(number "L2")
				)
				(pin bidirectional line
					(at 66.04 -125.73 180)
					(length 3.81)
					(name "PB54B/PCLKC3_0")
					(number "L3")
				)
				(pin bidirectional line
					(at 66.04 -123.19 180)
					(length 3.81)
					(name "PB54A/PCLKT3_0/VREF3_1")
					(number "L4")
				)
				(pin bidirectional line
					(at 66.04 -115.57 180)
					(length 3.81)
					(name "PB44A/PCLKT4_0")
					(number "L5")
				)
				(pin bidirectional line
					(at 66.04 -92.71 180)
					(length 3.81)
					(name "PB30A")
					(number "L6")
				)
				(pin bidirectional line
					(at 66.04 -80.01 180)
					(length 3.81)
					(name "PB26B")
					(number "L7")
				)
				(pin bidirectional line
					(at 66.04 -77.47 180)
					(length 3.81)
					(name "PB26A")
					(number "L8")
				)
				(pin bidirectional line
					(at 66.04 -39.37 180)
					(length 3.81)
					(name "PB16A/VREF4_1")
					(number "L9")
				)
				(pin bidirectional line
					(at 66.04 -31.75 180)
					(length 3.81)
					(name "PB12A/PCLKT5_3")
					(number "L10")
				)
				(pin bidirectional line
					(at 66.04 -26.67 180)
					(length 3.81)
					(name "PB10B/PCLKC5_2")
					(number "L11")
				)
			)
			(symbol "CrossLink_LIFCL-40-9MG121I_2_1"
				(pin power_in line
					(at 0 -22.86 0)
					(length 3.81)
					(name "VCCADPHY1")
					(number "A4")
				)
				(pin power_in line
					(at 30.48 -48.26 180)
					(length 3.81)
					(name "VSSADPHY")
					(number "B4")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 3.81)
					(name "VCCDPHY1")
					(number "C4")
				)
				(pin passive line
					(at 30.48 -48.26 180)
					(length 3.81)
					(hide yes)
					(name "VSSADPHY")
					(number "C5")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 3.81)
					(name "VCCPLLDPHY1")
					(number "C6")
				)
				(pin passive line
					(at 30.48 -48.26 180)
					(length 3.81)
					(hide yes)
					(name "VSSADPHY")
					(number "C7")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 3.81)
					(name "VCCPLLDPHY0")
					(number "C8")
				)
				(pin passive line
					(at 30.48 -48.26 180)
					(length 3.81)
					(hide yes)
					(name "VSSADPHY")
					(number "C9")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 3.81)
					(name "VCCIO1")
					(number "D2")
				)
				(pin power_in line
					(at 30.48 -45.72 180)
					(length 3.81)
					(name "VSS")
					(number "D3")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 3.81)
					(name "VCCIO0")
					(number "D4")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 3.81)
					(name "VCCDPHY0")
					(number "D9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VCC")
					(number "E9")
				)
				(pin passive line
					(at 30.48 -45.72 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "F4")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VCCECLK")
					(number "F8")
				)
				(pin passive line
					(at 30.48 -45.72 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F9")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 3.81)
					(name "VCCADPHY0")
					(number "F10")
				)
				(pin passive line
					(at 30.48 -48.26 180)
					(length 3.81)
					(hide yes)
					(name "VSSADPHY")
					(number "F11")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VCCAUX")
					(number "G3")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VCCAUXH4")
					(number "G6")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 3.81)
					(name "VCCAUXH5")
					(number "G9")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VCCAUXH3")
					(number "H3")
				)
				(pin passive line
					(at 30.48 -45.72 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H6")
				)
				(pin passive line
					(at 30.48 -45.72 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H9")
				)
				(pin passive line
					(at 30.48 -45.72 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J3")
				)
				(pin power_in line
					(at 0 -45.72 0)
					(length 3.81)
					(name "VCCIO4")
					(number "J6")
				)
				(pin power_in line
					(at 0 -48.26 0)
					(length 3.81)
					(name "VCCIO5")
					(number "J9")
				)
				(pin power_in line
					(at 0 -43.18 0)
					(length 3.81)
					(name "VCCIO3")
					(number "K3")
				)
			)
			(embedded_fonts no)
		)
)
