(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LM339_TSSOP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 27.94 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LM339_TSSOP"
				(at 27.94 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LM339_TSSOP"
				(at 27.94 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm339b.pdf?ts=1679641364820&ref_url=https%253A%252F%252Fwww.google.com%252F"
				(at 27.94 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Analogue Comparator, Differential, 4 Comparators, 300 ns, 2V to 36V, TSSOP, 14 Pins"
				(at 27.94 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LM339PW"
				(at 27.94 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 27.94 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 27.94 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, AMP, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LM339_TSSOP_1_1"
				(text "+"
					(at 3.81 -4.826 0)
				)
				(text "-"
					(at 3.81 -7.112 0)
				)
				(text "+"
					(at 3.81 -11.176 0)
				)
				(text "-"
					(at 3.81 -13.462 0)
				)
				(text "+"
					(at 3.81 -17.78 0)
				)
				(text "-"
					(at 3.81 -20.066 0)
				)
				(text "+"
					(at 3.81 -23.876 0)
				)
				(text "-"
					(at 3.81 -26.162 0)
				)
				(pin output line
					(at 12.7 -11.43 180)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin output line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V+")
					(number "3")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "")
					(number "6")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "")
					(number "7")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "")
					(number "8")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 2.54)
					(name "")
					(number "9")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "")
					(number "10")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "")
					(number "11")
				)
				(pin power_in line
					(at 0 -29.21 0)
					(length 2.54)
					(name "V-")
					(number "12")
				)
				(pin output line
					(at 12.7 -24.13 180)
					(length 2.54)
					(name "")
					(number "13")
				)
				(pin output line
					(at 12.7 -17.78 180)
					(length 2.54)
					(name "")
					(number "14")
				)
			)
			(embedded_fonts no)
		)
)
