(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LM4861M"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 34.29 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LM4861M"
				(at 34.29 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LM4861M"
				(at 34.29 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm4861.pdf?ts=1717756748393&ref_url=https%253A%252F%252Feu.mouser.com%252F"
				(at 34.29 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Audio Amplifiers 1.1W AUDIO POWER AMP"
				(at 34.29 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LM4861M/NOPB"
				(at 34.29 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 34.29 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 34.29 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 34.29 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, POWER, AMP, AUDIO"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LM4861M_1_1"
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "BYPASS")
					(number "2")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "IN+")
					(number "3")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "IN-")
					(number "4")
				)
				(pin output line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "V_{o}1")
					(number "5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{DD}")
					(number "6")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "GND")
					(number "7")
				)
				(pin output line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "V_{o}2")
					(number "8")
				)
			)
			(symbol "LM4861M_2_1"
				(pin power_in line
					(at 0 -27.94 0)
					(length 2.54)
					(name "VCCD12_RX")
					(number "1")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "VCCA12_RX")
					(number "4")
				)
				(pin power_in line
					(at 0 -45.72 0)
					(length 2.54)
					(name "VCC33_RX")
					(number "7")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "VCC12_PI")
					(number "10")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 2.54)
					(name "VCC12_RXPLL")
					(number "13")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 2.54)
					(name "VCC33_IO")
					(number "14")
				)
				(pin no_connect line
					(at 33.02 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "17")
				)
				(pin no_connect line
					(at 33.02 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "RSVD")
					(number "18")
				)
				(pin no_connect line
					(at 33.02 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "19")
				)
				(pin input line
					(at 35.56 -30.48 180)
					(length 2.54)
					(name "RST_N")
					(number "20")
				)
				(pin bidirectional line
					(at 35.56 0 180)
					(length 2.54)
					(name "CSCL_GPIO10")
					(number "21")
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 2.54)
					(name "CSDA_GPIO11")
					(number "22")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "24")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(hide yes)
					(name "VCC33_IO")
					(number "25")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 2.54)
					(name "INTIO_GPIO5")
					(number "26")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 2.54)
					(name "I2S_WS_GPIO7")
					(number "27")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 2.54)
					(name "I2S_SCLK_GPIO8")
					(number "28")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 2.54)
					(name "I2S_MCLK_GPIO9")
					(number "29")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "30")
				)
				(pin output line
					(at 35.56 -15.24 180)
					(length 2.54)
					(name "I2S_D0_SPDIF")
					(number "31")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(hide yes)
					(name "VCC33_IO")
					(number "32")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 2.54)
					(name "VCC33_MTX3")
					(number "33")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "VCC12_MTX3")
					(number "34")
				)
				(pin power_in line
					(at 0 -35.56 0)
					(length 2.54)
					(name "VCC33_MTX2")
					(number "45")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VCC12_MTX2")
					(number "46")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 2.54)
					(name "VCC33_MTXPLL")
					(number "47")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VCC12_MTX1")
					(number "48")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VCC12_MTX0")
					(number "59")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "60")
				)
				(pin output line
					(at 35.56 -43.18 180)
					(length 2.54)
					(name "REXT")
					(number "61")
				)
				(pin power_in line
					(at 0 -48.26 0)
					(length 2.54)
					(name "VCC33_BG")
					(number "62")
				)
				(pin output line
					(at 35.56 -35.56 180)
					(length 2.54)
					(name "XTALO")
					(number "63")
				)
				(pin input line
					(at 35.56 -38.1 180)
					(length 2.54)
					(name "XTALI")
					(number "64")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 2.54)
					(name "GND")
					(number "65")
				)
			)
			(embedded_fonts no)
		)
)
