(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LMH1218RTWT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LMH1218RTWT"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LMH1218RTWT"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/gpn/LMH1218"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Low Power Ultra HD Cable Driver With Integrated Reclocker"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LMH1218RTWT"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LMH1218RTWT_1_1"
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "MODE_SEL")
					(number "1")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "SS_N")
					(number "2")
					(alternate "ADDR0" passive line)
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "SCK")
					(number "3")
					(alternate "SCL" passive line)
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "MOSI")
					(number "4")
					(alternate "SDA" passive line)
				)
				(pin no_connect line
					(at 29.21 -40.64 180)
					(length 2.54)
					(name "NC")
					(number "5")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "ENABLE")
					(number "6")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "7")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "IN1+")
					(number "8")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "IN1-")
					(number "9")
				)
				(pin power_in line
					(at 31.75 -43.18 180)
					(length 2.54)
					(name "GND")
					(number "10")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "IN0+")
					(number "11")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "IN0-")
					(number "12")
				)
				(pin output line
					(at 31.75 0 180)
					(length 2.54)
					(name "LOS_INT_N")
					(number "13")
				)
				(pin passive line
					(at 31.75 -30.48 180)
					(length 2.54)
					(name "SMPTE_10GbE")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "MISO")
					(number "15")
					(alternate "ADDR1" passive line)
				)
				(pin output line
					(at 31.75 -2.54 180)
					(length 2.54)
					(name "LOCK")
					(number "16")
				)
				(pin no_connect line
					(at 29.21 -40.64 180)
					(length 2.54)
					(name "NC")
					(number "17")
				)
				(pin no_connect line
					(at 29.21 -40.64 180)
					(length 2.54)
					(name "NC")
					(number "18")
				)
				(pin output line
					(at 31.75 -12.7 180)
					(length 2.54)
					(name "OUT0-")
					(number "19")
				)
				(pin output line
					(at 31.75 -15.24 180)
					(length 2.54)
					(name "OUT0+")
					(number "20")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "21")
				)
				(pin output line
					(at 31.75 -20.32 180)
					(length 2.54)
					(name "OUT1-")
					(number "22")
				)
				(pin output line
					(at 31.75 -22.86 180)
					(length 2.54)
					(name "OUT1+")
					(number "23")
				)
				(pin passive line
					(at 31.75 -43.18 180)
					(length 2.54)
					(name "GND")
					(number "24")
				)
				(pin passive line
					(at 31.75 -43.18 180)
					(length 2.54)
					(name "GND")
					(number "25")
				)
			)
			(embedded_fonts no)
		)
)
