(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LMH1297"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LMH1297"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LMH1297"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lmh1297.pdf?ts=1770286497891&ref_url=https%253A%252F%252Fwww.google.com%252F"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "12G UHD-SDI Bidirectional I/O With Integrated Reclocker"
				(at 43.18 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LMH1297RTVT"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LMH1297_1_1"
				(pin passive line
					(at 29.21 0 180)
					(length 2.54)
					(name "SDI_IO+")
					(number "1")
				)
				(pin passive line
					(at 29.21 -2.54 180)
					(length 2.54)
					(name "SDI_IO-")
					(number "2")
				)
				(pin passive line
					(at 29.21 -49.53 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "3")
				)
				(pin passive line
					(at 0 -41.91 0)
					(length 2.54)
					(name "OUT0_SEL")
					(number "4")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 2.54)
					(name "EQ_CD_SEL")
					(number "5")
				)
				(pin passive line
					(at 29.21 -49.53 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "6")
				)
				(pin passive line
					(at 29.21 -10.16 180)
					(length 2.54)
					(name "SDI_OUT-")
					(number "7")
				)
				(pin passive line
					(at 29.21 -7.62 180)
					(length 2.54)
					(name "SDI_OUT+")
					(number "8")
				)
				(pin passive line
					(at 0 -52.07 0)
					(length 2.54)
					(name "HOST_EQ0")
					(number "9")
				)
				(pin no_connect line
					(at 26.67 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "RSV1")
					(number "10")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 2.54)
					(name "~{SS}")
					(number "11")
					(alternate "ADDR0" passive line)
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 2.54)
					(name "MODE_SEL")
					(number "12")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 2.54)
					(name "MOSI")
					(number "13")
					(alternate "SDA" passive line)
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 2.54)
					(name "SDI_OUT_SEL")
					(number "14")
				)
				(pin no_connect line
					(at 26.67 -44.45 180)
					(length 2.54)
					(hide yes)
					(name "RSV2")
					(number "15")
				)
				(pin no_connect line
					(at 26.67 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "RSV3")
					(number "16")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 2.54)
					(name "OUT_CTRL")
					(number "17")
				)
				(pin passive line
					(at 29.21 -26.67 180)
					(length 2.54)
					(name "IN0-")
					(number "18")
				)
				(pin passive line
					(at 29.21 -24.13 180)
					(length 2.54)
					(name "IN0+")
					(number "19")
				)
				(pin passive line
					(at 29.21 -49.53 180)
					(length 2.54)
					(name "VSS")
					(number "20")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD_CDR")
					(number "21")
				)
				(pin passive line
					(at 29.21 -34.29 180)
					(length 2.54)
					(name "OUT0-")
					(number "22")
				)
				(pin passive line
					(at 29.21 -31.75 180)
					(length 2.54)
					(name "OUT0+")
					(number "23")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 2.54)
					(name "SDI_VOD")
					(number "24")
				)
				(pin no_connect line
					(at 26.67 -46.99 180)
					(length 2.54)
					(hide yes)
					(name "RSV4")
					(number "25")
				)
				(pin no_connect line
					(at 26.67 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "RSV5")
					(number "26")
				)
				(pin passive line
					(at 29.21 -41.91 180)
					(length 2.54)
					(name "~{LOCK}")
					(number "27")
				)
				(pin output line
					(at 0 -19.05 0)
					(length 2.54)
					(name "MISO")
					(number "28")
					(alternate "ADDR1" passive line)
				)
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "SCK")
					(number "29")
					(alternate "SCL" passive line)
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "30")
				)
				(pin power_out line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDD_LDO")
					(number "31")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "ENABLE")
					(number "32")
				)
				(pin power_in line
					(at 29.21 -52.07 180)
					(length 2.54)
					(name "EP")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
