(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LMK04828BISQ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LMK04828BISQ"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LMK04828BISQ"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.ti.com/lit/gpn/lmk04828"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Ultra Low Jitter Synthesizer and Jitter Cleaner"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LMK04828BISQ/NOPB"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, IC, CLOCK, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LMK04828BISQ_1_1"
				(pin output line
					(at 38.1 0 180)
					(length 2.54)
					(name "DCLKOUT0_1")
					(number "1")
				)
				(pin output line
					(at 38.1 -2.54 180)
					(length 2.54)
					(name "DCLKOUT0_2")
					(number "2")
				)
				(pin output line
					(at 38.1 -5.08 180)
					(length 2.54)
					(name "SDCLKOUT1_1")
					(number "3")
				)
				(pin output line
					(at 38.1 -7.62 180)
					(length 2.54)
					(name "SDCLKOUT1_2")
					(number "4")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 2.54)
					(name "RESET")
					(number "5")
					(alternate "GPO" output line)
				)
				(pin input line
					(at 0 -34.29 0)
					(length 2.54)
					(name "SYNC")
					(number "6")
					(alternate "SYSREF_REQ" input line)
				)
				(pin no_connect line
					(at 35.56 -74.93 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin no_connect line
					(at 35.56 -76.2 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "8")
				)
				(pin no_connect line
					(at 35.56 -77.47 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC1_VCO")
					(number "10")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 2.54)
					(name "LDOBYP1")
					(number "11")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 2.54)
					(name "LDOBYP2")
					(number "12")
				)
				(pin output line
					(at 38.1 -15.24 180)
					(length 2.54)
					(name "SDCLKOUT3_1")
					(number "13")
				)
				(pin output line
					(at 38.1 -17.78 180)
					(length 2.54)
					(name "SDCLKOUT3_2")
					(number "14")
				)
				(pin output line
					(at 38.1 -10.16 180)
					(length 2.54)
					(name "DCLKOUT2_1")
					(number "15")
				)
				(pin output line
					(at 38.1 -12.7 180)
					(length 2.54)
					(name "DCLKOUT2_2")
					(number "16")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VCC2_CG1")
					(number "17")
				)
				(pin input line
					(at 0 -46.99 0)
					(length 2.54)
					(name "CS")
					(number "18")
				)
				(pin input line
					(at 0 -44.45 0)
					(length 2.54)
					(name "SCK")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 2.54)
					(name "SDIO")
					(number "20")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VCC3_SYSREF")
					(number "21")
				)
				(pin output line
					(at 38.1 -25.4 180)
					(length 2.54)
					(name "SDCLKOUT5_1")
					(number "22")
				)
				(pin output line
					(at 38.1 -27.94 180)
					(length 2.54)
					(name "SDCLKOUT5_2")
					(number "23")
				)
				(pin output line
					(at 38.1 -20.32 180)
					(length 2.54)
					(name "DCLKOUT4_1")
					(number "24")
				)
				(pin output line
					(at 38.1 -22.86 180)
					(length 2.54)
					(name "DCLKOUT4_2")
					(number "25")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VCC4_CG2")
					(number "26")
				)
				(pin output line
					(at 38.1 -30.48 180)
					(length 2.54)
					(name "DCLKOUT6_1")
					(number "27")
				)
				(pin output line
					(at 38.1 -33.02 180)
					(length 2.54)
					(name "DCLKOUT6_2")
					(number "28")
				)
				(pin output line
					(at 38.1 -35.56 180)
					(length 2.54)
					(name "SDCLKOUT7_1")
					(number "29")
				)
				(pin output line
					(at 38.1 -38.1 180)
					(length 2.54)
					(name "SDCLKOUT7_2")
					(number "30")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 2.54)
					(name "STATUS_LD1")
					(number "31")
				)
				(pin output line
					(at 0 -72.39 0)
					(length 2.54)
					(name "CPOUT1")
					(number "32")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VCC5_DIG")
					(number "33")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 2.54)
					(name "CLKIN1")
					(number "34")
					(alternate "FBCLKIN_1" passive line)
					(alternate "FIN" passive line)
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 2.54)
					(hide yes)
					(name "CLKIN1")
					(number "35")
					(alternate "FBCLKIN_2" input line)
					(alternate "FIN" input line)
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "VCC6_PLL1")
					(number "36")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 2.54)
					(name "CLKIN0_1")
					(number "37")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 2.54)
					(name "CLKIN0_2")
					(number "38")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "VCC7_OSCOUT")
					(number "39")
				)
				(pin passive line
					(at 38.1 -72.39 180)
					(length 2.54)
					(name "OSCOUT")
					(number "40")
					(alternate "CLKIN2_1" passive line)
				)
				(pin passive line
					(at 38.1 -72.39 180)
					(length 2.54)
					(hide yes)
					(name "OSCOUT")
					(number "41")
					(alternate "CLKIN2_2" input line)
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "VCC8_OSCIN")
					(number "42")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 2.54)
					(name "OSCIN_1")
					(number "43")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 2.54)
					(name "OSCIN_2")
					(number "44")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "VCC9_CP2")
					(number "45")
				)
				(pin output line
					(at 0 -74.93 0)
					(length 2.54)
					(name "CPOUT2")
					(number "46")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 2.54)
					(name "VCC10_PLL2")
					(number "47")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 2.54)
					(name "STATUS_LD2")
					(number "48")
				)
				(pin output line
					(at 38.1 -45.72 180)
					(length 2.54)
					(name "SDCLKOUT9_1")
					(number "49")
				)
				(pin output line
					(at 38.1 -48.26 180)
					(length 2.54)
					(name "SDCLKOUT9_2")
					(number "50")
				)
				(pin output line
					(at 38.1 -40.64 180)
					(length 2.54)
					(name "DCLKOUT8_1")
					(number "51")
				)
				(pin output line
					(at 38.1 -43.18 180)
					(length 2.54)
					(name "DCLKOUT8_2")
					(number "52")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 2.54)
					(name "VCC11_CG3")
					(number "53")
				)
				(pin output line
					(at 38.1 -50.8 180)
					(length 2.54)
					(name "DCLKOUT10_1")
					(number "54")
				)
				(pin output line
					(at 38.1 -53.34 180)
					(length 2.54)
					(name "DCLKOUT10_2")
					(number "55")
				)
				(pin output line
					(at 38.1 -55.88 180)
					(length 2.54)
					(name "SDCLKOUT11_1")
					(number "56")
				)
				(pin output line
					(at 38.1 -58.42 180)
					(length 2.54)
					(name "SDCLKOUT11_2")
					(number "57")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 2.54)
					(name "CLKIN_SEL0")
					(number "58")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 2.54)
					(name "CLKIN_SEL1")
					(number "59")
				)
				(pin output line
					(at 38.1 -66.04 180)
					(length 2.54)
					(name "SDCLKOUT13_1")
					(number "60")
				)
				(pin output line
					(at 38.1 -68.58 180)
					(length 2.54)
					(name "SDCLKOUT13_2")
					(number "61")
				)
				(pin output line
					(at 38.1 -60.96 180)
					(length 2.54)
					(name "DCLKOUT12_1")
					(number "62")
				)
				(pin output line
					(at 38.1 -63.5 180)
					(length 2.54)
					(name "DCLKOUT12_2")
					(number "63")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 2.54)
					(name "VCC12_CG0")
					(number "64")
				)
				(pin power_in line
					(at 38.1 -81.28 180)
					(length 2.54)
					(name "GND")
					(number "65")
				)
			)
			(embedded_fonts no)
		)
)
