(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LMK1C1102DQFT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 27.94 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LMK1C1102DQFT"
				(at 27.94 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LMK1C1102DQFT"
				(at 27.94 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lmk1c1102.pdf"
				(at 27.94 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Clock Buffer 2-channel output LVC MOS 1.8-V buffer 8"
				(at 27.94 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 27.94 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LMK1C1102DQFT"
				(at 27.94 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 27.94 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, IC, CLOCK, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LMK1C1102DQFT_1_1"
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "CLKIN")
					(number "1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "1G")
					(number "2")
				)
				(pin output line
					(at 16.51 0 180)
					(length 2.54)
					(name "Y0")
					(number "3")
				)
				(pin power_in line
					(at 16.51 -5.08 180)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin no_connect line
					(at 11.43 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "6")
				)
				(pin no_connect line
					(at 11.43 -6.35 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin output line
					(at 16.51 -2.54 180)
					(length 2.54)
					(name "Y1")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
