(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LPC11U24FHI33"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LPC11U24FHI33"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LPC11U24FHI33"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC11U1X.pdf"
				(at 43.18 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ARM MCU, LPC Family LPC1100 Series Microcontrollers, ARM Cortex-M0, 32 bit, 50 MHz, 32 KB"
				(at 43.18 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "NXP"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LPC11U24FHI33/301"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MICROCONTROLLER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LPC11U24FHI33_1_1"
				(pin passive line
					(at 27.94 -48.26 180)
					(length 2.54)
					(name "PIO1_19")
					(number "1")
					(alternate "SSEL1" passive line)
					(alternate "~{DTR}" passive line)
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{RESET}")
					(number "2")
					(alternate "PIO_0" passive line)
				)
				(pin passive line
					(at 27.94 0 180)
					(length 2.54)
					(name "PIO0_1")
					(number "3")
					(alternate "CLKOUT" passive line)
					(alternate "CT32B0_MAT2" passive line)
					(alternate "USB_FTOGGLE" passive line)
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "XTALIN")
					(number "4")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "XTALOUT")
					(number "5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "6")
				)
				(pin passive line
					(at 27.94 -34.29 180)
					(length 2.54)
					(name "PIO0_20")
					(number "7")
					(alternate "CT16B1_CAP0" passive line)
				)
				(pin passive line
					(at 27.94 -2.54 180)
					(length 2.54)
					(name "PIO0_2")
					(number "8")
					(alternate "CT16B0_CAP0" passive line)
					(alternate "SSEL0" passive line)
				)
				(pin passive line
					(at 27.94 -5.08 180)
					(length 2.54)
					(name "PIO0_3")
					(number "9")
					(alternate "USB_VBUS" passive line)
				)
				(pin passive line
					(at 27.94 -7.62 180)
					(length 2.54)
					(name "PIO0_4")
					(number "10")
					(alternate "SCL" passive line)
				)
				(pin passive line
					(at 27.94 -10.16 180)
					(length 2.54)
					(name "PIO0_5")
					(number "11")
					(alternate "SDA" passive line)
				)
				(pin passive line
					(at 27.94 -36.83 180)
					(length 2.54)
					(name "PIO0_21")
					(number "12")
					(alternate "CT16B1_MAT0" passive line)
					(alternate "MOSI1" passive line)
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "USB_DM")
					(number "13")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "USB_DP")
					(number "14")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 2.54)
					(name "PIO0_6")
					(number "15")
					(alternate "SCK0" passive line)
					(alternate "~{USB_CONNECT}" passive line)
				)
				(pin passive line
					(at 27.94 -15.24 180)
					(length 2.54)
					(name "PIO0_7")
					(number "16")
					(alternate "~{CTS}" passive line)
				)
				(pin passive line
					(at 27.94 -17.78 180)
					(length 2.54)
					(name "PIO0_8")
					(number "17")
					(alternate "CT16B0_MAT0" passive line)
					(alternate "MISO0" passive line)
				)
				(pin passive line
					(at 27.94 -20.32 180)
					(length 2.54)
					(name "PIO0_9")
					(number "18")
					(alternate "CT16B0_MAT1" passive line)
					(alternate "MOSI0" passive line)
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(name "SWCLK")
					(number "19")
					(alternate "CT16B0_MAT2" passive line)
					(alternate "PIO0_10" passive line)
					(alternate "SCK0" passive line)
				)
				(pin passive line
					(at 27.94 -39.37 180)
					(length 2.54)
					(name "PIO0_22")
					(number "20")
					(alternate "AD6" passive line)
					(alternate "CT16B1_MAT1" passive line)
					(alternate "MISO1" passive line)
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "TDI")
					(number "21")
					(alternate "AD0" passive line)
					(alternate "CT32B0_MAT3" passive line)
					(alternate "PIO0_11" passive line)
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "TMS")
					(number "22")
					(alternate "AD1" passive line)
					(alternate "CT32B1_CAP0" passive line)
					(alternate "PIO0_12" passive line)
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "TDO")
					(number "23")
					(alternate "AD2" passive line)
					(alternate "CT32B1_MAT0" passive line)
					(alternate "PIO0_13" passive line)
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "~{TRST}")
					(number "24")
					(alternate "AD3" passive line)
					(alternate "CT32B1_MAT1" passive line)
					(alternate "PIO0_14" passive line)
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "SWDIO")
					(number "25")
					(alternate "AD4" passive line)
					(alternate "CT32B1_MAT2" passive line)
					(alternate "PIO0_15" passive line)
				)
				(pin passive line
					(at 27.94 -24.13 180)
					(length 2.54)
					(name "PIO0_16")
					(number "26")
					(alternate "AD5" passive line)
					(alternate "CT32B1_MAT3" passive line)
					(alternate "WAKEUP" passive line)
				)
				(pin passive line
					(at 27.94 -41.91 180)
					(length 2.54)
					(name "PIO0_23")
					(number "27")
					(alternate "AD7" passive line)
				)
				(pin passive line
					(at 27.94 -45.72 180)
					(length 2.54)
					(name "PIO1_15")
					(number "28")
					(alternate "CT16B0_MAT2" passive line)
					(alternate "SCK1" passive line)
					(alternate "~{DCD}" passive line)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "29")
				)
				(pin passive line
					(at 27.94 -26.67 180)
					(length 2.54)
					(name "PIO0_17")
					(number "30")
					(alternate "CT32B0_CAP0" passive line)
					(alternate "SCLK" passive line)
					(alternate "~{RTS}" passive line)
				)
				(pin passive line
					(at 27.94 -29.21 180)
					(length 2.54)
					(name "PIO0_18")
					(number "31")
					(alternate "CT32B0_MAT0" passive line)
					(alternate "RXD" passive line)
				)
				(pin passive line
					(at 27.94 -31.75 180)
					(length 2.54)
					(name "PIO0_19")
					(number "32")
					(alternate "CT32B0_MAT1" passive line)
					(alternate "TXD" passive line)
				)
				(pin power_in line
					(at 0 -48.26 0)
					(length 2.54)
					(name "VSS")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
