(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LPC5536JBD100E"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 63.5 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LPC5536JBD100E"
				(at 63.5 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LPC5536JBD100E"
				(at 63.5 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC553x.pdf"
				(at 63.5 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ARM Microcontrollers - MCU Arm Cortex-M33-based Microcontroller with 8KB Cache"
				(at 63.5 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LPC5536JBD100E"
				(at 63.5 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "NXP Semiconductors"
				(at 63.5 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 63.5 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 63.5 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "MICROCONTROLLER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LPC5536JBD100E_1_1"
				(pin input line
					(at 0 -34.29 0)
					(length 3.81)
					(name "OPAMP2_INN")
					(number "2")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 3.81)
					(name "ADC1IN1B")
					(number "7")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 3.81)
					(name "ADC1IN1A")
					(number "8")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VDDIO_1")
					(number "12")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDDA")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 3.81)
					(name "VREF_OUT")
					(number "14")
					(alternate "ADC0IN5A" passive line)
					(alternate "ADC1IN5A" passive line)
				)
				(pin input line
					(at 0 -38.1 0)
					(length 3.81)
					(name "VREFP")
					(number "15")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 3.81)
					(name "VREFN")
					(number "16")
					(alternate "ADC0IN5B" passive line)
					(alternate "ADC1IN5B" passive line)
				)
				(pin power_in line
					(at 39.37 -57.15 180)
					(length 3.81)
					(name "VSSA")
					(number "17")
				)
				(pin passive line
					(at 39.37 -57.15 180)
					(length 3.81)
					(hide yes)
					(name "VSSA")
					(number "18")
				)
				(pin input line
					(at 0 -29.21 0)
					(length 3.81)
					(name "OPAMP0_INN")
					(number "27")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 3.81)
					(name "OPAMP1_INN")
					(number "29")
				)
				(pin bidirectional line
					(at 39.37 -3.81 180)
					(length 3.81)
					(name "DAC0_OUT")
					(number "31")
					(alternate "ADC0IN4A" passive line)
					(alternate "ADC1IN4A" passive line)
					(alternate "HSCMP0_IN5" passive line)
				)
				(pin output clock
					(at 0 -57.15 0)
					(length 3.81)
					(name "XTAL32M_N")
					(number "32")
				)
				(pin input clock
					(at 0 -54.61 0)
					(length 3.81)
					(name "XTAL32M_P")
					(number "33")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 3.81)
					(name "~{RESET}")
					(number "34")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDD_CORE")
					(number "38")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "VDDIO_1")
					(number "43")
				)
				(pin power_in line
					(at 39.37 -54.61 180)
					(length 3.81)
					(name "VSS_MAIN_PWR")
					(number "44")
				)
				(pin power_in line
					(at 39.37 -52.07 180)
					(length 3.81)
					(name "VSS_MAIN")
					(number "45")
				)
				(pin output line
					(at 39.37 0 180)
					(length 3.81)
					(name "LX")
					(number "46")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDD_MAIN_PWR")
					(number "47")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDD_MAIN")
					(number "48")
				)
				(pin input clock
					(at 0 -48.26 0)
					(length 3.81)
					(name "XTAL32K_P")
					(number "51")
				)
				(pin output clock
					(at 0 -50.8 0)
					(length 3.81)
					(name "XTAL32K_N")
					(number "52")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VBAT")
					(number "53")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 3.81)
					(name "VDDIO_2")
					(number "63")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "VDDIO_2")
					(number "74")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "VDDIO_2")
					(number "85")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "VDDIO_2")
					(number "96")
				)
				(pin power_in line
					(at 39.37 -36.83 180)
					(length 3.81)
					(name "USB0_3V3")
					(number "97")
				)
				(pin bidirectional line
					(at 39.37 -39.37 180)
					(length 3.81)
					(name "USB0_DP")
					(number "98")
				)
				(pin bidirectional line
					(at 39.37 -41.91 180)
					(length 3.81)
					(name "USB0_DM")
					(number "99")
				)
				(pin power_in line
					(at 39.37 -44.45 180)
					(length 3.81)
					(name "USB0_VSS")
					(number "100")
				)
				(pin power_in line
					(at 39.37 -49.53 180)
					(length 3.81)
					(name "VSS")
					(number "101")
				)
			)
			(symbol "LPC5536JBD100E_2_1"
				(pin bidirectional line
					(at 39.37 -85.09 180)
					(length 3.81)
					(name "PIO2_1")
					(number "1")
					(alternate "OPAMP2_INP" passive line)
				)
				(pin bidirectional line
					(at 39.37 -60.96 180)
					(length 3.81)
					(name "PIO1_24")
					(number "3")
					(alternate "ADC1IN8B" passive line)
				)
				(pin bidirectional line
					(at 39.37 -17.78 180)
					(length 3.81)
					(name "PIO1_7")
					(number "4")
					(alternate "ADC1IN3B" passive line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PIO0_1")
					(number "5")
					(alternate "ADC1IN2B" passive line)
				)
				(pin bidirectional line
					(at 39.37 0 180)
					(length 3.81)
					(name "PIO1_0")
					(number "6")
					(alternate "ADC1IN0B" passive line)
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PIO0_11")
					(number "9")
					(alternate "ADC1IN2A" passive line)
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PIO0_12")
					(number "10")
					(alternate "ADC1IN3A" passive line)
				)
				(pin bidirectional line
					(at 39.37 -50.8 180)
					(length 3.81)
					(name "PIO1_20")
					(number "11")
					(alternate "ADC1IN8A" passive line)
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "PIO0_23")
					(number "19")
					(alternate "ADC0IN8B" passive line)
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PIO0_16")
					(number "20")
					(alternate "ADC0IN3B" passive line)
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PIO0_10")
					(number "21")
					(alternate "ADC0IN1A" passive line)
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PIO0_15")
					(number "22")
					(alternate "ADC0IN3A" passive line)
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 3.81)
					(name "PIO0_31")
					(number "23")
					(alternate "ADC0IN8A" passive line)
				)
				(pin bidirectional line
					(at 39.37 -82.55 180)
					(length 3.81)
					(name "PIO2_0")
					(number "24")
					(alternate "ADC0IN9A" passive line)
				)
				(pin bidirectional line
					(at 39.37 -22.86 180)
					(length 3.81)
					(name "PIO1_9")
					(number "25")
					(alternate "ADC0IN0A" passive line)
					(alternate "HSCMP0_IN4" passive line)
					(alternate "OPAMP0_OUT" passive line)
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PIO0_8")
					(number "26")
					(alternate "OPAMP0_INP" passive line)
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 3.81)
					(name "PIO0_27")
					(number "28")
					(alternate "OPAMP1_INP" passive line)
				)
				(pin bidirectional line
					(at 39.37 -48.26 180)
					(length 3.81)
					(name "PIO1_19")
					(number "30")
					(alternate "ADC0IN4B" passive line)
					(alternate "DAC1_OUT" passive line)
					(alternate "HSCMP1_IN5" passive line)
				)
				(pin bidirectional line
					(at 39.37 -12.7 180)
					(length 3.81)
					(name "PIO1_5")
					(number "35")
					(alternate "HSCMP0_IN3" passive line)
				)
				(pin bidirectional line
					(at 39.37 -20.32 180)
					(length 3.81)
					(name "PIO1_8")
					(number "36")
				)
				(pin bidirectional line
					(at 39.37 -53.34 180)
					(length 3.81)
					(name "PIO1_21")
					(number "37")
				)
				(pin bidirectional line
					(at 39.37 -25.4 180)
					(length 3.81)
					(name "PIO1_10")
					(number "39")
					(alternate "HSCMP1_IN3" passive line)
				)
				(pin bidirectional line
					(at 39.37 -55.88 180)
					(length 3.81)
					(name "PIO1_22")
					(number "40")
					(alternate "DAC0_OUT" passive line)
					(alternate "HSCMP1_IN1" passive line)
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PIO0_17")
					(number "41")
					(alternate "HSCMP2_IN0" passive line)
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PIO0_7")
					(number "42")
					(alternate "HSCMP1_IN0" passive line)
				)
				(pin bidirectional line
					(at 39.37 -58.42 180)
					(length 3.81)
					(name "PIO1_23")
					(number "49")
					(alternate "HSCMP2_IN1" passive line)
				)
				(pin bidirectional line
					(at 39.37 -15.24 180)
					(length 3.81)
					(name "PIO1_6")
					(number "50")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "PIO0_0")
					(number "54")
					(alternate "ACMP0_A" passive line)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PIO0_9")
					(number "55")
					(alternate "ACMP0_B" passive line)
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PIO0_18")
					(number "56")
					(alternate "ACMP0_C" passive line)
				)
				(pin bidirectional line
					(at 39.37 -35.56 180)
					(length 3.81)
					(name "PIO1_14")
					(number "57")
					(alternate "ACMP0_D" passive line)
				)
				(pin bidirectional line
					(at 39.37 -33.02 180)
					(length 3.81)
					(name "PIO1_13")
					(number "58")
					(alternate "ACMP0VREF" passive line)
				)
				(pin bidirectional line
					(at 39.37 -2.54 180)
					(length 3.81)
					(name "PIO1_1")
					(number "59")
					(alternate "TAMPER0" passive line)
					(alternate "WAKEUP0" passive line)
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 3.81)
					(name "PIO0_26")
					(number "60")
					(alternate "TAMPER2" passive line)
					(alternate "WAKEUP4" passive line)
				)
				(pin bidirectional line
					(at 39.37 -5.08 180)
					(length 3.81)
					(name "PIO1_2")
					(number "61")
				)
				(pin bidirectional line
					(at 39.37 -7.62 180)
					(length 3.81)
					(name "PIO1_3")
					(number "62")
				)
				(pin bidirectional line
					(at 39.37 -45.72 180)
					(length 3.81)
					(name "PIO1_18")
					(number "64")
					(alternate "TAMPER3" passive line)
					(alternate "WAKEUP2" passive line)
				)
				(pin bidirectional line
					(at 39.37 -76.2 180)
					(length 3.81)
					(name "PIO1_30")
					(number "65")
					(alternate "WAKEUP3" passive line)
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 3.81)
					(name "PIO0_28")
					(number "66")
					(alternate "TAMPER1" passive line)
					(alternate "WAKEUP1" passive line)
				)
				(pin bidirectional line
					(at 39.37 -30.48 180)
					(length 3.81)
					(name "PIO1_12")
					(number "67")
					(alternate "HSCMP0_IN1" passive line)
				)
				(pin bidirectional line
					(at 39.37 -66.04 180)
					(length 3.81)
					(name "PIO1_26")
					(number "68")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "PIO0_24")
					(number "69")
					(alternate "HSCMP0_IN0" passive line)
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PIO0_13")
					(number "70")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PIO0_14")
					(number "71")
				)
				(pin bidirectional line
					(at 39.37 -71.12 180)
					(length 3.81)
					(name "PIO1_28")
					(number "72")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "PIO0_20")
					(number "73")
				)
				(pin bidirectional line
					(at 39.37 -10.16 180)
					(length 3.81)
					(name "PIO1_4")
					(number "75")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PIO0_21")
					(number "76")
				)
				(pin bidirectional line
					(at 39.37 -63.5 180)
					(length 3.81)
					(name "PIO1_25")
					(number "77")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "PIO0_22")
					(number "78")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 3.81)
					(name "PIO0_25")
					(number "79")
				)
				(pin bidirectional line
					(at 39.37 -73.66 180)
					(length 3.81)
					(name "PIO1_29")
					(number "80")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PIO0_2")
					(number "81")
					(alternate "TRST" passive line)
				)
				(pin bidirectional line
					(at 39.37 -38.1 180)
					(length 3.81)
					(name "PIO1_15")
					(number "82")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PIO0_19")
					(number "83")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PIO0_3")
					(number "84")
					(alternate "TCK" passive line)
				)
				(pin bidirectional line
					(at 39.37 -68.58 180)
					(length 3.81)
					(name "PIO1_27")
					(number "86")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PIO0_4")
					(number "87")
					(alternate "TMS" passive line)
				)
				(pin bidirectional line
					(at 39.37 -40.64 180)
					(length 3.81)
					(name "PIO1_16")
					(number "88")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PIO0_6")
					(number "89")
					(alternate "TDO" passive line)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PIO0_5")
					(number "90")
					(alternate "TDI" passive line)
				)
				(pin bidirectional line
					(at 39.37 -43.18 180)
					(length 3.81)
					(name "PIO1_17")
					(number "91")
				)
				(pin bidirectional line
					(at 39.37 -78.74 180)
					(length 3.81)
					(name "PIO1_31")
					(number "92")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 3.81)
					(name "PIO0_29")
					(number "93")
				)
				(pin bidirectional line
					(at 39.37 -27.94 180)
					(length 3.81)
					(name "PIO1_11")
					(number "94")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 3.81)
					(name "PIO0_30")
					(number "95")
				)
			)
			(embedded_fonts no)
		)
)
