(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LT4356IMS_MSOP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 27.94 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LT4356IMS_MSOP"
				(at 27.94 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LT4356IMS_MSOP"
				(at 27.94 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.linear.com/docs/25228"
				(at 27.94 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Surge suppression IC"
				(at 27.94 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LT4356IMS-1#PBF"
				(at 27.94 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Maxim Integrated Products"
				(at 27.94 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 27.94 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LT4356IMS_MSOP_1_1"
				(pin input line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "FB")
					(number "1")
				)
				(pin output line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "OUT")
					(number "2")
				)
				(pin input line
					(at 17.78 0 180)
					(length 2.54)
					(name "GATE")
					(number "3")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SNS")
					(number "4")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "5")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{SHDN}")
					(number "6")
				)
				(pin output line
					(at 17.78 -10.16 180)
					(length 2.54)
					(name "~{FLT}")
					(number "7")
				)
				(pin output line
					(at 17.78 -7.62 180)
					(length 2.54)
					(name "EN")
					(number "8")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "GND")
					(number "9")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "TMR")
					(number "10")
				)
			)
			(embedded_fonts no)
		)
)
