(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LTC4151-1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LTC4151-1"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LTC4151-1"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4151ff.pdf"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "High Voltage I2C Current and Voltage Monitor, 7V to 80V, 12-bit ADC, Split I2C pins for opto-isolators"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Analog Devices"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LTC4151IMS-1#PBF"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MONITOR, VOLTAGE, IC, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LTC4151-1_1_1"
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(name "SENSE+")
					(number "1")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "2")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "ADR1")
					(number "3")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "ADR0")
					(number "4")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "ADIN")
					(number "5")
				)
				(pin input line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "SCL")
					(number "6")
				)
				(pin input line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "SDAI")
					(number "7")
				)
				(pin output line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "~{SDAO}")
					(number "8")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "GND")
					(number "9")
				)
				(pin input line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "SENSE-")
					(number "10")
				)
			)
			(embedded_fonts no)
		)
)
