(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LTC4312CMS_PBF"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LTC4312CMS_PBF"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LTC4312CMS_PBF"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4312f.pdf"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Pin-Selectable, 2-Channel, 2-Wire Multiplexer with Bus Buffer"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LTC4312CMS#PBF"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 43.18 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "I2C, SMT, IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LTC4312CMS_PBF_1_1"
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "DISCEN")
					(number "1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "2")
				)
				(pin bidirectional line
					(at 26.67 -6.35 180)
					(length 2.54)
					(name "SCLOUT1")
					(number "3")
				)
				(pin bidirectional line
					(at 26.67 -3.81 180)
					(length 2.54)
					(name "SDAOUT1")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "SDAIN")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "SCLIN")
					(number "6")
				)
				(pin bidirectional line
					(at 26.67 -13.97 180)
					(length 2.54)
					(name "SCLOUT2")
					(number "7")
				)
				(pin bidirectional line
					(at 26.67 -11.43 180)
					(length 2.54)
					(name "SDAOUT2")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 2.54)
					(name "ENABLE2")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 2.54)
					(name "ENABLE1")
					(number "10")
				)
				(pin output line
					(at 0 -3.81 0)
					(length 2.54)
					(name "~{FAULT}")
					(number "11")
				)
				(pin power_in line
					(at 26.67 0 180)
					(length 2.54)
					(name "VCC2")
					(number "12")
				)
				(pin no_connect line
					(at 24.13 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "13")
				)
				(pin no_connect line
					(at 24.13 -19.05 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "14")
				)
				(pin power_in line
					(at 0 -24.13 0)
					(length 2.54)
					(name "GND")
					(number "15")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(name "~{ACC}")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
