(footprint "DFN-6-1EP_3x2mm_P0.5mm_EP1.65x1.35mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -1.4 -1.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-6-1EP_3x2mm_P0.5mm_EP1.65x1.35mm"
		(at -1.1 2.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -2.45 3.95 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2.45 5.15 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -2.45 6.35 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.41 -0.34)
		(size 0.67 0.54)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.41 0.34)
		(size 0.67 0.54)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.41 -0.34)
		(size 0.67 0.54)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.41 0.34)
		(size 0.67 0.54)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd rect
		(at -1.425 -0.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.425 0)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.425 0.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.425 0.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.425 0)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.425 -0.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0 0)
		(size 1.65 1.35)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "antmicro_ltc6994cdcb_1_trmpbf.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
