(footprint "DFN-8-1EP_3x2mm_P0.5mm_EP1.36x1.46mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -1.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-8-1EP_3x2mm_P0.5mm_EP1.36x1.46mm"
		(at 0 2.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -2.27 4.052 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2.27 5.253 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -2.27 6.453 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.451 -0.749 270)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.451 -0.25 270)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.451 0.249 270)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.451 0.75 270)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.448 0.75 270)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.448 0.249 270)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.448 -0.25 270)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.448 -0.749 270)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0 0 270)
		(size 1.5 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.1)
	)
	(embedded_fonts no)
	(model "antmicro_m24c64_fmc6tg.glb"
		(offset
			(xyz -0.3 0 0.85)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
)
