(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "M24M01-TSSOP8"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "M24M01-TSSOP8"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "M24M01-TSSOP8"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/m24m01-a125.pdf"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "EEPROM, 128K x 8bit, Serial I2C (2-Wire), 1 MHz, TSSOP, 8 Pins"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "M24M01-DWDW3TP/K"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, STORAGE, I2C, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "UFDFPN8DFN8_2X3_STM UFDFPN8DFN8_2X3_STM-M UFDFPN8DFN8_2X3_STM-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "M24M01-TSSOP8_1_1"
				(pin no_connect line
					(at 2.54 -6.35 0)
					(length 2.54)
					(hide yes)
					(name "E0")
					(number "1")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "E1")
					(number "2")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "E2")
					(number "3")
				)
				(pin power_in line
					(at 15.24 -11.43 180)
					(length 2.54)
					(name "VSS")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SDA")
					(number "5")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "SCL")
					(number "6")
				)
				(pin input line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "~{WC}")
					(number "7")
				)
				(pin power_in line
					(at 15.24 0 180)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
