(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX22191"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX22191"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX22191"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX22191.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Ultra-Low-Power, Parasitically Powered Digital Input Digital Isolator"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX22191AUT+T"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, TRANSCEIVER, CAN, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX22191_1_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "IN")
					(number "1")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin passive line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "REXT")
					(number "3")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "TEST")
					(number "4")
				)
				(pin passive line
					(at 17.78 -10.16 180)
					(length 2.54)
					(name "VCC")
					(number "5")
				)
				(pin output line
					(at 17.78 0 180)
					(length 2.54)
					(name "OUT")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
