(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX3221IPWR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX3221IPWR"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX3221IPWR"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/gpn/MAX3221"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "3-V to 5.5-V Single-Channel RS-232 Line Driver/Receiver"
				(at 43.18 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX3221IPWR"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, DRIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX3221IPWR_1_1"
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{EN}")
					(number "1")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "C1+")
					(number "2")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 2.54)
					(name "V+")
					(number "3")
				)
				(pin passive line
					(at 22.86 -10.16 180)
					(length 2.54)
					(name "C1-")
					(number "4")
				)
				(pin passive line
					(at 22.86 -15.24 180)
					(length 2.54)
					(name "C2+")
					(number "5")
				)
				(pin passive line
					(at 22.86 -17.78 180)
					(length 2.54)
					(name "C2-")
					(number "6")
				)
				(pin passive line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "V-")
					(number "7")
				)
				(pin input line
					(at 22.86 -25.4 180)
					(length 2.54)
					(name "RIN")
					(number "8")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 2.54)
					(name "ROUT")
					(number "9")
				)
				(pin output line
					(at 22.86 -30.48 180)
					(length 2.54)
					(name "~{INVALID}")
					(number "10")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "DIN")
					(number "11")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "FORCEON")
					(number "12")
				)
				(pin output line
					(at 22.86 -22.86 180)
					(length 2.54)
					(name "DOUT")
					(number "13")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 2.54)
					(name "GND")
					(number "14")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "15")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{FORCEOFF}")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
