(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX32650GCE+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX32650GCE+"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX32650GCE+"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/609/MAX32650_MAX32652-3469593.pdf"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ARM MCU, DARWIN Family MAX326xx Series Microcontroller, ARM Cortex-M4, 32 bit, 120 MHz, 3 MB"
				(at 43.18 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX32650GCE+"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "MCU, SMT, MICROCONTROLLER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "21-0087_C144+1C_MXM 21-0087_C144+1C_MXM-M 21-0087_C144+1C_MXM-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX32650GCE+_1_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "5")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDDIOH")
					(number "9")
				)
				(pin power_in line
					(at 29.21 -36.83 180)
					(length 3.81)
					(name "VSS")
					(number "11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VCORE")
					(number "14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDDIOH")
					(number "18")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDDIO")
					(number "21")
				)
				(pin passive line
					(at 29.21 -36.83 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "27")
				)
				(pin passive line
					(at 29.21 -36.83 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "29")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDDIO")
					(number "33")
				)
				(pin passive line
					(at 29.21 -36.83 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "47")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDDIOH")
					(number "54")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDDIO")
					(number "55")
				)
				(pin passive line
					(at 29.21 -36.83 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "60")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 3.81)
					(name "HYP_CLKN")
					(number "64")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 3.81)
					(name "HYP_CLK")
					(number "65")
				)
				(pin no_connect line
					(at 25.4 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "73")
				)
				(pin no_connect line
					(at 25.4 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "74")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDDB")
					(number "76")
				)
				(pin no_connect line
					(at 25.4 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "77")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "DP")
					(number "78")
				)
				(pin no_connect line
					(at 25.4 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "79")
				)
				(pin passive line
					(at 29.21 -36.83 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "80")
				)
				(pin passive line
					(at 29.21 -36.83 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "81")
				)
				(pin no_connect line
					(at 25.4 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "82")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "DM")
					(number "83")
				)
				(pin no_connect line
					(at 25.4 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "84")
				)
				(pin passive line
					(at 29.21 -36.83 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "85")
				)
				(pin no_connect line
					(at 25.4 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "86")
				)
				(pin no_connect line
					(at 25.4 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "87")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "88")
				)
				(pin passive line
					(at 29.21 -36.83 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "89")
				)
				(pin power_in line
					(at 29.21 -34.29 180)
					(length 3.81)
					(name "VSSA")
					(number "98")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDDA")
					(number "99")
				)
				(pin no_connect line
					(at 25.4 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "105")
				)
				(pin output line
					(at 0 -36.83 0)
					(length 3.81)
					(name "32KOUT")
					(number "106")
				)
				(pin input line
					(at 0 -34.29 0)
					(length 3.81)
					(name "32KIN")
					(number "107")
				)
				(pin no_connect line
					(at 25.4 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "108")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VRTC")
					(number "111")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 3.81)
					(name "RSTN")
					(number "114")
				)
				(pin passive line
					(at 29.21 -36.83 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "119")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDDIO")
					(number "126")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDDIOH")
					(number "128")
				)
				(pin passive line
					(at 29.21 -36.83 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "136")
				)
			)
			(symbol "MAX32650GCE+_2_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "P0.1")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "P0.2")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "P0.3")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "P0.4")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "P0.5")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "P0.6")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "P0.22")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "P0.7")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "P0.8")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "P0.9")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "P0.10")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "P0.11")
					(number "22")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "P0.12")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "P0.23")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "P0.13")
					(number "25")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "P0.14")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "P0.15")
					(number "28")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "P0.16")
					(number "30")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "P0.17")
					(number "31")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "P0.18")
					(number "32")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "P0.19")
					(number "34")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "P0.20")
					(number "35")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "P0.21")
					(number "36")
				)
				(pin bidirectional line
					(at 29.21 0 180)
					(length 3.81)
					(name "P1.0")
					(number "37")
				)
				(pin bidirectional line
					(at 29.21 -17.78 180)
					(length 3.81)
					(name "P1.7")
					(number "38")
				)
				(pin bidirectional line
					(at 29.21 -2.54 180)
					(length 3.81)
					(name "P1.1")
					(number "39")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "P0.24")
					(number "40")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "P0.25")
					(number "41")
				)
				(pin bidirectional line
					(at 29.21 -5.08 180)
					(length 3.81)
					(name "P1.2")
					(number "42")
				)
				(pin bidirectional line
					(at 29.21 -7.62 180)
					(length 3.81)
					(name "P1.3")
					(number "43")
				)
				(pin bidirectional line
					(at 29.21 -10.16 180)
					(length 3.81)
					(name "P1.4")
					(number "45")
				)
				(pin bidirectional line
					(at 29.21 -20.32 180)
					(length 3.81)
					(name "P1.8")
					(number "46")
				)
				(pin bidirectional line
					(at 29.21 -22.86 180)
					(length 3.81)
					(name "P1.9")
					(number "48")
				)
				(pin bidirectional line
					(at 29.21 -15.24 180)
					(length 3.81)
					(name "P1.6")
					(number "49")
				)
				(pin bidirectional line
					(at 29.21 -25.4 180)
					(length 3.81)
					(name "P1.10")
					(number "50")
				)
				(pin bidirectional line
					(at 29.21 -12.7 180)
					(length 3.81)
					(name "P1.5")
					(number "51")
				)
				(pin bidirectional line
					(at 29.21 -27.94 180)
					(length 3.81)
					(name "P1.11")
					(number "52")
				)
				(pin bidirectional line
					(at 29.21 -30.48 180)
					(length 3.81)
					(name "P1.12")
					(number "53")
				)
				(pin bidirectional line
					(at 29.21 -33.02 180)
					(length 3.81)
					(name "P1.13")
					(number "56")
				)
				(pin bidirectional line
					(at 29.21 -38.1 180)
					(length 3.81)
					(name "P1.15")
					(number "58")
				)
				(pin bidirectional line
					(at 29.21 -40.64 180)
					(length 3.81)
					(name "P1.16")
					(number "59")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 3.81)
					(name "P0.31")
					(number "61")
				)
				(pin bidirectional line
					(at 29.21 -48.26 180)
					(length 3.81)
					(name "P1.19")
					(number "62")
				)
				(pin bidirectional line
					(at 29.21 -45.72 180)
					(length 3.81)
					(name "P1.18")
					(number "63")
				)
				(pin bidirectional line
					(at 29.21 -50.8 180)
					(length 3.81)
					(name "P1.20")
					(number "66")
				)
				(pin bidirectional line
					(at 29.21 -53.34 180)
					(length 3.81)
					(name "P1.21")
					(number "67")
				)
				(pin bidirectional line
					(at 29.21 -35.56 180)
					(length 3.81)
					(name "P1.14")
					(number "68")
				)
				(pin bidirectional line
					(at 29.21 -43.18 180)
					(length 3.81)
					(name "P1.17")
					(number "69")
				)
				(pin bidirectional line
					(at 29.21 -58.42 180)
					(length 3.81)
					(name "P1.23")
					(number "70")
				)
				(pin bidirectional line
					(at 29.21 -76.2 180)
					(length 3.81)
					(name "P1.30")
					(number "71")
				)
				(pin bidirectional line
					(at 29.21 -63.5 180)
					(length 3.81)
					(name "P1.25")
					(number "72")
				)
				(pin bidirectional line
					(at 29.21 -55.88 180)
					(length 3.81)
					(name "P1.22")
					(number "75")
				)
				(pin bidirectional line
					(at 29.21 -60.96 180)
					(length 3.81)
					(name "P1.24")
					(number "92")
				)
				(pin bidirectional line
					(at 29.21 -78.74 180)
					(length 3.81)
					(name "P1.31")
					(number "93")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 3.81)
					(name "P0.27")
					(number "100")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 3.81)
					(name "P0.26")
					(number "103")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 3.81)
					(name "P0.29")
					(number "110")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 3.81)
					(name "P0.30")
					(number "112")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 3.81)
					(name "P0.28")
					(number "113")
				)
				(pin bidirectional line
					(at 29.21 -66.04 180)
					(length 3.81)
					(name "P1.26")
					(number "115")
				)
				(pin bidirectional line
					(at 29.21 -68.58 180)
					(length 3.81)
					(name "P1.27")
					(number "116")
				)
				(pin bidirectional line
					(at 29.21 -71.12 180)
					(length 3.81)
					(name "P1.28")
					(number "117")
				)
				(pin bidirectional line
					(at 29.21 -73.66 180)
					(length 3.81)
					(name "P1.29")
					(number "118")
				)
			)
			(symbol "MAX32650GCE+_3_1"
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "P2.16")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "P2.30")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "P2.17")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "P2.18")
					(number "20")
				)
				(pin bidirectional line
					(at 29.21 0 180)
					(length 3.81)
					(name "P3.0")
					(number "44")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "P2.23")
					(number "57")
				)
				(pin bidirectional line
					(at 29.21 -22.86 180)
					(length 3.81)
					(name "P3.9")
					(number "90")
				)
				(pin bidirectional line
					(at 29.21 -15.24 180)
					(length 3.81)
					(name "P3.6")
					(number "91")
				)
				(pin bidirectional line
					(at 29.21 -20.32 180)
					(length 3.81)
					(name "P3.8")
					(number "94")
				)
				(pin bidirectional line
					(at 29.21 -12.7 180)
					(length 3.81)
					(name "P3.5")
					(number "95")
				)
				(pin bidirectional line
					(at 29.21 -17.78 180)
					(length 3.81)
					(name "P3.7")
					(number "96")
				)
				(pin bidirectional line
					(at 29.21 -10.16 180)
					(length 3.81)
					(name "P3.4")
					(number "97")
				)
				(pin passive line
					(at 29.21 -58.42 180)
					(length 3.81)
					(name "AIN3")
					(number "101")
				)
				(pin passive line
					(at 29.21 -55.88 180)
					(length 3.81)
					(name "AIN2")
					(number "102")
				)
				(pin passive line
					(at 29.21 -53.34 180)
					(length 3.81)
					(name "AIN1")
					(number "104")
				)
				(pin passive line
					(at 29.21 -50.8 180)
					(length 3.81)
					(name "AIN0")
					(number "109")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "P2.0")
					(number "120")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "P2.1")
					(number "121")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "P2.2")
					(number "122")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "P2.3")
					(number "123")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "P2.4")
					(number "124")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "P2.5")
					(number "125")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "P2.6")
					(number "127")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "P2.7")
					(number "129")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "P2.8")
					(number "130")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "P2.9")
					(number "131")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "P2.11")
					(number "132")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "P2.25")
					(number "133")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "P2.10")
					(number "134")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "P2.26")
					(number "135")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "P2.12")
					(number "137")
				)
				(pin bidirectional line
					(at 29.21 -2.54 180)
					(length 3.81)
					(name "P3.1")
					(number "138")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "P2.28")
					(number "139")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "P2.13")
					(number "140")
				)
				(pin bidirectional line
					(at 29.21 -5.08 180)
					(length 3.81)
					(name "P3.2")
					(number "141")
				)
				(pin bidirectional line
					(at 29.21 -7.62 180)
					(length 3.81)
					(name "P3.3")
					(number "142")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "P2.14")
					(number "143")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "P2.15")
					(number "144")
				)
			)
			(embedded_fonts no)
		)
)
