(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX44263_SC70"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 27.94 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX44263_SC70"
				(at 27.94 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX44263_SC70"
				(at 27.94 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/609/MAX44259_MAX44263-3129068.pdf"
				(at 27.94 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Operational Amplifiers - Op Amps 1.8V, 15MHz, Low-Offset, Dual Op Amp with RRIO"
				(at 27.94 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX44263AXA+T"
				(at 27.94 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 27.94 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 27.94 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, AMP, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX44263_SC70_1_1"
				(text "+"
					(at 3.81 -3.556 0)
				)
				(text "-"
					(at 3.81 -5.842 0)
				)
				(text "+"
					(at 3.81 -9.906 0)
				)
				(text "-"
					(at 3.81 -12.192 0)
				)
				(pin output line
					(at 12.7 -3.81 180)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin power_in line
					(at 0 -13.97 0)
					(length 2.54)
					(name "V-")
					(number "4")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "")
					(number "6")
				)
				(pin output line
					(at 12.7 -10.16 180)
					(length 2.54)
					(name "")
					(number "7")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V+")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
