(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX5419META+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX5419META+"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX5419META+"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max5417-max5419.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Non Volatile Digital Potentiometer, 200 kohm, Single, 2 Wire, I2C, Serial, Linear, 2.7 V"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Analog Devices"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX5419META+"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, DIGITAL, POTENTIOMETER, IC, I2C, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX5419META+_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{DD}")
					(number "1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SCL")
					(number "2")
					(alternate "NC" no_connect line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SDA")
					(number "3")
					(alternate "SDA" bidirectional line)
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "A0")
					(number "4")
					(alternate "SCL" input line)
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin passive line
					(at 16.51 -10.16 180)
					(length 2.54)
					(name "L")
					(number "6")
				)
				(pin passive line
					(at 16.51 -7.62 180)
					(length 2.54)
					(name "W")
					(number "7")
				)
				(pin passive line
					(at 16.51 -5.08 180)
					(length 2.54)
					(name "H")
					(number "8")
				)
				(pin power_in line
					(at 16.51 -15.24 180)
					(length 2.54)
					(name "EP")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
