(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX9295A"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 50.8 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX9295A"
				(at 50.8 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX9295A"
				(at 50.8 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/en/product-category/gigabit-multimedia-serial-link.html"
				(at 50.8 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "CSI-2 to GMSL2/GMSL1 Serializer"
				(at 50.8 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX9295A"
				(at 50.8 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Maxim Integrated Products"
				(at 50.8 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 50.8 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, GMSL"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX9295A_1_1"
				(text "1.2/1.0V"
					(at 7.112 -3.556 0)
				)
				(text "1.8/3.3V"
					(at 17.78 -1.016 0)
				)
				(pin passive line
					(at 35.56 -2.54 180)
					(length 2.54)
					(name "PWDNB")
					(number "1")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 2.54)
					(name "MFP0")
					(number "2")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 2.54)
					(name "MFP1/CFG0")
					(number "3")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 2.54)
					(name "MFP2/CFG1")
					(number "4")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 2.54)
					(name "MFP9")
					(number "5")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 2.54)
					(name "MFP10")
					(number "6")
				)
				(pin passive line
					(at 35.56 -5.08 180)
					(length 2.54)
					(name "VREF")
					(number "7")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "X1/OSC")
					(number "8")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "X2")
					(number "9")
				)
				(pin input line
					(at 0 -41.91 0)
					(length 2.54)
					(name "XRES")
					(number "10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD_1.8V")
					(number "11")
				)
				(pin bidirectional line
					(at 35.56 -8.89 180)
					(length 2.54)
					(name "SIO_P")
					(number "12")
				)
				(pin bidirectional line
					(at 35.56 -11.43 180)
					(length 2.54)
					(name "SIO_N")
					(number "13")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 2.54)
					(name "CAP_VDD")
					(number "14")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "15")
				)
				(pin power_in line
					(at 35.56 0 180)
					(length 2.54)
					(name "VDDIO")
					(number "16")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 2.54)
					(name "MFP3")
					(number "17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 2.54)
					(name "MFP4")
					(number "18")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 2.54)
					(name "D2_P")
					(number "19")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "D2_N")
					(number "20")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 2.54)
					(name "MFP5")
					(number "21")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 2.54)
					(name "MFP6")
					(number "22")
				)
				(pin input line
					(at 0 -26.67 0)
					(length 2.54)
					(name "D3_P")
					(number "23")
				)
				(pin input line
					(at 0 -29.21 0)
					(length 2.54)
					(name "D3_N")
					(number "24")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "D0_P")
					(number "25")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "D0_N")
					(number "26")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "CK_P")
					(number "27")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "CK_N")
					(number "28")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 2.54)
					(name "D1_P")
					(number "29")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "D1_N")
					(number "30")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 2.54)
					(name "MFP7")
					(number "31")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 2.54)
					(name "MFP8")
					(number "32")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 2.54)
					(name "GND")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
