(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX96717GTJ_VY+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.26 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX96717GTJ_VY+"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX96717GTJ_VY+"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max96717.pdf"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "CSI-2 to GMSL2 Serializer"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX96717GTJ/VY+"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, GMSL, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX96717GTJ_VY+_1_1"
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "PWDNB")
					(number "1")
				)
				(pin bidirectional line
					(at 27.94 -27.94 180)
					(length 2.54)
					(name "MFP0")
					(number "2")
					(alternate "GPIO0" bidirectional line)
					(alternate "SCLK" output line)
					(alternate "VTG0" output line)
				)
				(pin bidirectional line
					(at 27.94 -30.48 180)
					(length 2.54)
					(name "MFP1")
					(number "3")
					(alternate "BNE" output line)
					(alternate "CFG0" input line)
					(alternate "GPO1" output line)
					(alternate "SS1" output line)
					(alternate "VTG1" output line)
				)
				(pin bidirectional line
					(at 27.94 -33.02 180)
					(length 2.54)
					(name "MFP2")
					(number "4")
					(alternate "CFG1" input line)
					(alternate "DPLL_OUT(Alt)" output line)
					(alternate "GPO2" output line)
					(alternate "RCLKOUT(Alt)" output line)
					(alternate "VTG2" output line)
				)
				(pin bidirectional line
					(at 27.94 -50.8 180)
					(length 2.54)
					(name "MFP9")
					(number "5")
					(alternate "OD09_GPI9" bidirectional line)
					(alternate "SDA2_RX2" bidirectional line)
					(alternate "SDA_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 27.94 -53.34 180)
					(length 2.54)
					(name "MFP10")
					(number "6")
					(alternate "ODO10_GPI10" bidirectional line)
					(alternate "SCL2_TX2" bidirectional line)
					(alternate "SCL_TX*" bidirectional line)
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "VREF")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "X1/OSC")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "X2")
					(number "9")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(name "XRES")
					(number "10")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD18")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "SIOP")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "SION")
					(number "13")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 2.54)
					(name "CAP_VDD")
					(number "14")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "15")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDDIO")
					(number "16")
				)
				(pin bidirectional line
					(at 27.94 -35.56 180)
					(length 2.54)
					(name "MFP3")
					(number "17")
					(alternate "ADC0" input line)
					(alternate "ERRB" output line)
					(alternate "GPIO3" bidirectional line)
					(alternate "LOCK" output line)
					(alternate "VTG3" output line)
				)
				(pin bidirectional line
					(at 27.94 -38.1 180)
					(length 2.54)
					(name "MFP4")
					(number "18")
					(alternate "DPLL_OUT" output line)
					(alternate "GPIO4" bidirectional line)
					(alternate "RCLKOUT" output line)
					(alternate "RO" input line)
					(alternate "SS2" output line)
					(alternate "VTG4" output line)
				)
				(pin input line
					(at 27.94 -15.24 180)
					(length 2.54)
					(name "D2P")
					(number "19")
				)
				(pin input line
					(at 27.94 -17.78 180)
					(length 2.54)
					(name "D2N")
					(number "20")
				)
				(pin bidirectional line
					(at 27.94 -40.64 180)
					(length 2.54)
					(name "MFP5")
					(number "21")
					(alternate "ADC1" input line)
					(alternate "LMN0" input line)
					(alternate "ODO5_GPI5" input line)
				)
				(pin bidirectional line
					(at 27.94 -43.18 180)
					(length 2.54)
					(name "MFP6")
					(number "22")
					(alternate "ADC2" input line)
					(alternate "LMN1" input line)
					(alternate "ODO6_GPI6" input line)
				)
				(pin input line
					(at 27.94 -20.32 180)
					(length 2.54)
					(name "D3P")
					(number "23")
				)
				(pin input line
					(at 27.94 -22.86 180)
					(length 2.54)
					(name "D3N")
					(number "24")
				)
				(pin input line
					(at 27.94 -5.08 180)
					(length 2.54)
					(name "D0P")
					(number "25")
				)
				(pin input line
					(at 27.94 -7.62 180)
					(length 2.54)
					(name "D0N")
					(number "26")
				)
				(pin input line
					(at 27.94 0 180)
					(length 2.54)
					(name "CKP")
					(number "27")
				)
				(pin input line
					(at 27.94 -2.54 180)
					(length 2.54)
					(name "CKN")
					(number "28")
				)
				(pin input line
					(at 27.94 -10.16 180)
					(length 2.54)
					(name "D1P")
					(number "29")
				)
				(pin input line
					(at 27.94 -12.7 180)
					(length 2.54)
					(name "D1N")
					(number "30")
				)
				(pin bidirectional line
					(at 27.94 -45.72 180)
					(length 2.54)
					(name "MFP7")
					(number "31")
					(alternate "GPI7" input line)
					(alternate "GPIO7" bidirectional line)
					(alternate "LOCK (Alt)" output line)
					(alternate "MOSI" bidirectional line)
					(alternate "RX1" input line)
					(alternate "SDA1" open_collector line)
					(alternate "VTG7" output line)
				)
				(pin bidirectional line
					(at 27.94 -48.26 180)
					(length 2.54)
					(name "MFP8")
					(number "32")
					(alternate "ERRB (Alt)" output line)
					(alternate "GPIO8" bidirectional line)
					(alternate "MISO" input line)
					(alternate "MS" input line)
					(alternate "SCL1" open_collector line)
					(alternate "TX1" output line)
					(alternate "VTG8" output line)
				)
				(pin power_in line
					(at 0 -53.34 0)
					(length 2.54)
					(name "GND")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
