(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX96724GTN_VY+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 50.8 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX96724GTN_VY+"
				(at 50.8 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX96724GTN_VY+"
				(at 50.8 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/609/max96724-3135154.pdf"
				(at 50.8 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ADI GMSL2/1 Tunneling Quad Deserializer 6GHz with 2x4 or 4x2 MIPI DPHY/CPHY Outputs"
				(at 50.8 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX96724GTN/VY+"
				(at 50.8 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 50.8 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 50.8 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, GMSL, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX96724GTN_VY+_1_1"
				(text "1.2/1.0V"
					(at 7.112 -3.556 0)
				)
				(text "1.8/3.3V"
					(at 17.78 -1.016 0)
				)
				(text "1.2V"
					(at 21.082 -6.096 0)
				)
				(text "4-lane"
					(at 21.59 -40.005 900)
				)
				(text "4-lane"
					(at 21.59 -78.74 900)
				)
				(text "2-lane"
					(at 24.765 -31.115 900)
				)
				(text "2-lane"
					(at 24.765 -45.085 900)
				)
				(text "2-lane"
					(at 24.765 -68.58 900)
				)
				(text "2-lane"
					(at 24.765 -83.82 900)
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "MFP0")
					(number "1")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "MFP1")
					(number "2")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 2.54)
					(name "MFP2")
					(number "3")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(name "CFG0")
					(number "4")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "SIOD_P")
					(number "5")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(name "SIOD_N")
					(number "6")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD_1.8V")
					(number "7")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 2.54)
					(hide yes)
					(name "CAP_VDD")
					(number "8")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "SIOC_N")
					(number "9")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "SIOC_P")
					(number "10")
				)
				(pin passive line
					(at 35.56 -2.54 180)
					(length 2.54)
					(name "PWDNB")
					(number "11")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 2.54)
					(name "MFP3")
					(number "12")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 2.54)
					(name "MFP4")
					(number "13")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 2.54)
					(name "MFP5")
					(number "14")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 2.54)
					(name "X1/OSC")
					(number "15")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 2.54)
					(name "X2")
					(number "16")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 2.54)
					(name "XRES")
					(number "17")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "SIOB_P")
					(number "18")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "SIOB_N")
					(number "19")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 2.54)
					(name "CAP_VDD")
					(number "20")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VDD_1.8V")
					(number "21")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "SIOA_N")
					(number "22")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SIOA_P")
					(number "23")
				)
				(pin passive line
					(at 35.56 0 180)
					(length 2.54)
					(name "VDDIO")
					(number "24")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 2.54)
					(name "CFG1/MFP6")
					(number "25")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 2.54)
					(name "SDA1/MFP7")
					(number "26")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 2.54)
					(name "SCL1/MFP8")
					(number "27")
				)
				(pin passive line
					(at 35.56 -12.7 180)
					(length 2.54)
					(name "SDA")
					(number "28")
				)
				(pin passive line
					(at 35.56 -10.16 180)
					(length 2.54)
					(name "SCL")
					(number "29")
				)
				(pin passive line
					(at 35.56 -5.08 180)
					(length 2.54)
					(name "VTERM")
					(number "30")
				)
				(pin passive line
					(at 35.56 -25.4 180)
					(length 2.54)
					(name "DA0_P")
					(number "31")
				)
				(pin passive line
					(at 35.56 -27.94 180)
					(length 2.54)
					(name "DA0_N")
					(number "32")
				)
				(pin passive line
					(at 35.56 -20.32 180)
					(length 2.54)
					(name "CKC_P")
					(number "33")
				)
				(pin passive line
					(at 35.56 -22.86 180)
					(length 2.54)
					(name "CKC_N")
					(number "34")
				)
				(pin passive line
					(at 35.56 -30.48 180)
					(length 2.54)
					(name "DA1_P")
					(number "35")
				)
				(pin passive line
					(at 35.56 -33.02 180)
					(length 2.54)
					(name "DA1_N")
					(number "36")
				)
				(pin passive line
					(at 35.56 -35.56 180)
					(length 2.54)
					(name "DA2_P")
					(number "37")
				)
				(pin passive line
					(at 35.56 -38.1 180)
					(length 2.54)
					(name "DA2_N")
					(number "38")
				)
				(pin passive line
					(at 35.56 -45.72 180)
					(length 2.54)
					(name "CKA_P")
					(number "39")
				)
				(pin passive line
					(at 35.56 -48.26 180)
					(length 2.54)
					(name "CKA_N")
					(number "40")
				)
				(pin passive line
					(at 35.56 -40.64 180)
					(length 2.54)
					(name "DA3_P")
					(number "41")
				)
				(pin passive line
					(at 35.56 -43.18 180)
					(length 2.54)
					(name "DA3_N")
					(number "42")
				)
				(pin passive line
					(at 35.56 -63.5 180)
					(length 2.54)
					(name "DB0_P")
					(number "43")
				)
				(pin passive line
					(at 35.56 -66.04 180)
					(length 2.54)
					(name "DB0_N")
					(number "44")
				)
				(pin passive line
					(at 35.56 -83.82 180)
					(length 2.54)
					(name "CKB_P")
					(number "45")
				)
				(pin passive line
					(at 35.56 -86.36 180)
					(length 2.54)
					(name "CKB_N")
					(number "46")
				)
				(pin passive line
					(at 35.56 -68.58 180)
					(length 2.54)
					(name "DB1_P")
					(number "47")
				)
				(pin passive line
					(at 35.56 -71.12 180)
					(length 2.54)
					(name "DB1_N")
					(number "48")
				)
				(pin passive line
					(at 35.56 -73.66 180)
					(length 2.54)
					(name "DB2_P")
					(number "49")
				)
				(pin passive line
					(at 35.56 -76.2 180)
					(length 2.54)
					(name "DB2_N")
					(number "50")
				)
				(pin passive line
					(at 35.56 -58.42 180)
					(length 2.54)
					(name "CKF_P")
					(number "51")
				)
				(pin passive line
					(at 35.56 -60.96 180)
					(length 2.54)
					(name "CKF_N")
					(number "52")
				)
				(pin passive line
					(at 35.56 -78.74 180)
					(length 2.54)
					(name "DB3_P")
					(number "53")
				)
				(pin passive line
					(at 35.56 -81.28 180)
					(length 2.54)
					(name "DB3_N")
					(number "54")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "55")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "56")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 2.54)
					(name "GND")
					(number "57")
				)
			)
			(embedded_fonts no)
		)
)
