(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX98091"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX98091"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX98091"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max98091.pdf"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Ultra-Low Power Stereo Audio Codec"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX98091ETM+"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Maxim Integrated"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, CONTROLLER, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX98091_1_1"
				(pin passive line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "C1N")
					(number "1")
				)
				(pin power_in line
					(at 0 -43.18 0)
					(length 2.54)
					(name "HPGND")
					(number "2")
				)
				(pin power_out line
					(at 30.48 -30.48 180)
					(length 2.54)
					(name "CPVSS")
					(number "3")
				)
				(pin power_out line
					(at 30.48 -27.94 180)
					(length 2.54)
					(name "CPVDD")
					(number "4")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 2.54)
					(name "SPKRGND")
					(number "11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "SPKVDD")
					(number "14")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SPKVDD")
					(number "15")
				)
				(pin no_connect line
					(at 27.94 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "16")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 2.54)
					(name "SPKLGND")
					(number "19")
				)
				(pin no_connect line
					(at 27.94 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "22")
				)
				(pin no_connect line
					(at 27.94 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "24")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 2.54)
					(name "REF")
					(number "29")
				)
				(pin passive line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "BIAS")
					(number "30")
				)
				(pin power_in line
					(at 0 -45.72 0)
					(length 2.54)
					(name "AGND")
					(number "31")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "AVDD")
					(number "32")
				)
				(pin no_connect line
					(at 27.94 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "33")
				)
				(pin no_connect line
					(at 27.94 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "34")
				)
				(pin no_connect line
					(at 27.94 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "35")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 2.54)
					(name "DVDD")
					(number "36")
				)
				(pin power_in line
					(at 0 -48.26 0)
					(length 2.54)
					(name "DGND")
					(number "37")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "DVDDIO")
					(number "38")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "HPVDD")
					(number "47")
				)
				(pin passive line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "C1P")
					(number "48")
				)
				(pin passive line
					(at 30.48 -48.26 180)
					(length 2.54)
					(name "EP")
					(number "49")
				)
			)
			(symbol "MAX98091_2_1"
				(pin passive line
					(at 30.48 -38.1 180)
					(length 2.54)
					(name "HPL")
					(number "5")
				)
				(pin passive line
					(at 30.48 -43.18 180)
					(length 2.54)
					(name "HPSNS")
					(number "6")
				)
				(pin passive line
					(at 30.48 -40.64 180)
					(length 2.54)
					(name "HPR")
					(number "7")
				)
				(pin passive line
					(at 30.48 -53.34 180)
					(length 2.54)
					(name "JACKSNS")
					(number "8")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 2.54)
					(name "RCVP/LOUTL")
					(number "9")
				)
				(pin passive line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "RCVN/LOUTR")
					(number "10")
				)
				(pin passive line
					(at 30.48 -27.94 180)
					(length 2.54)
					(name "SPKRN")
					(number "12")
				)
				(pin passive line
					(at 30.48 -25.4 180)
					(length 2.54)
					(name "SPKRP")
					(number "13")
				)
				(pin passive line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "SPKLN")
					(number "17")
				)
				(pin passive line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "SPKLP")
					(number "18")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(name "IN2/DMC1")
					(number "20")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "IN1/DMD1")
					(number "21")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "IN3")
					(number "23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 2.54)
					(name "IN5/DMD2")
					(number "25")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "IN4")
					(number "26")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 2.54)
					(name "IN6/DMC2")
					(number "27")
				)
				(pin passive line
					(at 30.48 -63.5 180)
					(length 2.54)
					(name "MICBIAS")
					(number "28")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "SDOUT")
					(number "39")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "SDIN")
					(number "40")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "LRCLK")
					(number "41")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "BCLK")
					(number "42")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "~{IRQ}")
					(number "43")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "MCLK")
					(number "44")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SCL")
					(number "45")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SDA")
					(number "46")
				)
			)
			(embedded_fonts no)
		)
)
