(footprint "TQFN-16-1EP_3x3mm_P0.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Footprint based on: https://www.analog.com/media/en/package-pcb-resources/land-pattern/tqfn/90-0031.pdf")
	(property "Reference" "REF**"
		(at 0 -2.27 0)
		(layer "F.SilkS")
	)
	(property "Value" "TQFN-16-1EP_3x3mm_P0.5mm"
		(at 0 3.17 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 5.5 -0.08 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 5.5 -0.08 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -2.43 4.07 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2.43 5.27 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -2.43 6.47 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.425 -0.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "2" smd roundrect
		(at -1.425 -0.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "3" smd roundrect
		(at -1.425 0.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "4" smd roundrect
		(at -1.425 0.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "5" smd roundrect
		(at -0.75 1.425)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "6" smd roundrect
		(at -0.25 1.425)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "7" smd roundrect
		(at 0.25 1.425)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "8" smd roundrect
		(at 0.75 1.425)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "9" smd roundrect
		(at 1.425 0.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "10" smd roundrect
		(at 1.425 0.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "11" smd roundrect
		(at 1.425 -0.25)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "12" smd roundrect
		(at 1.425 -0.75)
		(size 0.8 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "13" smd roundrect
		(at 0.75 -1.425)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "14" smd roundrect
		(at 0.25 -1.425)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "15" smd roundrect
		(at -0.25 -1.425)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "16" smd roundrect
		(at -0.75 -1.425)
		(size 0.3 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "17" smd rect
		(at 0 0)
		(size 1.23 1.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.085)
	)
	(embedded_fonts no)
	(model "antmicro_max98357aete_t.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
