(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX98357A"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX98357A"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX98357A"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max98357a-max98357b.pdf"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "I2S Class D Amplifier, 2.5V to 5.5V, 3.2W into 4Ω at 5V, TQFN-16"
				(at 38.1 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Analog Devices"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX98357AETE+T"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, POWER, AMP, AUDIO, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX98357A_1_1"
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "DIN")
					(number "1")
				)
				(pin input line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "GAIN_SLOT")
					(number "2")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "3")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{SD_MODE}")
					(number "4")
				)
				(pin no_connect line
					(at 22.86 -13.97 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin no_connect line
					(at 22.86 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "6")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "7")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "8")
				)
				(pin output line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "OUT_P")
					(number "9")
				)
				(pin output line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "OUT_N")
					(number "10")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "GND")
					(number "11")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "12")
				)
				(pin no_connect line
					(at 22.86 -16.51 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "13")
				)
				(pin input clock
					(at 0 -10.16 0)
					(length 2.54)
					(name "LRCLK")
					(number "14")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "15")
				)
				(pin input clock
					(at 0 -7.62 0)
					(length 2.54)
					(name "BCLK")
					(number "16")
				)
				(pin free line
					(at 0 -17.78 0)
					(length 2.54)
					(name "EP")
					(number "17")
				)
			)
			(embedded_fonts no)
		)
)
