(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MB85RC1MTPNF-G"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MB85RC1MTPNF-G"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MB85RC1MTPNF-G"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.fujitsu.com/jp/group/fsm/en/documents/products/feram/lineup/MB85RC1MT-DS501-00027-5v0-E.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "FRAM (Ferroelectric RAM) Memory IC 1Mbit I²C 3.4 MHz 130 ns 8-SOP"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MB85RC1MTPNF-G-JNERE1"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Fujitsu"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, I2C, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MB85RC1MTPNF-G_1_1"
				(pin no_connect line
					(at 0 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "1")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "A1")
					(number "2")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "A2")
					(number "3")
				)
				(pin power_in line
					(at 10.16 -20.32 90)
					(length 2.54)
					(name "VSS")
					(number "4")
				)
				(pin bidirectional line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "SDA")
					(number "5")
				)
				(pin input line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "SCL")
					(number "6")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "WP")
					(number "7")
				)
				(pin power_in line
					(at 10.16 0 270)
					(length 2.54)
					(name "VDD")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
