(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MB85RS1MTPW-G_WLP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MB85RS1MTPW-G_WLP"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MB85RS1MTPW-G_WLP"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.fujitsu.com/uk/Images/MB85RS1MT.pdf"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "1Mbit FRAM (Ferroelectric RAM) Memory; SPI 30 MHz; WLP-8 2.3x3.1mm"
				(at 33.02 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MB85RS1MTPW-G-APEWE1"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Fujitsu"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, SPI, No-RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MB85RS1MTPW-G_WLP_1_1"
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "GND")
					(number "A1")
				)
				(pin input line
					(at 17.78 0 180)
					(length 2.54)
					(name "D_{IN}")
					(number "A3")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{WP}")
					(number "B2")
				)
				(pin output line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "D_{OUT}")
					(number "C1")
				)
				(pin input line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "SCK")
					(number "C3")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{HOLD}")
					(number "D2")
				)
				(pin input line
					(at 17.78 -7.62 180)
					(length 2.54)
					(name "~{CS}")
					(number "E1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "E3")
				)
			)
			(embedded_fonts no)
		)
)
