(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MCIMX7D5EVM10SC"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 98.552 -3.556 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MCIMX7D5EVM10SC"
				(at 98.552 -11.176 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MCIMX7D5EVM10SC"
				(at 98.552 -13.716 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/mcds/MCIMX7D5EVM10SC.pdf"
				(at 98.552 -16.256 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ARM® Cortex®-A7, ARM® Cortex®-M4 Microprocessor IC i.MX7D 2 Core, 32-Bit 1.0GHz 541-MAPBGA (19x19)"
				(at 98.552 -23.876 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MCIMX7D5EVM10SC"
				(at 98.552 -6.096 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "NXP"
				(at 98.552 -8.636 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 98.552 -18.796 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 98.552 -21.336 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "BGA, IC, ARM, MICROPROCESSOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MCIMX7D5EVM10SC_1_1"
				(pin power_in line
					(at 50.8 -68.58 180)
					(length 5.08)
					(name "VSS")
					(number "A1")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A3")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A6")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A9")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A13")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A17")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A21")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A25")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA1")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA2")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA6")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA8")
				)
				(pin power_out line
					(at 0 -30.48 0)
					(length 5.08)
					(name "VDDD_1P0_CAP")
					(number "AA9")
				)
				(pin power_in line
					(at 50.8 -39.37 180)
					(length 5.08)
					(name "PCIE_VP")
					(number "AA10")
				)
				(pin power_in line
					(at 50.8 -41.91 180)
					(length 5.08)
					(name "PCIE_VP_TX")
					(number "AA11")
				)
				(pin power_in line
					(at 50.8 -44.45 180)
					(length 5.08)
					(name "PCIE_VP_RX")
					(number "AA12")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA15")
				)
				(pin passive line
					(at 50.8 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "NVCC_DRAM")
					(number "AA16")
				)
				(pin passive line
					(at 50.8 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "NVCC_DRAM")
					(number "AA17")
				)
				(pin passive line
					(at 50.8 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "NVCC_DRAM")
					(number "AA18")
				)
				(pin passive line
					(at 50.8 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "NVCC_DRAM")
					(number "AA19")
				)
				(pin passive line
					(at 50.8 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "NVCC_DRAM")
					(number "AA20")
				)
				(pin passive line
					(at 50.8 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "NVCC_DRAM")
					(number "AA21")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA23")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 5.08)
					(name "VDDA_ADC2_1P8")
					(number "AB3")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB4")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB5")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB7")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB9")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB12")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 5.08)
					(name "VDDA_ADC1_1P8")
					(number "AC3")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 5.08)
					(name "VDD_TEMPSENSOR_1P8")
					(number "AC4")
				)
				(pin power_out line
					(at 0 -43.18 0)
					(length 5.08)
					(name "VDD_LPSR_1P0_CAP")
					(number "AC5")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC6")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC9")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC12")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC15")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC17")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC19")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC21")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC23")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD2")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD5")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD7")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 5.08)
					(name "VDD_SNVS_IN")
					(number "AD8")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD9")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD12")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE1")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE5")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE7")
				)
				(pin power_out line
					(at 0 -40.64 0)
					(length 5.08)
					(name "VDD_SNVS_1P8_CAP")
					(number "AE8")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE9")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE12")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE24")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE25")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B3")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B6")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B9")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B13")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B17")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B21")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C9")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C13")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VDD_SOC")
					(number "C14")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C15")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C16")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VDD_ARM")
					(number "C17")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C18")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_ARM")
					(number "C20")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D1")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D2")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D4")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D7")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "D14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_ARM")
					(number "D17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_ARM")
					(number "D20")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D22")
				)
				(pin power_in line
					(at 50.8 -7.62 180)
					(length 5.08)
					(name "NVCC_SD1")
					(number "E7")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "F3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "F4")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F7")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F8")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 5.08)
					(name "VDD_USB_OTG2_3P3_IN")
					(number "F9")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 5.08)
					(name "VDD_USB_OTG1_3P3_IN")
					(number "F10")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F11")
				)
				(pin power_in line
					(at 50.8 -5.08 180)
					(length 5.08)
					(name "NVCC_SAI")
					(number "F12")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F13")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "F18")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "F19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_ARM")
					(number "F22")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_ARM")
					(number "F23")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G4")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G7")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G9")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G11")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G13")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G15")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G17")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G19")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G22")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H1")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H2")
				)
				(pin power_in line
					(at 50.8 -10.16 180)
					(length 5.08)
					(name "NVCC_SD2")
					(number "H8")
				)
				(pin power_out line
					(at 0 -35.56 0)
					(length 5.08)
					(name "VDD_USB_OTG1_1P0_CAP")
					(number "H10")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 5.08)
					(name "VDD_USB_H_1P2")
					(number "H12")
				)
				(pin power_out line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PVCC_ENET_CAP")
					(number "H14")
				)
				(pin power_in line
					(at 50.8 -15.24 180)
					(length 5.08)
					(name "NVCC_ENET1")
					(number "H16")
				)
				(pin power_out line
					(at 50.8 -57.15 180)
					(length 5.08)
					(name "MIPI_VREG_0P4V")
					(number "H18")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "J3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "J4")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J7")
				)
				(pin power_out line
					(at 0 -58.42 0)
					(length 5.08)
					(name "PVCC_SAI_SD_CAP")
					(number "J9")
				)
				(pin power_out line
					(at 0 -38.1 0)
					(length 5.08)
					(name "VDD_USB_OTG2_1P0_CAP")
					(number "J11")
				)
				(pin power_in line
					(at 0 -54.61 0)
					(length 5.08)
					(name "VDDA_MIPI_1P8")
					(number "J13")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 5.08)
					(name "VDD_MIPI_1P0")
					(number "J15")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(hide yes)
					(name "VDD_MIPI_1P0")
					(number "J17")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_ARM")
					(number "J22")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_ARM")
					(number "J23")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K4")
				)
				(pin power_in line
					(at 50.8 -12.7 180)
					(length 5.08)
					(name "NVCC_SD3")
					(number "K8")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K10")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K12")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K14")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K16")
				)
				(pin power_in line
					(at 50.8 -17.78 180)
					(length 5.08)
					(name "NVCC_LCD")
					(number "K18")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K22")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L7")
				)
				(pin power_in line
					(at 50.8 -27.94 180)
					(length 5.08)
					(name "NVCC_SPI")
					(number "L9")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L11")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L13")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L15")
				)
				(pin power_in line
					(at 50.8 -22.86 180)
					(length 5.08)
					(name "NVCC_EPDC2")
					(number "L17")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L19")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "M3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "M4")
				)
				(pin power_in line
					(at 50.8 -25.4 180)
					(length 5.08)
					(name "NVCC_I2C")
					(number "M8")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M10")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M12")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M14")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M16")
				)
				(pin power_in line
					(at 50.8 -20.32 180)
					(length 5.08)
					(name "NVCC_EPDC1")
					(number "M18")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M24")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M25")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N4")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N7")
				)
				(pin power_in line
					(at 50.8 -30.48 180)
					(length 5.08)
					(name "NVCC_UART")
					(number "N9")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N11")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N13")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N15")
				)
				(pin power_out line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PVCC_EPDC_LCD_CAP")
					(number "N17")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N19")
				)
				(pin power_in line
					(at 50.8 -33.02 180)
					(length 5.08)
					(name "NVCC_GPIO1")
					(number "P8")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P10")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P12")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P14")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P16")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "P18")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "R3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "R4")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R7")
				)
				(pin power_out line
					(at 0 -66.04 0)
					(length 5.08)
					(name "PVCC_I2C_SPI_UART_CAP")
					(number "R9")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R11")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R13")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R15")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "R17")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R19")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R20")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R21")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R23")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T4")
				)
				(pin power_in line
					(at 50.8 -35.56 180)
					(length 5.08)
					(name "NVCC_GPIO2")
					(number "T8")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T10")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T12")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T14")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T16")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "T18")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T20")
				)
				(pin power_in line
					(at 50.8 -2.54 180)
					(length 5.08)
					(name "NVCC_DRAM")
					(number "T21")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U7")
				)
				(pin power_out line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VDD_1P2_CAP")
					(number "U9")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U13")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U15")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U17")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U19")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U20")
				)
				(pin passive line
					(at 50.8 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "NVCC_DRAM")
					(number "U21")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U23")
				)
				(pin power_out line
					(at 0 -49.53 0)
					(length 5.08)
					(name "VDDA_1P0_CAP")
					(number "V3")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 5.08)
					(name "VDD_XTAL_1P8")
					(number "V5")
				)
				(pin power_in line
					(at 0 -46.99 0)
					(length 5.08)
					(name "VDDA_1P8_IN")
					(number "V6")
				)
				(pin power_out line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PVCC_GPIO_CAP")
					(number "V10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "V12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "V14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "V16")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "V18")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V20")
				)
				(pin passive line
					(at 50.8 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "NVCC_DRAM")
					(number "V21")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W1")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W2")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W4")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 5.08)
					(hide yes)
					(name "VDDA_1P8_IN")
					(number "W5")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 5.08)
					(name "VDD_LPSR_IN")
					(number "W6")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W7")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W9")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W11")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W13")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W15")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W17")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W19")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W20")
				)
				(pin passive line
					(at 50.8 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "NVCC_DRAM")
					(number "W21")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W23")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y6")
				)
				(pin power_in line
					(at 0 -52.07 0)
					(length 5.08)
					(name "VDDA_PHY_1P8")
					(number "Y9")
				)
				(pin power_in line
					(at 50.8 -48.26 180)
					(length 5.08)
					(name "PCIE_VPH")
					(number "Y10")
				)
				(pin power_in line
					(at 50.8 -50.8 180)
					(length 5.08)
					(name "PCIE_VPH_TX")
					(number "Y11")
				)
				(pin power_in line
					(at 50.8 -53.34 180)
					(length 5.08)
					(name "PCIE_VPH_RX")
					(number "Y12")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y13")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y14")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y15")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y16")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y17")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y18")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y19")
				)
				(pin power_in line
					(at 50.8 0 180)
					(length 5.08)
					(name "NVCC_DRAM_CKE")
					(number "Y20")
				)
				(pin passive line
					(at 50.8 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "NVCC_DRAM")
					(number "Y21")
				)
			)
			(symbol "MCIMX7D5EVM10SC_2_1"
				(pin input line
					(at 46.99 -41.91 180)
					(length 5.08)
					(name "SNVS_TAMPER08")
					(number "AA3")
				)
				(pin input line
					(at 46.99 -36.83 180)
					(length 5.08)
					(name "SNVS_TAMPER06")
					(number "AA4")
				)
				(pin input line
					(at 46.99 -31.75 180)
					(length 5.08)
					(name "SNVS_TAMPER04")
					(number "AA5")
				)
				(pin input line
					(at 46.99 -21.59 180)
					(length 5.08)
					(name "SNVS_TAMPER00")
					(number "AA7")
				)
				(pin input line
					(at 46.99 -26.67 180)
					(length 5.08)
					(name "SNVS_TAMPER02")
					(number "AB6")
				)
				(pin output line
					(at 46.99 -19.05 180)
					(length 5.08)
					(name "SNVS_PMIC_ON_REQ")
					(number "AB8")
				)
				(pin output line
					(at 46.99 -16.51 180)
					(length 5.08)
					(name "PMIC_STBY_REQ")
					(number "AC7")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "ONOFF")
					(number "AC8")
				)
				(pin passive line
					(at 46.99 -50.8 180)
					(length 5.08)
					(name "TEMPSENSOR_RESERVE")
					(number "AD4")
				)
				(pin output line
					(at 0 -8.89 0)
					(length 5.08)
					(name "RTC_XTALO")
					(number "AD6")
				)
				(pin passive line
					(at 46.99 -48.26 180)
					(length 5.08)
					(name "TEMPSENSOR_REXT")
					(number "AE4")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 5.08)
					(name "RTC_XTALI")
					(number "AE6")
				)
				(pin input line
					(at 0 -29.21 0)
					(length 5.08)
					(name "BOOT_MODE0")
					(number "P4")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 5.08)
					(name "BOOT_MODE1")
					(number "P5")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "TEST_MODE")
					(number "P6")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "~{POR_B}")
					(number "R6")
				)
				(pin input line
					(at 46.99 -12.7 180)
					(length 5.08)
					(name "JTAG_MOD")
					(number "U1")
				)
				(pin input line
					(at 46.99 -10.16 180)
					(length 5.08)
					(name "JTAG_TRST_B")
					(number "U2")
				)
				(pin input line
					(at 46.99 -5.08 180)
					(length 5.08)
					(name "JTAG_TDI")
					(number "U3")
				)
				(pin input line
					(at 46.99 0 180)
					(length 5.08)
					(name "JTAG_TMS")
					(number "U4")
				)
				(pin input line
					(at 46.99 -7.62 180)
					(length 5.08)
					(name "JTAG_TCK")
					(number "U5")
				)
				(pin output line
					(at 46.99 -2.54 180)
					(length 5.08)
					(name "JTAG_TDO")
					(number "U6")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "XTALI")
					(number "V1")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 5.08)
					(name "XTALO")
					(number "V2")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 5.08)
					(name "GPANAIO")
					(number "V4")
				)
				(pin power_in line
					(at 0 -41.91 0)
					(length 5.08)
					(name "FUSE_FSOURCE")
					(number "V8")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "CCM_CLK2")
					(number "W3")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "CCM_CLK1_N")
					(number "Y1")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "CCM_CLK1_P")
					(number "Y2")
				)
				(pin input line
					(at 46.99 -44.45 180)
					(length 5.08)
					(name "SNVS_TAMPER09")
					(number "Y3")
				)
				(pin input line
					(at 46.99 -39.37 180)
					(length 5.08)
					(name "SNVS_TAMPER07")
					(number "Y4")
				)
				(pin input line
					(at 46.99 -34.29 180)
					(length 5.08)
					(name "SNVS_TAMPER05")
					(number "Y5")
				)
				(pin input line
					(at 46.99 -29.21 180)
					(length 5.08)
					(name "SNVS_TAMPER03")
					(number "Y7")
				)
				(pin input line
					(at 46.99 -24.13 180)
					(length 5.08)
					(name "SNVS_TAMPER01")
					(number "Y8")
				)
			)
			(symbol "MCIMX7D5EVM10SC_3_1"
				(pin output line
					(at 0 -82.55 0)
					(length 5.08)
					(name "DRAM_ODT1")
					(number "AA14")
				)
				(pin output line
					(at 0 -53.34 0)
					(length 5.08)
					(name "DRAM_CS1_B")
					(number "AA22")
				)
				(pin bidirectional line
					(at 46.99 -87.63 180)
					(length 5.08)
					(name "DRAM_DQM2")
					(number "AA24")
				)
				(pin bidirectional line
					(at 46.99 -40.64 180)
					(length 5.08)
					(name "DRAM_DATA16")
					(number "AA25")
				)
				(pin output line
					(at 0 -86.36 0)
					(length 5.08)
					(name "DRAM_ZQPAD")
					(number "AB13")
				)
				(pin output line
					(at 0 -63.5 0)
					(length 5.08)
					(name "DRAM_SDWE_B")
					(number "AB14")
				)
				(pin output line
					(at 0 -59.69 0)
					(length 5.08)
					(name "DRAM_RAS_B")
					(number "AB15")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 5.08)
					(name "DRAM_ADDR01")
					(number "AB16")
				)
				(pin output line
					(at 0 -67.31 0)
					(length 5.08)
					(name "DRAM_SDCKE0")
					(number "AB17")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 5.08)
					(name "DRAM_ADDR14")
					(number "AB18")
				)
				(pin output line
					(at 0 0 0)
					(length 5.08)
					(name "DRAM_ADDR00")
					(number "AB19")
				)
				(pin output line
					(at 0 -38.1 0)
					(length 5.08)
					(name "DRAM_ADDR15")
					(number "AB20")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 5.08)
					(name "DRAM_ADDR04")
					(number "AB21")
				)
				(pin output line
					(at 0 -69.85 0)
					(length 5.08)
					(name "DRAM_SDCKE1")
					(number "AB22")
				)
				(pin output line
					(at 0 -50.8 0)
					(length 5.08)
					(name "DRAM_CS0_B")
					(number "AB23")
				)
				(pin bidirectional line
					(at 46.99 -55.88 180)
					(length 5.08)
					(name "DRAM_DATA22")
					(number "AB24")
				)
				(pin bidirectional line
					(at 46.99 -53.34 180)
					(length 5.08)
					(name "DRAM_DATA21")
					(number "AB25")
				)
				(pin power_in line
					(at 0 -93.98 0)
					(length 5.08)
					(name "DRAM_VREF")
					(number "AC13")
				)
				(pin output line
					(at 0 -57.15 0)
					(length 5.08)
					(name "DRAM_CAS_B")
					(number "AC14")
				)
				(pin output line
					(at 0 -80.01 0)
					(length 5.08)
					(name "DRAM_ODT0")
					(number "AC16")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 5.08)
					(name "DRAM_ADDR02")
					(number "AC18")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 5.08)
					(name "DRAM_ADDR03")
					(number "AC20")
				)
				(pin input line
					(at 0 -90.17 0)
					(length 5.08)
					(name "DRAM_RESET")
					(number "AC22")
				)
				(pin bidirectional line
					(at 46.99 -58.42 180)
					(length 5.08)
					(name "DRAM_DATA23")
					(number "AC24")
				)
				(pin bidirectional line
					(at 46.99 -50.8 180)
					(length 5.08)
					(name "DRAM_DATA20")
					(number "AC25")
				)
				(pin bidirectional line
					(at 46.99 -35.56 180)
					(length 5.08)
					(name "DRAM_DATA14")
					(number "AD13")
				)
				(pin bidirectional line
					(at 46.99 -33.02 180)
					(length 5.08)
					(name "DRAM_DATA13")
					(number "AD14")
				)
				(pin bidirectional line
					(at 46.99 -100.33 180)
					(length 5.08)
					(name "DRAM_SDQS1_P")
					(number "AD15")
				)
				(pin bidirectional line
					(at 46.99 -27.94 180)
					(length 5.08)
					(name "DRAM_DATA11")
					(number "AD16")
				)
				(pin bidirectional line
					(at 46.99 -85.09 180)
					(length 5.08)
					(name "DRAM_DQM1")
					(number "AD17")
				)
				(pin bidirectional line
					(at 46.99 -15.24 180)
					(length 5.08)
					(name "DRAM_DATA06")
					(number "AD18")
				)
				(pin bidirectional line
					(at 46.99 -12.7 180)
					(length 5.08)
					(name "DRAM_DATA05")
					(number "AD19")
				)
				(pin bidirectional line
					(at 46.99 -82.55 180)
					(length 5.08)
					(name "DRAM_DQM0")
					(number "AD20")
				)
				(pin bidirectional line
					(at 46.99 -96.52 180)
					(length 5.08)
					(name "DRAM_SDQS0_N")
					(number "AD21")
				)
				(pin bidirectional line
					(at 46.99 0 180)
					(length 5.08)
					(name "DRAM_DATA00")
					(number "AD22")
				)
				(pin bidirectional line
					(at 46.99 -2.54 180)
					(length 5.08)
					(name "DRAM_DATA01")
					(number "AD23")
				)
				(pin output line
					(at 0 -73.66 0)
					(length 5.08)
					(name "DRAM_SDCLK0_P")
					(number "AD24")
				)
				(pin output line
					(at 0 -76.2 0)
					(length 5.08)
					(name "DRAM_SDCLK0_N")
					(number "AD25")
				)
				(pin bidirectional line
					(at 46.99 -38.1 180)
					(length 5.08)
					(name "DRAM_DATA15")
					(number "AE13")
				)
				(pin bidirectional line
					(at 46.99 -20.32 180)
					(length 5.08)
					(name "DRAM_DATA08")
					(number "AE14")
				)
				(pin bidirectional line
					(at 46.99 -102.87 180)
					(length 5.08)
					(name "DRAM_SDQS1_N")
					(number "AE15")
				)
				(pin bidirectional line
					(at 46.99 -30.48 180)
					(length 5.08)
					(name "DRAM_DATA12")
					(number "AE16")
				)
				(pin bidirectional line
					(at 46.99 -25.4 180)
					(length 5.08)
					(name "DRAM_DATA10")
					(number "AE17")
				)
				(pin bidirectional line
					(at 46.99 -22.86 180)
					(length 5.08)
					(name "DRAM_DATA09")
					(number "AE18")
				)
				(pin bidirectional line
					(at 46.99 -17.78 180)
					(length 5.08)
					(name "DRAM_DATA07")
					(number "AE19")
				)
				(pin bidirectional line
					(at 46.99 -5.08 180)
					(length 5.08)
					(name "DRAM_DATA02")
					(number "AE20")
				)
				(pin bidirectional line
					(at 46.99 -93.98 180)
					(length 5.08)
					(name "DRAM_SDQS0_P")
					(number "AE21")
				)
				(pin bidirectional line
					(at 46.99 -10.16 180)
					(length 5.08)
					(name "DRAM_DATA04")
					(number "AE22")
				)
				(pin bidirectional line
					(at 46.99 -7.62 180)
					(length 5.08)
					(name "DRAM_DATA03")
					(number "AE23")
				)
				(pin output line
					(at 0 -46.99 0)
					(length 5.08)
					(name "DRAM_SDBA2")
					(number "N23")
				)
				(pin bidirectional line
					(at 46.99 -63.5 180)
					(length 5.08)
					(name "DRAM_DATA25")
					(number "N24")
				)
				(pin bidirectional line
					(at 46.99 -68.58 180)
					(length 5.08)
					(name "DRAM_DATA27")
					(number "N25")
				)
				(pin output line
					(at 0 -44.45 0)
					(length 5.08)
					(name "DRAM_SDBA1")
					(number "P22")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 5.08)
					(name "DRAM_ADDR13")
					(number "P23")
				)
				(pin bidirectional line
					(at 46.99 -90.17 180)
					(length 5.08)
					(name "DRAM_DQM3")
					(number "P24")
				)
				(pin bidirectional line
					(at 46.99 -66.04 180)
					(length 5.08)
					(name "DRAM_DATA26")
					(number "P25")
				)
				(pin output line
					(at 0 -41.91 0)
					(length 5.08)
					(name "DRAM_SDBA0")
					(number "R22")
				)
				(pin bidirectional line
					(at 46.99 -73.66 180)
					(length 5.08)
					(name "DRAM_DATA29")
					(number "R24")
				)
				(pin bidirectional line
					(at 46.99 -60.96 180)
					(length 5.08)
					(name "DRAM_DATA24")
					(number "R25")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 5.08)
					(name "DRAM_ADDR12")
					(number "T22")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 5.08)
					(name "DRAM_ADDR10")
					(number "T23")
				)
				(pin bidirectional line
					(at 46.99 -113.03 180)
					(length 5.08)
					(name "DRAM_SDQS3_P")
					(number "T24")
				)
				(pin bidirectional line
					(at 46.99 -115.57 180)
					(length 5.08)
					(name "DRAM_SDQS3_N")
					(number "T25")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 5.08)
					(name "DRAM_ADDR11")
					(number "U22")
				)
				(pin bidirectional line
					(at 46.99 -76.2 180)
					(length 5.08)
					(name "DRAM_DATA30")
					(number "U24")
				)
				(pin bidirectional line
					(at 46.99 -71.12 180)
					(length 5.08)
					(name "DRAM_DATA28")
					(number "U25")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 5.08)
					(name "DRAM_ADDR06")
					(number "V22")
				)
				(pin output line
					(at 0 -22.86 0)
					(length 5.08)
					(name "DRAM_ADDR09")
					(number "V23")
				)
				(pin bidirectional line
					(at 46.99 -78.74 180)
					(length 5.08)
					(name "DRAM_DATA31")
					(number "V24")
				)
				(pin bidirectional line
					(at 46.99 -45.72 180)
					(length 5.08)
					(name "DRAM_DATA18")
					(number "V25")
				)
				(pin output line
					(at 0 -20.32 0)
					(length 5.08)
					(name "DRAM_ADDR08")
					(number "W22")
				)
				(pin bidirectional line
					(at 46.99 -43.18 180)
					(length 5.08)
					(name "DRAM_DATA17")
					(number "W24")
				)
				(pin bidirectional line
					(at 46.99 -48.26 180)
					(length 5.08)
					(name "DRAM_DATA19")
					(number "W25")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 5.08)
					(name "DRAM_ADDR07")
					(number "Y22")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 5.08)
					(name "DRAM_ADDR05")
					(number "Y23")
				)
				(pin bidirectional line
					(at 46.99 -106.68 180)
					(length 5.08)
					(name "DRAM_SDQS2_P")
					(number "Y24")
				)
				(pin bidirectional line
					(at 46.99 -109.22 180)
					(length 5.08)
					(name "DRAM_SDQS2_N")
					(number "Y25")
				)
			)
			(symbol "MCIMX7D5EVM10SC_4_1"
				(pin bidirectional line
					(at 39.37 -27.94 180)
					(length 5.08)
					(name "ECSPI1_MOSI")
					(number "G5")
				)
				(pin bidirectional line
					(at 39.37 -39.37 180)
					(length 5.08)
					(name "ECSPI2_MOSI")
					(number "G6")
				)
				(pin bidirectional line
					(at 39.37 -30.48 180)
					(length 5.08)
					(name "ECSPI1_SCLK")
					(number "H3")
				)
				(pin bidirectional line
					(at 39.37 -25.4 180)
					(length 5.08)
					(name "ECSPI1_MISO")
					(number "H4")
				)
				(pin bidirectional line
					(at 39.37 -33.02 180)
					(length 5.08)
					(name "ECSPI1_SS0")
					(number "H5")
				)
				(pin bidirectional line
					(at 39.37 -36.83 180)
					(length 5.08)
					(name "ECSPI2_MISO")
					(number "H6")
				)
				(pin bidirectional line
					(at 39.37 0 180)
					(length 5.08)
					(name "I2C1_SCL")
					(number "J2")
				)
				(pin bidirectional line
					(at 39.37 -41.91 180)
					(length 5.08)
					(name "ECSPI2_SCLK")
					(number "J5")
				)
				(pin bidirectional line
					(at 39.37 -44.45 180)
					(length 5.08)
					(name "ECSPI2_SS0")
					(number "J6")
				)
				(pin bidirectional line
					(at 39.37 -2.54 180)
					(length 5.08)
					(name "I2C1_SDA")
					(number "K1")
				)
				(pin bidirectional line
					(at 39.37 -6.35 180)
					(length 5.08)
					(name "I2C2_SCL")
					(number "K2")
				)
				(pin bidirectional line
					(at 39.37 -8.89 180)
					(length 5.08)
					(name "I2C2_SDA")
					(number "K3")
				)
				(pin bidirectional line
					(at 39.37 -12.7 180)
					(length 5.08)
					(name "I2C3_SCL")
					(number "K5")
				)
				(pin bidirectional line
					(at 39.37 -15.24 180)
					(length 5.08)
					(name "I2C3_SDA")
					(number "K6")
				)
				(pin bidirectional line
					(at 39.37 -19.05 180)
					(length 5.08)
					(name "I2C4_SCL")
					(number "L1")
				)
				(pin bidirectional line
					(at 39.37 -21.59 180)
					(length 5.08)
					(name "I2C4_SDA")
					(number "L2")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "UART1_RXD")
					(number "L3")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "UART1_TXD")
					(number "L4")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "UART2_RXD")
					(number "L5")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "UART2_TXD")
					(number "L6")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "UART3_RXD")
					(number "M1")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "UART3_TXD")
					(number "M2")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "UART3_RTS")
					(number "M5")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "UART3_CTS")
					(number "M6")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GPIO1_IO00")
					(number "N1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GPIO1_IO01")
					(number "N2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GPIO1_IO02")
					(number "N3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GPIO1_IO03")
					(number "N5")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GPIO1_IO04")
					(number "N6")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GPIO1_IO05")
					(number "P1")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GPIO1_IO06")
					(number "P2")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GPIO1_IO07")
					(number "P3")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GPIO1_IO08")
					(number "R1")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GPIO1_IO09")
					(number "R2")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GPIO1_IO10")
					(number "R5")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GPIO1_IO11")
					(number "T1")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GPIO1_IO12")
					(number "T2")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GPIO1_IO13")
					(number "T3")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GPIO1_IO14")
					(number "T5")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GPIO1_IO15")
					(number "T6")
				)
			)
			(symbol "MCIMX7D5EVM10SC_5_1"
				(pin bidirectional line
					(at 39.37 -2.54 180)
					(length 5.08)
					(name "LCD1_DATA01")
					(number "A22")
				)
				(pin bidirectional line
					(at 39.37 -7.62 180)
					(length 5.08)
					(name "LCD1_DATA03")
					(number "A23")
				)
				(pin bidirectional line
					(at 39.37 -15.24 180)
					(length 5.08)
					(name "LCD1_DATA06")
					(number "A24")
				)
				(pin bidirectional line
					(at 39.37 -5.08 180)
					(length 5.08)
					(name "LCD1_DATA02")
					(number "B22")
				)
				(pin bidirectional line
					(at 39.37 -12.7 180)
					(length 5.08)
					(name "LCD1_DATA05")
					(number "B23")
				)
				(pin bidirectional line
					(at 39.37 -25.4 180)
					(length 5.08)
					(name "LCD1_DATA10")
					(number "B24")
				)
				(pin bidirectional line
					(at 39.37 -40.64 180)
					(length 5.08)
					(name "LCD1_DATA16")
					(number "B25")
				)
				(pin bidirectional line
					(at 39.37 -76.2 180)
					(length 5.08)
					(name "LCD1_RESET")
					(number "C21")
				)
				(pin bidirectional line
					(at 39.37 -10.16 180)
					(length 5.08)
					(name "LCD1_DATA04")
					(number "C22")
				)
				(pin bidirectional line
					(at 39.37 -22.86 180)
					(length 5.08)
					(name "LCD1_DATA09")
					(number "C23")
				)
				(pin bidirectional line
					(at 39.37 -38.1 180)
					(length 5.08)
					(name "LCD1_DATA15")
					(number "C24")
				)
				(pin bidirectional line
					(at 39.37 -50.8 180)
					(length 5.08)
					(name "LCD1_DATA20")
					(number "C25")
				)
				(pin bidirectional line
					(at 39.37 0 180)
					(length 5.08)
					(name "LCD1_DATA00")
					(number "D21")
				)
				(pin bidirectional line
					(at 39.37 -35.56 180)
					(length 5.08)
					(name "LCD1_DATA14")
					(number "D23")
				)
				(pin bidirectional line
					(at 39.37 -48.26 180)
					(length 5.08)
					(name "LCD1_DATA19")
					(number "D24")
				)
				(pin bidirectional line
					(at 39.37 -55.88 180)
					(length 5.08)
					(name "LCD1_DATA22")
					(number "D25")
				)
				(pin bidirectional line
					(at 39.37 -62.23 180)
					(length 5.08)
					(name "LCD1_CLK")
					(number "E20")
				)
				(pin bidirectional line
					(at 39.37 -20.32 180)
					(length 5.08)
					(name "LCD1_DATA08")
					(number "E21")
				)
				(pin bidirectional line
					(at 39.37 -33.02 180)
					(length 5.08)
					(name "LCD1_DATA13")
					(number "E22")
				)
				(pin bidirectional line
					(at 39.37 -45.72 180)
					(length 5.08)
					(name "LCD1_DATA18")
					(number "E23")
				)
				(pin bidirectional line
					(at 39.37 -53.34 180)
					(length 5.08)
					(name "LCD1_DATA21")
					(number "E24")
				)
				(pin bidirectional line
					(at 39.37 -69.85 180)
					(length 5.08)
					(name "LCD1_HSYNC")
					(number "E25")
				)
				(pin bidirectional line
					(at 39.37 -17.78 180)
					(length 5.08)
					(name "LCD1_DATA07")
					(number "F20")
				)
				(pin bidirectional line
					(at 39.37 -30.48 180)
					(length 5.08)
					(name "LCD1_DATA12")
					(number "F21")
				)
				(pin bidirectional line
					(at 39.37 -72.39 180)
					(length 5.08)
					(name "LCD1_VSYNC")
					(number "F24")
				)
				(pin bidirectional line
					(at 39.37 -66.04 180)
					(length 5.08)
					(name "LCD1_ENABLE")
					(number "F25")
				)
				(pin bidirectional line
					(at 39.37 -27.94 180)
					(length 5.08)
					(name "LCD1_DATA11")
					(number "G20")
				)
				(pin bidirectional line
					(at 39.37 -43.18 180)
					(length 5.08)
					(name "LCD1_DATA17")
					(number "G21")
				)
				(pin bidirectional line
					(at 39.37 -58.42 180)
					(length 5.08)
					(name "LCD1_DATA23")
					(number "G23")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "EPDC1_SDCE1")
					(number "G24")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "EPDC1_SDCE0")
					(number "G25")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "EPDC1_SDSHR")
					(number "H20")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "EPDC1_SDOE")
					(number "H21")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "EPDC1_SDCE3")
					(number "H22")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "EPDC1_SDCE2")
					(number "H23")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "EPDC1_PWRCOM")
					(number "H24")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 5.08)
					(name "EPDC1_GDSP")
					(number "H25")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "EPDC1_SDLE")
					(number "J20")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "EPDC1_SDCLK")
					(number "J21")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "EPDC1_GDOE")
					(number "J24")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "EPDC1_GDCLK")
					(number "J25")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "EPDC1_PWRSTAT")
					(number "K20")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 5.08)
					(name "EPDC1_GDRL")
					(number "K21")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "EPDC1_BDR1")
					(number "K23")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "EPDC1_BDR0")
					(number "K24")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "EPDC1_DATA15")
					(number "K25")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "EPDC1_DATA14")
					(number "L20")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "EPDC1_DATA13")
					(number "L21")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "EPDC1_DATA12")
					(number "L22")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "EPDC1_DATA11")
					(number "L23")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "EPDC1_DATA10")
					(number "L24")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "EPDC1_DATA09")
					(number "L25")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "EPDC1_DATA05")
					(number "M20")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "EPDC1_DATA06")
					(number "M21")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "EPDC1_DATA07")
					(number "M22")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "EPDC1_DATA08")
					(number "M23")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "EPDC1_DATA02")
					(number "N20")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "EPDC1_DATA03")
					(number "N21")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "EPDC1_DATA04")
					(number "N22")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "EPDC1_DATA00")
					(number "P20")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "EPDC1_DATA01")
					(number "P21")
				)
			)
			(symbol "MCIMX7D5EVM10SC_6_1"
				(pin bidirectional line
					(at 39.37 -2.54 180)
					(length 5.08)
					(name "SD3_DATA1")
					(number "A2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "SD1_DATA2")
					(number "A4")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "SD1_DATA0")
					(number "A5")
				)
				(pin bidirectional line
					(at 39.37 -17.78 180)
					(length 5.08)
					(name "SD3_DATA7")
					(number "B1")
				)
				(pin bidirectional line
					(at 39.37 0 180)
					(length 5.08)
					(name "SD3_DATA0")
					(number "B2")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "SD1_RESET_B")
					(number "B4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "SD1_CLK")
					(number "B5")
				)
				(pin bidirectional line
					(at 39.37 -20.32 180)
					(length 5.08)
					(name "SD3_CLK")
					(number "C1")
				)
				(pin bidirectional line
					(at 39.37 -15.24 180)
					(length 5.08)
					(name "SD3_DATA6")
					(number "C2")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "SD2_WP")
					(number "C3")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "SD1_WP")
					(number "C4")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "SD1_CMD")
					(number "C5")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "SD1_CD_B")
					(number "C6")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "SD2_CD_B")
					(number "D3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "SD1_DATA3")
					(number "D5")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "SD1_DATA1")
					(number "D6")
				)
				(pin bidirectional line
					(at 39.37 -22.86 180)
					(length 5.08)
					(name "SD3_CMD")
					(number "E1")
				)
				(pin bidirectional line
					(at 39.37 -12.7 180)
					(length 5.08)
					(name "SD3_DATA5")
					(number "E2")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "SD2_CLK")
					(number "E3")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "SD2_DATA0")
					(number "E4")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "SD2_DATA1")
					(number "E5")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "SD2_DATA3")
					(number "E6")
				)
				(pin bidirectional line
					(at 39.37 -7.62 180)
					(length 5.08)
					(name "SD3_DATA3")
					(number "F1")
				)
				(pin bidirectional line
					(at 39.37 -10.16 180)
					(length 5.08)
					(name "SD3_DATA4")
					(number "F2")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "SD2_DATA2")
					(number "F5")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "SD2_CMD")
					(number "F6")
				)
				(pin bidirectional line
					(at 39.37 -27.94 180)
					(length 5.08)
					(name "SD3_RESET_B")
					(number "G1")
				)
				(pin bidirectional line
					(at 39.37 -5.08 180)
					(length 5.08)
					(name "SD3_DATA2")
					(number "G2")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "SD2_RESET_B")
					(number "G3")
				)
				(pin bidirectional line
					(at 39.37 -25.4 180)
					(length 5.08)
					(name "SD3_STROBE")
					(number "J1")
				)
			)
			(symbol "MCIMX7D5EVM10SC_7_1"
				(pin bidirectional line
					(at 39.37 -2.54 180)
					(length 5.08)
					(name "SAI1_TXC")
					(number "C11")
				)
				(pin bidirectional line
					(at 39.37 -12.7 180)
					(length 5.08)
					(name "SAI1_RXFS")
					(number "C12")
				)
				(pin bidirectional line
					(at 39.37 -21.59 180)
					(length 5.08)
					(name "SAI2_TXC")
					(number "D8")
				)
				(pin bidirectional line
					(at 39.37 -24.13 180)
					(length 5.08)
					(name "SAI2_TXFS")
					(number "D9")
				)
				(pin bidirectional line
					(at 39.37 -5.08 180)
					(length 5.08)
					(name "SAI1_TXFS")
					(number "D11")
				)
				(pin bidirectional line
					(at 39.37 -10.16 180)
					(length 5.08)
					(name "SAI1_RXC")
					(number "D12")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "ENET1_RDATA2")
					(number "D13")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "ENET1_RX_CLK")
					(number "D15")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "ENET1_TX_CLK")
					(number "D16")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "ENET1_TDATA3")
					(number "D18")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "ENET1_COL")
					(number "D19")
				)
				(pin bidirectional line
					(at 39.37 -19.05 180)
					(length 5.08)
					(name "SAI2_TXD")
					(number "E8")
				)
				(pin bidirectional line
					(at 39.37 -26.67 180)
					(length 5.08)
					(name "SAI2_RXD")
					(number "E9")
				)
				(pin bidirectional line
					(at 39.37 -15.24 180)
					(length 5.08)
					(name "SAI1_MCLK")
					(number "E10")
				)
				(pin bidirectional line
					(at 39.37 0 180)
					(length 5.08)
					(name "SAI1_TXD")
					(number "E11")
				)
				(pin bidirectional line
					(at 39.37 -7.62 180)
					(length 5.08)
					(name "SAI1_RXD")
					(number "E12")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "ENET1_RDATA3")
					(number "E13")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "ENET1_RDATA0")
					(number "E14")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "ENET1_RX_CTL")
					(number "E15")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "ENET1_TX_CTL")
					(number "E16")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "ENET1_TDATA1")
					(number "E17")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "ENET1_TDATA2")
					(number "E18")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "ENET1_CRS")
					(number "E19")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "ENET1_RDATA1")
					(number "F14")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "ENET1_RXC")
					(number "F15")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "ENET1_TXC")
					(number "F16")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "ENET1_TDATA0")
					(number "F17")
				)
			)
			(symbol "MCIMX7D5EVM10SC_8_1"
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "USB_OTG1_REXT")
					(number "A7")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 5.08)
					(name "USB_OTG1_DN")
					(number "A8")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "USB_OTG2_DN")
					(number "A10")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 5.08)
					(name "USB_OTG2_REXT")
					(number "A11")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "USB_H_DATA")
					(number "A12")
				)
				(pin input line
					(at 44.45 -6.35 180)
					(length 5.08)
					(name "MIPI_CSI_D1_N")
					(number "A14")
				)
				(pin input line
					(at 44.45 -15.24 180)
					(length 5.08)
					(name "MIPI_CSI_CLK_N")
					(number "A15")
				)
				(pin input line
					(at 44.45 -2.54 180)
					(length 5.08)
					(name "MIPI_CSI_D0_N")
					(number "A16")
				)
				(pin output line
					(at 44.45 -27.94 180)
					(length 5.08)
					(name "MIPI_DSI_D1_N")
					(number "A18")
				)
				(pin output line
					(at 44.45 -34.29 180)
					(length 5.08)
					(name "MIPI_DSI_CLK_N")
					(number "A19")
				)
				(pin output line
					(at 44.45 -21.59 180)
					(length 5.08)
					(name "MIPI_DSI_D0_N")
					(number "A20")
				)
				(pin passive line
					(at 44.45 -63.5 180)
					(length 5.08)
					(name "PCIE_REXT")
					(number "AA13")
				)
				(pin passive line
					(at 0 -57.15 0)
					(length 5.08)
					(name "ADC2_IN2")
					(number "AB1")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 5.08)
					(name "ADC2_IN3")
					(number "AB2")
				)
				(pin output line
					(at 44.45 -57.15 180)
					(length 5.08)
					(name "PCIE_REFCLKOUT_P")
					(number "AB10")
				)
				(pin output line
					(at 44.45 -38.1 180)
					(length 5.08)
					(name "PCIE_TX_P")
					(number "AB11")
				)
				(pin passive line
					(at 0 -52.07 0)
					(length 5.08)
					(name "ADC2_IN0")
					(number "AC1")
				)
				(pin passive line
					(at 0 -54.61 0)
					(length 5.08)
					(name "ADC2_IN1")
					(number "AC2")
				)
				(pin output line
					(at 44.45 -59.69 180)
					(length 5.08)
					(name "PCIE_REFCLKOUT_N")
					(number "AC10")
				)
				(pin output line
					(at 44.45 -40.64 180)
					(length 5.08)
					(name "PCIE_TX_N")
					(number "AC11")
				)
				(pin passive line
					(at 0 -41.91 0)
					(length 5.08)
					(name "ADC1_IN0")
					(number "AD1")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 5.08)
					(name "ADC1_IN1")
					(number "AD3")
				)
				(pin input line
					(at 44.45 -50.8 180)
					(length 5.08)
					(name "PCIE_REFCLKIN_P")
					(number "AD10")
				)
				(pin input line
					(at 44.45 -44.45 180)
					(length 5.08)
					(name "PCIE_RX_P")
					(number "AD11")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 5.08)
					(name "ADC1_IN2")
					(number "AE2")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 5.08)
					(name "ADC1_IN3")
					(number "AE3")
				)
				(pin input line
					(at 44.45 -53.34 180)
					(length 5.08)
					(name "PCIE_REFCLKIN_N")
					(number "AE10")
				)
				(pin input line
					(at 44.45 -46.99 180)
					(length 5.08)
					(name "PCIE_RX_N")
					(number "AE11")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "USB_OTG1_ID")
					(number "B7")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 5.08)
					(name "USB_OTG1_DP")
					(number "B8")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "USB_OTG2_DP")
					(number "B10")
				)
				(pin input line
					(at 0 -29.21 0)
					(length 5.08)
					(name "USB_OTG2_ID")
					(number "B11")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "USB_H_STROBE")
					(number "B12")
				)
				(pin input line
					(at 44.45 -8.89 180)
					(length 5.08)
					(name "MIPI_CSI_D1_P")
					(number "B14")
				)
				(pin input line
					(at 44.45 -12.7 180)
					(length 5.08)
					(name "MIPI_CSI_CLK_P")
					(number "B15")
				)
				(pin input line
					(at 44.45 0 180)
					(length 5.08)
					(name "MIPI_CSI_D0_P")
					(number "B16")
				)
				(pin output line
					(at 44.45 -25.4 180)
					(length 5.08)
					(name "MIPI_DSI_D1_P")
					(number "B18")
				)
				(pin output line
					(at 44.45 -31.75 180)
					(length 5.08)
					(name "MIPI_DSI_CLK_P")
					(number "B19")
				)
				(pin output line
					(at 44.45 -19.05 180)
					(length 5.08)
					(name "MIPI_DSI_D0_P")
					(number "B20")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "USB_OTG1_CHD_B")
					(number "C7")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "USB_OTG1_VBUS")
					(number "C8")
				)
				(pin power_in line
					(at 0 -19.05 0)
					(length 5.08)
					(name "USB_OTG2_VBUS")
					(number "C10")
				)
			)
			(embedded_fonts no)
		)
)
