(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MCP23016-I_SO"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MCP23016-I_SO"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MCP23016-I_SO"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/20090C.pdf"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "I/O Expander, 16 bit, I2C, 2-5.5 V, SOIC, 28 Pins"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MCP23016-I_SO"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "SOIC28-W_MC_MCH SOIC28-W_MC_MCH-M SOIC28-W_MC_MCH-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MCP23016-I_SO_1_1"
				(pin power_in line
					(at 0 -40.64 0)
					(length 2.54)
					(name "VSS")
					(number "1")
				)
				(pin bidirectional line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "GP1-0")
					(number "2")
				)
				(pin bidirectional line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "GP1-1")
					(number "3")
				)
				(pin bidirectional line
					(at 25.4 -27.94 180)
					(length 2.54)
					(name "GP1-2")
					(number "4")
				)
				(pin bidirectional line
					(at 25.4 -30.48 180)
					(length 2.54)
					(name "GP1-3")
					(number "5")
				)
				(pin open_collector line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{INT}")
					(number "6")
				)
				(pin bidirectional line
					(at 25.4 -33.02 180)
					(length 2.54)
					(name "GP1-4")
					(number "7")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "8")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "CLK")
					(number "9")
				)
				(pin no_connect line
					(at 0 -17.78 0)
					(length 2.54)
					(name "TP")
					(number "10")
				)
				(pin bidirectional line
					(at 25.4 -35.56 180)
					(length 2.54)
					(name "GP1-5")
					(number "11")
				)
				(pin bidirectional line
					(at 25.4 -38.1 180)
					(length 2.54)
					(name "GP1-6")
					(number "12")
				)
				(pin bidirectional line
					(at 25.4 -40.64 180)
					(length 2.54)
					(name "GP1-7")
					(number "13")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SCL")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SDA")
					(number "15")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "A0")
					(number "16")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "A1")
					(number "17")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "A2")
					(number "18")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "19")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "20")
				)
				(pin bidirectional line
					(at 25.4 0 180)
					(length 2.54)
					(name "GP0-0")
					(number "21")
				)
				(pin bidirectional line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "GP0-1")
					(number "22")
				)
				(pin bidirectional line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "GP0-2")
					(number "23")
				)
				(pin bidirectional line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "GP0-3")
					(number "24")
				)
				(pin bidirectional line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "GP0-4")
					(number "25")
				)
				(pin bidirectional line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "GP0-5")
					(number "26")
				)
				(pin bidirectional line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "GP0-6")
					(number "27")
				)
				(pin bidirectional line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "GP0-7")
					(number "28")
				)
			)
			(embedded_fonts no)
		)
)
