(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MCP23017T-E_QFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MCP23017T-E_QFN"
				(at 38.1 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MCP23017T-E_QFN"
				(at 38.1 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MCP23017-Data-Sheet-DS20001952.pdf"
				(at 38.1 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "I/O Expander, 16 bit, I2C, 1.8-5.5 V, QFN, 28 Pins"
				(at 38.1 -26.67 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 38.1 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MCP23017T-E/ML"
				(at 38.1 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 38.1 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MCP23017T-E_QFN_1_1"
				(pin bidirectional line
					(at 25.4 -33.02 180)
					(length 2.54)
					(name "GPB4")
					(number "1")
				)
				(pin bidirectional line
					(at 25.4 -35.56 180)
					(length 2.54)
					(name "GPB5")
					(number "2")
				)
				(pin bidirectional line
					(at 25.4 -38.1 180)
					(length 2.54)
					(name "GPB6")
					(number "3")
				)
				(pin output line
					(at 25.4 -40.64 180)
					(length 2.54)
					(name "GPB7")
					(number "4")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "5")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 2.54)
					(name "VSS")
					(number "6")
				)
				(pin no_connect line
					(at 2.54 -21.59 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SCK")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SDA")
					(number "9")
				)
				(pin no_connect line
					(at 2.54 -24.13 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "10")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "A0")
					(number "11")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "A1")
					(number "12")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "A2")
					(number "13")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{RESET}")
					(number "14")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 2.54)
					(name "INTB")
					(number "15")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 2.54)
					(name "INTA")
					(number "16")
				)
				(pin bidirectional line
					(at 25.4 0 180)
					(length 2.54)
					(name "GPA0")
					(number "17")
				)
				(pin bidirectional line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "GPA1")
					(number "18")
				)
				(pin bidirectional line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "GPA2")
					(number "19")
				)
				(pin bidirectional line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "GPA3")
					(number "20")
				)
				(pin bidirectional line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "GPA4")
					(number "21")
				)
				(pin bidirectional line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "GPA5")
					(number "22")
				)
				(pin bidirectional line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "GPA6")
					(number "23")
				)
				(pin output line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "GPA7")
					(number "24")
				)
				(pin bidirectional line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "GPB0")
					(number "25")
				)
				(pin bidirectional line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "GPB1")
					(number "26")
				)
				(pin bidirectional line
					(at 25.4 -27.94 180)
					(length 2.54)
					(name "GPB2")
					(number "27")
				)
				(pin bidirectional line
					(at 25.4 -30.48 180)
					(length 2.54)
					(name "GPB3")
					(number "28")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 2.54)
					(name "EP")
					(number "29")
				)
			)
			(embedded_fonts no)
		)
)
