(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MCP2515_QFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 39.37 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MCP2515_QFN"
				(at 39.37 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MCP2515_QFN"
				(at 39.37 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MCP2515-Family-Data-Sheet-DS20001801K.pdf"
				(at 39.37 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "CAN Interface, CAN Controller, SPI, 1 Mbps, 2.7 V, 5.5 V, QFN, 20 Pins"
				(at 39.37 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 39.37 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MCP2515-E/ML"
				(at 39.37 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 39.37 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 39.37 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, CONTROLLER, CAN, SPI, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MCP2515_QFN_1_1"
				(pin passive line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "CLKOUT")
					(number "1")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "~{TX0RTS}")
					(number "2")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "~{TX1RTS}")
					(number "3")
				)
				(pin no_connect line
					(at 22.86 -30.48 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "4")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "~{TX2RTS}")
					(number "5")
				)
				(pin passive line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "OSC2")
					(number "6")
				)
				(pin passive line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "OSC1")
					(number "7")
				)
				(pin power_in line
					(at 25.4 -35.56 180)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 2.54)
					(name "~{RX1BF}")
					(number "9")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 2.54)
					(name "~{RX0BF}")
					(number "10")
				)
				(pin output line
					(at 0 -22.86 0)
					(length 2.54)
					(name "~{INT}")
					(number "11")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SCK")
					(number "12")
				)
				(pin no_connect line
					(at 22.86 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "13")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "SI")
					(number "14")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 2.54)
					(name "SO")
					(number "15")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{CS}")
					(number "16")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{RESET}")
					(number "17")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "18")
				)
				(pin output line
					(at 25.4 0 180)
					(length 2.54)
					(name "TXCAN")
					(number "19")
				)
				(pin input line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "RXCAN")
					(number "20")
				)
				(pin passive line
					(at 25.4 -35.56 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
