(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MCP4661-502E_QFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MCP4661-502E_QFN"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MCP4661-502E_QFN"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/22107B.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "5kOhm 8-Bit Dual I2C Digital POT with Nonvolatile Memory"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MCP4661-502E/ML"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, POTENTIOMETER, IC, I2C"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MCP4661-502E_QFN_1_1"
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "SCL")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 2.54)
					(name "SDA")
					(number "2")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 2.54)
					(name "VSS")
					(number "3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "4")
				)
				(pin passive line
					(at 22.86 -22.86 180)
					(length 2.54)
					(name "P1B")
					(number "5")
				)
				(pin passive line
					(at 22.86 -20.32 180)
					(length 2.54)
					(name "P1W")
					(number "6")
				)
				(pin passive line
					(at 22.86 -17.78 180)
					(length 2.54)
					(name "P1A")
					(number "7")
				)
				(pin passive line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "P0A")
					(number "8")
				)
				(pin passive line
					(at 22.86 -5.08 180)
					(length 2.54)
					(name "P0W")
					(number "9")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "P0B")
					(number "10")
				)
				(pin no_connect line
					(at 20.32 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "11")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{WP}")
					(number "12")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "A2")
					(number "13")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 2.54)
					(name "A1")
					(number "14")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "15")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "HVC/A0")
					(number "16")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 2.54)
					(name "EP")
					(number "17")
				)
			)
			(embedded_fonts no)
		)
)
