(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MCP73833-AM_MSOP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MCP73833-AM_MSOP"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MCP73833-AM_MSOP"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.microchip.com/mymicrochip/filehandler.aspx?ddocname=en027983"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Battery Charger for 1 Cell  Li-Ion/Li-Pol battery, 6V input, 4.2V / 1.2A output, MSOP-10"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MCP73833-AMI/UN"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, CHARGER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MCP73833-AM_MSOP_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "2")
				)
				(pin output line
					(at 19.05 -2.54 180)
					(length 2.54)
					(name "STAT1")
					(number "3")
				)
				(pin output line
					(at 19.05 -5.08 180)
					(length 2.54)
					(name "STAT2")
					(number "4")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "PROG")
					(number "6")
				)
				(pin output line
					(at 19.05 -7.62 180)
					(length 2.54)
					(name "~{PG}")
					(number "7")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "THERM")
					(number "8")
				)
				(pin passive line
					(at 19.05 0 180)
					(length 2.54)
					(hide yes)
					(name "VBAT")
					(number "9")
				)
				(pin passive line
					(at 19.05 0 180)
					(length 2.54)
					(name "VBAT")
					(number "10")
				)
			)
			(embedded_fonts no)
		)
)
