(footprint "QFN-20-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/qfn_20_05-08-1710.pdf")
	(property "Reference" "REF**"
		(at -0.15 -4.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-20-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
		(at 0 5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -2.3 7 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2.3 8.2 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -2.3 9.4 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.9 -1)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "2" smd roundrect
		(at -1.9 -0.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "3" smd roundrect
		(at -1.9 0)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "4" smd roundrect
		(at -1.9 0.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "5" smd roundrect
		(at -1.9 1)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "6" smd roundrect
		(at -1 1.9 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "7" smd roundrect
		(at -0.5 1.9 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "8" smd roundrect
		(at 0 1.9 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "9" smd roundrect
		(at 0.5 1.9 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "10" smd roundrect
		(at 1 1.9 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "11" smd roundrect
		(at 1.9 1)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "12" smd roundrect
		(at 1.9 0.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "13" smd roundrect
		(at 1.9 0)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "14" smd roundrect
		(at 1.9 -0.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "15" smd roundrect
		(at 1.9 -1)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "16" smd roundrect
		(at 1 -1.9 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "17" smd roundrect
		(at 0.5 -1.9 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "18" smd roundrect
		(at 0 -1.9 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "19" smd roundrect
		(at -0.5 -1.9 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "20" smd roundrect
		(at -1 -1.9 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "21" smd roundrect
		(at 0 0)
		(size 2.45 2.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0)
		(chamfer_ratio 0.15)
		(chamfer top_left)
	)
	(embedded_fonts no)
	(model "antmicro_mcp73871_2cci_ml.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
