(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MCP73871-2CC"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MCP73871-2CC"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MCP73871-2CC"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.microchip.com/mymicrochip/filehandler.aspx?ddocname=en536709"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Battery Charger for 1 Cell Li-Ion/Li-Pol battery, 6V input, 4.2V / 1A output, QFN-20"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MCP73871-2CCI/ML"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, CHARGER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MCP73871-2CC_1_1"
				(pin power_out line
					(at 24.13 0 180)
					(length 2.54)
					(name "OUT")
					(number "1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VPCC")
					(number "2")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SEL")
					(number "3")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "PROG2")
					(number "4")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "THERM")
					(number "5")
				)
				(pin output line
					(at 24.13 -8.89 180)
					(length 2.54)
					(name "~{PG}")
					(number "6")
				)
				(pin output line
					(at 24.13 -13.97 180)
					(length 2.54)
					(name "STAT2")
					(number "7")
				)
				(pin output line
					(at 24.13 -11.43 180)
					(length 2.54)
					(name "STAT1/~{LBO}")
					(number "8")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{TE}")
					(number "9")
				)
				(pin power_in line
					(at 24.13 -20.32 180)
					(length 2.54)
					(name "GND")
					(number "10")
				)
				(pin passive line
					(at 24.13 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "11")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "PROG3")
					(number "12")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "PROG1")
					(number "13")
				)
				(pin passive line
					(at 24.13 -2.54 180)
					(length 2.54)
					(name "VBAT")
					(number "14")
				)
				(pin passive line
					(at 24.13 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VBAT")
					(number "15")
				)
				(pin input line
					(at 24.13 -5.08 180)
					(length 2.54)
					(name "VBAT_SENSE")
					(number "16")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "CE")
					(number "17")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "IN")
					(number "18")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "IN")
					(number "19")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 2.54)
					(hide yes)
					(name "OUT")
					(number "20")
				)
				(pin passive line
					(at 24.13 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
