(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MIMX94398DVMMAA"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 72.39 -2.286 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MIMX94398DVMMAA"
				(at 72.39 -7.366 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MIMX94398DVMMAA"
				(at 72.39 -9.906 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/fact-sheet/iMX94FAMFS.pdf"
				(at 72.39 -12.446 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "4xARM Cortex-A55, 2xARM Cortex-M7, 2xARM Cortex-M33, 1.7GHz, industrial, IoT and automotive iMX943 series processor"
				(at 72.39 -27.686 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MIMX94398DVMMAA"
				(at 72.39 -4.826 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "NXP"
				(at 72.39 -17.526 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 72.39 -20.066 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 72.39 -22.606 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, MICROPROCESSOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MIMX94398DVMMAA_1_1"
				(pin power_in line
					(at 44.45 -74.93 180)
					(length 5.08)
					(name "VSS")
					(number "A1")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A29")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA3")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 5.08)
					(name "VDD_ETH_0P8")
					(number "AA6")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA7")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 5.08)
					(name "VDD_ETH_1P8")
					(number "AA8")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA10")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA11")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 5.08)
					(name "VDD_ANAVDET_1P8")
					(number "AA14")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA16")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA19")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA20")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA22")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(hide yes)
					(name "VDD_ANAVDET_1P8")
					(number "AA26")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA27")
				)
				(pin power_in line
					(at 0 -11.43 0)
					(length 5.08)
					(name "VDD_ANA_0P8")
					(number "AB10")
				)
				(pin power_in line
					(at 0 -62.23 0)
					(length 5.08)
					(name "NVCC_WAKEUP")
					(number "AB18")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 5.08)
					(hide yes)
					(name "NVCC_WAKEUP")
					(number "AB20")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC3")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VDD_ANA_0P8")
					(number "AC24")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE3")
				)
				(pin power_in line
					(at 0 -69.85 0)
					(length 5.08)
					(name "NVCC_ENET1")
					(number "AE12")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE27")
				)
				(pin passive line
					(at 0 -69.85 0)
					(length 5.08)
					(hide yes)
					(name "NVCC_ENET1")
					(number "AF12")
				)
				(pin power_in line
					(at 0 -67.31 0)
					(length 5.08)
					(name "NVCC_ENET")
					(number "AF14")
				)
				(pin power_in line
					(at 0 -72.39 0)
					(length 5.08)
					(name "NVCC_SD2")
					(number "AF16")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VDD_SOC_SENSE")
					(number "AF24")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC_SENSE")
					(number "AF26")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG4")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG6")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG8")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG12")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 5.08)
					(hide yes)
					(name "NVCC_ENET")
					(number "AG14")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG16")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG20")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG24")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG26")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ1")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ29")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C4")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C6")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C8")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C10")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C12")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C14")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C16")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C18")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C22")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C26")
				)
				(pin power_in line
					(at 0 -41.91 0)
					(length 5.08)
					(name "VDD_USB_0P8")
					(number "D8")
				)
				(pin power_in line
					(at 0 -39.37 0)
					(length 5.08)
					(name "VDD_USB_1P8")
					(number "D10")
				)
				(pin power_in line
					(at 0 -48.26 0)
					(length 5.08)
					(name "VDD_PCI_1P8")
					(number "D14")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "NVCC_BBSM_1P8")
					(number "D16")
				)
				(pin power_in line
					(at 0 -55.88 0)
					(length 5.08)
					(name "VREFH_1P8_ADC")
					(number "D18")
				)
				(pin input line
					(at 44.45 -55.88 180)
					(length 5.08)
					(name "CLKIN1")
					(number "D22")
				)
				(pin input line
					(at 44.45 -71.12 180)
					(length 5.08)
					(name "XTALI_24M")
					(number "D26")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E3")
				)
				(pin output line
					(at 44.45 -62.23 180)
					(length 5.08)
					(name "RTC_XTALO")
					(number "E14")
				)
				(pin input line
					(at 44.45 -12.7 180)
					(length 5.08)
					(name "TAMPER1")
					(number "E16")
				)
				(pin input line
					(at 44.45 -58.42 180)
					(length 5.08)
					(name "CLKIN2")
					(number "E22")
				)
				(pin input line
					(at 44.45 -7.62 180)
					(length 5.08)
					(name "PMIC_STBY_REQ")
					(number "E24")
				)
				(pin output line
					(at 44.45 -68.58 180)
					(length 5.08)
					(name "XTALO_24M")
					(number "E26")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E27")
				)
				(pin input line
					(at 44.45 -64.77 180)
					(length 5.08)
					(name "RTC_XTALI")
					(number "F14")
				)
				(pin input line
					(at 44.45 -2.54 180)
					(length 5.08)
					(name "ONOFF")
					(number "F20")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G3")
				)
				(pin power_in line
					(at 0 -52.07 0)
					(length 5.08)
					(name "VDD_LVDS_1P8")
					(number "G6")
				)
				(pin input line
					(at 44.45 -10.16 180)
					(length 5.08)
					(name "TAMPER0")
					(number "G14")
				)
				(pin power_out line
					(at 0 -26.67 0)
					(length 5.08)
					(name "VDD_BBSM_0P8_CAP")
					(number "G16")
				)
				(pin power_in line
					(at 0 -13.97 0)
					(length 5.08)
					(name "VDD_ANA_1P8")
					(number "G22")
				)
				(pin output line
					(at 44.45 -5.08 180)
					(length 5.08)
					(name "PMIC_ON_REQ")
					(number "G24")
				)
				(pin passive line
					(at 0 -52.07 0)
					(length 5.08)
					(hide yes)
					(name "VDD_LVDS_1P8")
					(number "H8")
				)
				(pin power_in line
					(at 0 -36.83 0)
					(length 5.08)
					(name "VDD_USB_3P3")
					(number "H10")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "VDD_USB_3P3")
					(number "H12")
				)
				(pin power_in line
					(at 0 -45.72 0)
					(length 5.08)
					(name "VDD_PCI_0P8")
					(number "H14")
				)
				(pin input line
					(at 44.45 0 180)
					(length 5.08)
					(name "POR_B")
					(number "H16")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDD_ANA_1P8")
					(number "H22")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J3")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VDD_ANA_1P8")
					(number "J6")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J7")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J8")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J10")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J11")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J14")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J16")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J19")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J20")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J22")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VDD_ANA_0P8")
					(number "J23")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J27")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VDD_SOC")
					(number "K10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "K11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "K14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "K15")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "K16")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "K19")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "K20")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L3")
				)
				(pin power_in line
					(at 0 -16.51 0)
					(length 5.08)
					(name "VDDQ_DDR")
					(number "L7")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L8")
				)
				(pin power_in line
					(at 0 -8.89 0)
					(length 5.08)
					(name "VDD_DDR_0P8")
					(number "L9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "L10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "L11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "L12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "L13")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L14")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L16")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "L17")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "L18")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "L19")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "L20")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "L21")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L22")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VDD_ANA_0P8")
					(number "L23")
				)
				(pin power_in line
					(at 0 -59.69 0)
					(length 5.08)
					(name "NVCC_AON")
					(number "L26")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "M14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "M16")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M19")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N3")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_DDR")
					(number "N7")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N8")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VDD_DDR_0P8")
					(number "N9")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VDD_DDR_0P8")
					(number "N10")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "N12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "N13")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "N14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "N15")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "N16")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "N17")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "N18")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N19")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "N20")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "N21")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N22")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 5.08)
					(hide yes)
					(name "NVCC_AON")
					(number "N26")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N27")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "P14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "P16")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P19")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R3")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_DDR")
					(number "R5")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_DDR")
					(number "R6")
				)
				(pin power_in line
					(at 0 -19.05 0)
					(length 5.08)
					(name "VDD2H_DDR")
					(number "R7")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R8")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VDD_DDR_0P8")
					(number "R9")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VDD_DDR_0P8")
					(number "R10")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R11")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R12")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R13")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R14")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R16")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R17")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R18")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R19")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "R20")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "R21")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R22")
				)
				(pin power_in line
					(at 0 -64.77 0)
					(length 5.08)
					(name "NVCC_GPIO")
					(number "R26")
				)
				(pin passive line
					(at 0 -64.77 0)
					(length 5.08)
					(hide yes)
					(name "NVCC_GPIO")
					(number "R27")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "T14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "T16")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T19")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U3")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_DDR")
					(number "U7")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U8")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VDD_DDR_0P8")
					(number "U9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U10")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U13")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U15")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U16")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U17")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U18")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U19")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U20")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U21")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U22")
				)
				(pin passive line
					(at 0 -64.77 0)
					(length 5.08)
					(hide yes)
					(name "NVCC_GPIO")
					(number "U23")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U27")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "V14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "V16")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V19")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W3")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_DDR")
					(number "W7")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W8")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VDD_DDR_0P8")
					(number "W9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "W10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "W11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "W12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "W13")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W14")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W16")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "W17")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "W18")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "W19")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "W20")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "W21")
				)
				(pin passive line
					(at 44.45 -74.93 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W22")
				)
				(pin power_in line
					(at 0 -74.93 0)
					(length 5.08)
					(name "NVCC_CCM_DAP")
					(number "W27")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "Y10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "Y11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "Y14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "Y15")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "Y16")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "Y19")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "Y20")
				)
			)
			(symbol "MIMX94398DVMMAA_2_1"
				(pin bidirectional line
					(at 59.69 -54.61 180)
					(length 5.08)
					(name "DRAM_DMI0_B")
					(number "A2")
				)
				(pin bidirectional line
					(at 59.69 -85.09 180)
					(length 5.08)
					(name "DRAM_DQ05_B")
					(number "A3")
				)
				(pin bidirectional line
					(at 59.69 -90.17 180)
					(length 5.08)
					(name "DRAM_DQ07_B")
					(number "A4")
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 5.08)
					(name "DRAM_DQ01_A")
					(number "AA1")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 5.08)
					(name "DRAM_DQ00_A")
					(number "AA2")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "DRAM_DQS0_C_A")
					(number "AA4")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "DRAM_DQS0_T_A")
					(number "AA5")
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 5.08)
					(name "DRAM_DQ02_A")
					(number "AB1")
				)
				(pin bidirectional line
					(at 0 -107.95 0)
					(length 5.08)
					(name "DRAM_DQ14_A")
					(number "AB2")
				)
				(pin bidirectional line
					(at 0 -110.49 0)
					(length 5.08)
					(name "DRAM_DQ15_A")
					(number "AC1")
				)
				(pin bidirectional line
					(at 0 -105.41 0)
					(length 5.08)
					(name "DRAM_DQ13_A")
					(number "AC2")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "DRAM_WCK1_T_A")
					(number "AC4")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "DRAM_WCK1_C_A")
					(number "AC5")
				)
				(pin bidirectional line
					(at 0 -100.33 0)
					(length 5.08)
					(name "DRAM_DQ11_A")
					(number "AD1")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "DRAM_DMI1_A")
					(number "AD2")
				)
				(pin bidirectional line
					(at 0 -102.87 0)
					(length 5.08)
					(name "DRAM_DQ12_A")
					(number "AE1")
				)
				(pin bidirectional line
					(at 0 -92.71 0)
					(length 5.08)
					(name "DRAM_DQ08_A")
					(number "AE2")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "DRAM_DQS1_C_A")
					(number "AE4")
				)
				(pin bidirectional line
					(at 0 -97.79 0)
					(length 5.08)
					(name "DRAM_DQ10_A")
					(number "AF1")
				)
				(pin bidirectional line
					(at 0 -95.25 0)
					(length 5.08)
					(name "DRAM_DQ09_A")
					(number "AF2")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "DRAM_DQS1_T_A")
					(number "AF4")
				)
				(pin bidirectional line
					(at 59.69 -74.93 180)
					(length 5.08)
					(name "DRAM_DQ01_B")
					(number "B1")
				)
				(pin bidirectional line
					(at 59.69 -80.01 180)
					(length 5.08)
					(name "DRAM_DQ03_B")
					(number "B2")
				)
				(pin bidirectional line
					(at 59.69 -82.55 180)
					(length 5.08)
					(name "DRAM_DQ04_B")
					(number "B3")
				)
				(pin bidirectional line
					(at 59.69 -87.63 180)
					(length 5.08)
					(name "DRAM_DQ06_B")
					(number "B4")
				)
				(pin bidirectional line
					(at 59.69 -72.39 180)
					(length 5.08)
					(name "DRAM_DQ00_B")
					(number "C1")
				)
				(pin bidirectional line
					(at 59.69 -77.47 180)
					(length 5.08)
					(name "DRAM_DQ02_B")
					(number "C2")
				)
				(pin bidirectional line
					(at 59.69 -107.95 180)
					(length 5.08)
					(name "DRAM_DQ14_B")
					(number "D1")
				)
				(pin bidirectional line
					(at 59.69 -105.41 180)
					(length 5.08)
					(name "DRAM_DQ13_B")
					(number "D2")
				)
				(pin bidirectional line
					(at 59.69 -60.96 180)
					(length 5.08)
					(name "DRAM_DQS0_T_B")
					(number "D4")
				)
				(pin bidirectional line
					(at 59.69 -110.49 180)
					(length 5.08)
					(name "DRAM_DQ15_B")
					(number "E1")
				)
				(pin bidirectional line
					(at 59.69 -102.87 180)
					(length 5.08)
					(name "DRAM_DQ12_B")
					(number "E2")
				)
				(pin bidirectional line
					(at 59.69 -63.5 180)
					(length 5.08)
					(name "DRAM_DQS0_C_B")
					(number "E4")
				)
				(pin bidirectional line
					(at 59.69 -57.15 180)
					(length 5.08)
					(name "DRAM_DMI1_B")
					(number "F1")
				)
				(pin bidirectional line
					(at 59.69 -95.25 180)
					(length 5.08)
					(name "DRAM_DQ09_B")
					(number "F2")
				)
				(pin bidirectional line
					(at 59.69 -97.79 180)
					(length 5.08)
					(name "DRAM_DQ10_B")
					(number "G1")
				)
				(pin bidirectional line
					(at 59.69 -100.33 180)
					(length 5.08)
					(name "DRAM_DQ11_B")
					(number "G2")
				)
				(pin bidirectional line
					(at 59.69 -24.13 180)
					(length 5.08)
					(name "DRAM_WCK0_C_B")
					(number "G4")
				)
				(pin bidirectional line
					(at 59.69 -21.59 180)
					(length 5.08)
					(name "DRAM_WCK0_T_B")
					(number "G5")
				)
				(pin bidirectional line
					(at 59.69 -92.71 180)
					(length 5.08)
					(name "DRAM_DQ08_B")
					(number "H1")
				)
				(pin bidirectional line
					(at 59.69 -43.18 180)
					(length 5.08)
					(name "DRAM_CA4_B")
					(number "H2")
				)
				(pin bidirectional line
					(at 59.69 -48.26 180)
					(length 5.08)
					(name "DRAM_CA6_B")
					(number "J1")
				)
				(pin bidirectional line
					(at 59.69 -40.64 180)
					(length 5.08)
					(name "DRAM_CA3_B")
					(number "J2")
				)
				(pin bidirectional line
					(at 59.69 -68.58 180)
					(length 5.08)
					(name "DRAM_DQS1_C_B")
					(number "J4")
				)
				(pin bidirectional line
					(at 59.69 -66.04 180)
					(length 5.08)
					(name "DRAM_DQS1_T_B")
					(number "J5")
				)
				(pin bidirectional line
					(at 59.69 -19.05 180)
					(length 5.08)
					(name "DRAM_LP4CKE_LP5CS1_B")
					(number "K1")
				)
				(pin bidirectional line
					(at 59.69 -45.72 180)
					(length 5.08)
					(name "DRAM_CA5_B")
					(number "K2")
				)
				(pin bidirectional line
					(at 59.69 -33.02 180)
					(length 5.08)
					(name "DRAM_CA0_B")
					(number "L1")
				)
				(pin bidirectional line
					(at 59.69 -38.1 180)
					(length 5.08)
					(name "DRAM_CA2_B")
					(number "L2")
				)
				(pin bidirectional line
					(at 59.69 -26.67 180)
					(length 5.08)
					(name "DRAM_WCK1_T_B")
					(number "L4")
				)
				(pin bidirectional line
					(at 59.69 -29.21 180)
					(length 5.08)
					(name "DRAM_WCK1_C_B")
					(number "L5")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "DRAM_DTO")
					(number "L6")
				)
				(pin bidirectional line
					(at 59.69 -35.56 180)
					(length 5.08)
					(name "DRAM_CA1_B")
					(number "M1")
				)
				(pin bidirectional line
					(at 59.69 -50.8 180)
					(length 5.08)
					(name "DRAM_CA7_B")
					(number "M2")
				)
				(pin bidirectional line
					(at 59.69 -16.51 180)
					(length 5.08)
					(name "DRAM_LP4CKE_LP5CS0_B")
					(number "N1")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 5.08)
					(name "DRAM_LP4CKE_LP5CS0_A")
					(number "N2")
				)
				(pin bidirectional line
					(at 59.69 -13.97 180)
					(length 5.08)
					(name "DRAM_CK_C_B")
					(number "N4")
				)
				(pin bidirectional line
					(at 59.69 -11.43 180)
					(length 5.08)
					(name "DRAM_CK_T_B")
					(number "N5")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 5.08)
					(name "DRAM_RESET_N")
					(number "N6")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "DRAM_CA0_A")
					(number "P1")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "DRAM_CA1_A")
					(number "P2")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "DRAM_CA7_A")
					(number "R1")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 5.08)
					(name "DRAM_LP4CKE_LP5CS1_A")
					(number "R2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "DRAM_ATO")
					(number "R4")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "DRAM_CA3_A")
					(number "T1")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "DRAM_CA2_A")
					(number "T2")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "DRAM_CA4_A")
					(number "U1")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "DRAM_CA5_A")
					(number "U2")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 5.08)
					(name "DRAM_CK_C_A")
					(number "U4")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "DRAM_CK_T_A")
					(number "U5")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "DRAM_ZN")
					(number "U6")
				)
				(pin bidirectional line
					(at 0 -87.63 0)
					(length 5.08)
					(name "DRAM_DQ06_A")
					(number "V1")
				)
				(pin bidirectional line
					(at 0 -82.55 0)
					(length 5.08)
					(name "DRAM_DQ04_A")
					(number "V2")
				)
				(pin bidirectional line
					(at 0 -90.17 0)
					(length 5.08)
					(name "DRAM_DQ07_A")
					(number "W1")
				)
				(pin bidirectional line
					(at 0 -85.09 0)
					(length 5.08)
					(name "DRAM_DQ05_A")
					(number "W2")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "DRAM_WCK0_T_A")
					(number "W4")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "DRAM_WCK0_C_A")
					(number "W5")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "DRAM_CA6_A")
					(number "W6")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "DRAM_DMI0_A")
					(number "Y1")
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 5.08)
					(name "DRAM_DQ03_A")
					(number "Y2")
				)
			)
			(symbol "MIMX94398DVMMAA_3_1"
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "ETH0_RXD2")
					(number "AB8")
				)
				(pin output line
					(at 0 -81.28 0)
					(length 5.08)
					(name "ETH1_TXD2")
					(number "AB12")
				)
				(pin output line
					(at 52.07 -10.16 180)
					(length 5.08)
					(name "ETH2_TXD0")
					(number "AB14")
				)
				(pin output line
					(at 52.07 -12.7 180)
					(length 5.08)
					(name "ETH2_TXD1")
					(number "AB16")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "ETH0_RX_DV")
					(number "AC6")
				)
				(pin input line
					(at 0 -52.07 0)
					(length 5.08)
					(name "ETH0_RXD1")
					(number "AC8")
				)
				(pin input line
					(at 0 -57.15 0)
					(length 5.08)
					(name "ETH0_RXD3")
					(number "AC10")
				)
				(pin output line
					(at 0 -78.74 0)
					(length 5.08)
					(name "ETH1_TXD1")
					(number "AC12")
				)
				(pin output line
					(at 52.07 -7.62 180)
					(length 5.08)
					(name "ETH2_TX_CTL")
					(number "AC14")
				)
				(pin output line
					(at 52.07 -15.24 180)
					(length 5.08)
					(name "ETH2_TXD2")
					(number "AC16")
				)
				(pin output line
					(at 52.07 -54.61 180)
					(length 5.08)
					(name "ETH3_TXD3")
					(number "AC18")
				)
				(pin bidirectional line
					(at 52.07 -78.74 180)
					(length 5.08)
					(name "ETH4_TX_CLK")
					(number "AC20")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "ETH0_RX_CLK")
					(number "AD6")
				)
				(pin input line
					(at 0 -49.53 0)
					(length 5.08)
					(name "ETH0_RXD0")
					(number "AD8")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "ETH0_RX_ER")
					(number "AD10")
				)
				(pin output line
					(at 0 -76.2 0)
					(length 5.08)
					(name "ETH1_TXD0")
					(number "AD12")
				)
				(pin bidirectional line
					(at 52.07 -5.08 180)
					(length 5.08)
					(name "ETH2_TX_CLK")
					(number "AD14")
				)
				(pin output line
					(at 52.07 -17.78 180)
					(length 5.08)
					(name "ETH2_TXD3")
					(number "AD16")
				)
				(pin output line
					(at 52.07 -52.07 180)
					(length 5.08)
					(name "ETH3_TXD2")
					(number "AD18")
				)
				(pin output line
					(at 52.07 -81.28 180)
					(length 5.08)
					(name "ETH4_TX_CTL")
					(number "AD20")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "ETH_RX0_N")
					(number "AE6")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "ETH_RX1_N")
					(number "AE8")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "ETH1_TX_CLK")
					(number "AE10")
				)
				(pin output line
					(at 0 -83.82 0)
					(length 5.08)
					(name "ETH1_TXD3")
					(number "AE14")
				)
				(pin bidirectional line
					(at 52.07 -41.91 180)
					(length 5.08)
					(name "ETH3_TX_CLK")
					(number "AE16")
				)
				(pin output line
					(at 52.07 -49.53 180)
					(length 5.08)
					(name "ETH3_TXD1")
					(number "AE18")
				)
				(pin output line
					(at 52.07 -83.82 180)
					(length 5.08)
					(name "ETH4_TXD0")
					(number "AE20")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "ETH_RX0_P")
					(number "AF6")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "ETH_RX1_P")
					(number "AF8")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "ETH1_TX_EN")
					(number "AF10")
				)
				(pin output line
					(at 52.07 -46.99 180)
					(length 5.08)
					(name "ETH3_TXD0")
					(number "AF18")
				)
				(pin output line
					(at 52.07 -86.36 180)
					(length 5.08)
					(name "ETH4_TXD1")
					(number "AF20")
				)
				(pin output line
					(at 52.07 -91.44 180)
					(length 5.08)
					(name "ETH4_TXD3")
					(number "AF22")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "ETH_REF_PAD_CLK_N")
					(number "AG1")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "ETH_REF_PAD_CLK_P")
					(number "AG2")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "ETH1_TX_ER")
					(number "AG10")
				)
				(pin bidirectional line
					(at 52.07 -44.45 180)
					(length 5.08)
					(name "ETH3_TX_CTL")
					(number "AG18")
				)
				(pin bidirectional line
					(at 52.07 -88.9 180)
					(length 5.08)
					(name "ETH4_TXD2")
					(number "AG22")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 5.08)
					(name "ETH_TX0_P")
					(number "AH1")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 5.08)
					(name "ETH_TX0_N")
					(number "AH2")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 5.08)
					(name "ETH_TX1_P")
					(number "AH3")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "ETH0_TX_ER")
					(number "AH4")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "ETH0_TX_CLK")
					(number "AH5")
				)
				(pin output line
					(at 0 -36.83 0)
					(length 5.08)
					(name "ETH0_TXD1")
					(number "AH6")
				)
				(pin output line
					(at 0 -41.91 0)
					(length 5.08)
					(name "ETH0_TXD3")
					(number "AH7")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "ETH0_CRS")
					(number "AH8")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "ETH1_RX_DV")
					(number "AH9")
				)
				(pin input line
					(at 0 -93.98 0)
					(length 5.08)
					(name "ETH1_RXD1")
					(number "AH10")
				)
				(pin input line
					(at 0 -99.06 0)
					(length 5.08)
					(name "ETH1_RXD3")
					(number "AH11")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "ETH1_COL")
					(number "AH12")
				)
				(pin bidirectional line
					(at 52.07 -20.32 180)
					(length 5.08)
					(name "ETH2_RX_CLK")
					(number "AH13")
				)
				(pin input line
					(at 52.07 -25.4 180)
					(length 5.08)
					(name "ETH2_RXD0")
					(number "AH14")
				)
				(pin input line
					(at 52.07 -30.48 180)
					(length 5.08)
					(name "ETH2_RXD2")
					(number "AH15")
				)
				(pin bidirectional line
					(at 52.07 -2.54 180)
					(length 5.08)
					(name "ETH2_MDIO_GPIO2")
					(number "AH16")
				)
				(pin bidirectional line
					(at 52.07 -57.15 180)
					(length 5.08)
					(name "ETH3_RX_CLK")
					(number "AH17")
				)
				(pin input line
					(at 52.07 -62.23 180)
					(length 5.08)
					(name "ETH3_RXD0")
					(number "AH18")
				)
				(pin input line
					(at 52.07 -67.31 180)
					(length 5.08)
					(name "ETH3_RXD2")
					(number "AH19")
				)
				(pin bidirectional line
					(at 52.07 -39.37 180)
					(length 5.08)
					(name "ETH3_MDIO_GPIO2")
					(number "AH20")
				)
				(pin bidirectional line
					(at 52.07 -93.98 180)
					(length 5.08)
					(name "ETH4_RX_CLK")
					(number "AH21")
				)
				(pin input line
					(at 52.07 -99.06 180)
					(length 5.08)
					(name "ETH4_RXD0")
					(number "AH22")
				)
				(pin input line
					(at 52.07 -104.14 180)
					(length 5.08)
					(name "ETH4_RXD2")
					(number "AH23")
				)
				(pin bidirectional line
					(at 52.07 -76.2 180)
					(length 5.08)
					(name "ETH4_MDIO_GPIO2")
					(number "AH24")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "ETH_RESREF")
					(number "AJ2")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 5.08)
					(name "ETH_TX1_N")
					(number "AJ3")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "ETH0_TX_EN")
					(number "AJ4")
				)
				(pin output line
					(at 0 -34.29 0)
					(length 5.08)
					(name "ETH0_TXD0")
					(number "AJ5")
				)
				(pin output line
					(at 0 -39.37 0)
					(length 5.08)
					(name "ETH0_TXD2")
					(number "AJ6")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 5.08)
					(name "ETH0_COL")
					(number "AJ7")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "ETH1_RX_CLK")
					(number "AJ8")
				)
				(pin input line
					(at 0 -91.44 0)
					(length 5.08)
					(name "ETH1_RXD0")
					(number "AJ9")
				)
				(pin input line
					(at 0 -96.52 0)
					(length 5.08)
					(name "ETH1_RXD2")
					(number "AJ10")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "ETH1_RX_ER")
					(number "AJ11")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "ETH1_CRS")
					(number "AJ12")
				)
				(pin bidirectional line
					(at 52.07 -22.86 180)
					(length 5.08)
					(name "ETH2_RX_CTL")
					(number "AJ13")
				)
				(pin input line
					(at 52.07 -27.94 180)
					(length 5.08)
					(name "ETH2_RXD1")
					(number "AJ14")
				)
				(pin input line
					(at 52.07 -33.02 180)
					(length 5.08)
					(name "ETH2_RXD3")
					(number "AJ15")
				)
				(pin bidirectional line
					(at 52.07 0 180)
					(length 5.08)
					(name "ETH2_MDC_GPIO1")
					(number "AJ16")
				)
				(pin bidirectional line
					(at 52.07 -59.69 180)
					(length 5.08)
					(name "ETH3_RX_CTL")
					(number "AJ17")
				)
				(pin input line
					(at 52.07 -64.77 180)
					(length 5.08)
					(name "ETH3_RXD1")
					(number "AJ18")
				)
				(pin input line
					(at 52.07 -69.85 180)
					(length 5.08)
					(name "ETH3_RXD3")
					(number "AJ19")
				)
				(pin bidirectional line
					(at 52.07 -36.83 180)
					(length 5.08)
					(name "ETH3_MDC_GPIO1")
					(number "AJ20")
				)
				(pin bidirectional line
					(at 52.07 -96.52 180)
					(length 5.08)
					(name "ETH4_RX_CTL")
					(number "AJ21")
				)
				(pin input line
					(at 52.07 -101.6 180)
					(length 5.08)
					(name "ETH4_RXD1")
					(number "AJ22")
				)
				(pin input line
					(at 52.07 -106.68 180)
					(length 5.08)
					(name "ETH4_RXD3")
					(number "AJ23")
				)
				(pin bidirectional line
					(at 52.07 -73.66 180)
					(length 5.08)
					(name "ETH4_MDC_GPIO1")
					(number "AJ24")
				)
			)
			(symbol "MIMX94398DVMMAA_4_1"
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "LVDS0_D0_N")
					(number "A5")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 5.08)
					(name "LVDS0_D1_N")
					(number "A6")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "LVDS0_CLK_N")
					(number "A7")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 5.08)
					(name "LVDS0_D2_N")
					(number "A8")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "LVDS0_D3_N")
					(number "A9")
				)
				(pin output line
					(at 49.53 -20.32 180)
					(length 5.08)
					(name "USB1_TX1_N")
					(number "A10")
				)
				(pin input line
					(at 49.53 -30.48 180)
					(length 5.08)
					(name "USB1_RX1_N")
					(number "A11")
				)
				(pin output line
					(at 49.53 -12.7 180)
					(length 5.08)
					(name "USB1_TX0_P")
					(number "A12")
				)
				(pin input line
					(at 49.53 -22.86 180)
					(length 5.08)
					(name "USB1_RX0_P")
					(number "A13")
				)
				(pin output line
					(at 0 -16.51 0)
					(length 5.08)
					(name "PCIE1_TX0_N")
					(number "A14")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 5.08)
					(name "PCIE1_RX0_N")
					(number "A15")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 5.08)
					(name "PCIE1_REF_PAD_CLK_N")
					(number "A16")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PCIE2_TX0_N")
					(number "A17")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PCIE2_RX0_N")
					(number "A18")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PCIE2_REF_PAD_CLK_N")
					(number "A19")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "LVDS0_D0_P")
					(number "B5")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 5.08)
					(name "LVDS0_D1_P")
					(number "B6")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "LVDS0_CLK_P")
					(number "B7")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 5.08)
					(name "LVDS0_D2_P")
					(number "B8")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "LVDS0_D3_P")
					(number "B9")
				)
				(pin output line
					(at 49.53 -17.78 180)
					(length 5.08)
					(name "USB1_TX1_P")
					(number "B10")
				)
				(pin bidirectional line
					(at 49.53 -27.94 180)
					(length 5.08)
					(name "USB1_RX1_P")
					(number "B11")
				)
				(pin output line
					(at 49.53 -15.24 180)
					(length 5.08)
					(name "USB1_TX0_N")
					(number "B12")
				)
				(pin bidirectional line
					(at 49.53 -25.4 180)
					(length 5.08)
					(name "USB1_RX0_N")
					(number "B13")
				)
				(pin output line
					(at 0 -13.97 0)
					(length 5.08)
					(name "PCIE1_TX0_P")
					(number "B14")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 5.08)
					(name "PCIE1_RX0_P")
					(number "B15")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 5.08)
					(name "PCIE1_REF_PAD_CLK_P")
					(number "B16")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PCIE2_TX0_P")
					(number "B17")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "PCIE2_RX0_P")
					(number "B18")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PCIE2_REF_PAD_CLK_P")
					(number "B19")
				)
				(pin input line
					(at 49.53 -34.29 180)
					(length 5.08)
					(name "USB2_VBUS")
					(number "D6")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PCIE_RESREF")
					(number "D12")
				)
				(pin input line
					(at 49.53 0 180)
					(length 5.08)
					(name "USB1_VBUS")
					(number "E6")
				)
				(pin bidirectional line
					(at 49.53 -7.62 180)
					(length 5.08)
					(name "USB1_D_P")
					(number "E8")
				)
				(pin bidirectional line
					(at 49.53 -44.45 180)
					(length 5.08)
					(name "USB2_D_N")
					(number "E10")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PCIE_REF_OUT_CLK_N")
					(number "E12")
				)
				(pin input line
					(at 49.53 -5.08 180)
					(length 5.08)
					(name "USB1_TXRTUNE")
					(number "F6")
				)
				(pin bidirectional line
					(at 49.53 -10.16 180)
					(length 5.08)
					(name "USB1_D_N")
					(number "F8")
				)
				(pin bidirectional line
					(at 49.53 -41.91 180)
					(length 5.08)
					(name "USB2_D_P")
					(number "F10")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "PCIE_REF_OUT_CLK_P")
					(number "F12")
				)
				(pin no_connect line
					(at 44.45 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "USB1_DNU")
					(number "G8")
				)
				(pin input line
					(at 49.53 -36.83 180)
					(length 5.08)
					(name "USB2_ID")
					(number "G10")
				)
				(pin input line
					(at 49.53 -39.37 180)
					(length 5.08)
					(name "USB2_TXRTUNE")
					(number "G12")
				)
			)
			(symbol "MIMX94398DVMMAA_5_1"
				(pin output line
					(at 0 -81.28 0)
					(length 5.08)
					(name "UART1_TXD")
					(number "A20")
				)
				(pin output line
					(at 0 -86.36 0)
					(length 5.08)
					(name "UART2_TXD")
					(number "A21")
				)
				(pin bidirectional line
					(at 45.72 -22.86 180)
					(length 5.08)
					(name "SD1_DATA7")
					(number "AA23")
				)
				(pin bidirectional line
					(at 45.72 -71.12 180)
					(length 5.08)
					(name "CCM_CLKO4")
					(number "AA24")
				)
				(pin bidirectional line
					(at 45.72 -68.58 180)
					(length 5.08)
					(name "CCM_CLKO3")
					(number "AA25")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 5.08)
					(name "XSPI1_DATA5")
					(number "AA28")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 5.08)
					(name "XSPI1_DATA6")
					(number "AA29")
				)
				(pin bidirectional line
					(at 45.72 -12.7 180)
					(length 5.08)
					(name "SD1_DATA3")
					(number "AB22")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 5.08)
					(name "XSPI1_DATA3")
					(number "AB28")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 5.08)
					(name "XSPI1_DATA4")
					(number "AB29")
				)
				(pin bidirectional line
					(at 45.72 -25.4 180)
					(length 5.08)
					(name "SD1_STROBE")
					(number "AC22")
				)
				(pin bidirectional line
					(at 45.72 -20.32 180)
					(length 5.08)
					(name "SD1_DATA6")
					(number "AC25")
				)
				(pin bidirectional line
					(at 45.72 -7.62 180)
					(length 5.08)
					(name "SD1_DATA1")
					(number "AC26")
				)
				(pin bidirectional line
					(at 45.72 -10.16 180)
					(length 5.08)
					(name "SD1_DATA2")
					(number "AC27")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 5.08)
					(name "XSPI1_DATA1")
					(number "AC28")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 5.08)
					(name "XSPI1_DATA2")
					(number "AC29")
				)
				(pin bidirectional line
					(at 45.72 -2.54 180)
					(length 5.08)
					(name "SD1_CMD")
					(number "AD22")
				)
				(pin bidirectional line
					(at 45.72 -5.08 180)
					(length 5.08)
					(name "SD1_DATA0")
					(number "AD24")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 5.08)
					(name "XSPI1_DQS")
					(number "AD28")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 5.08)
					(name "XSPI1_DATA0")
					(number "AD29")
				)
				(pin bidirectional line
					(at 45.72 0 180)
					(length 5.08)
					(name "SD1_CLK")
					(number "AE22")
				)
				(pin bidirectional line
					(at 45.72 -15.24 180)
					(length 5.08)
					(name "SD1_DATA4")
					(number "AE24")
				)
				(pin bidirectional line
					(at 45.72 -17.78 180)
					(length 5.08)
					(name "SD1_DATA5")
					(number "AE26")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 5.08)
					(name "XSPI1_SCLK")
					(number "AE28")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 5.08)
					(name "XSPI1_SS1_B")
					(number "AE29")
				)
				(pin bidirectional line
					(at 45.72 -57.15 180)
					(length 5.08)
					(name "SD2_GPIO2")
					(number "AF28")
				)
				(pin bidirectional line
					(at 45.72 -59.69 180)
					(length 5.08)
					(name "SD2_GPIO3")
					(number "AF29")
				)
				(pin bidirectional line
					(at 45.72 -54.61 180)
					(length 5.08)
					(name "SD2_GPIO0")
					(number "AG28")
				)
				(pin bidirectional line
					(at 45.72 -52.07 180)
					(length 5.08)
					(name "SD2_GPIO1")
					(number "AG29")
				)
				(pin bidirectional line
					(at 45.72 -36.83 180)
					(length 5.08)
					(name "SD2_CD_B")
					(number "AH25")
				)
				(pin bidirectional line
					(at 45.72 -41.91 180)
					(length 5.08)
					(name "SD2_DATA0")
					(number "AH26")
				)
				(pin bidirectional line
					(at 45.72 -34.29 180)
					(length 5.08)
					(name "SD2_CMD")
					(number "AH27")
				)
				(pin bidirectional line
					(at 45.72 -46.99 180)
					(length 5.08)
					(name "SD2_DATA2")
					(number "AH28")
				)
				(pin bidirectional line
					(at 45.72 -49.53 180)
					(length 5.08)
					(name "SD2_DATA3")
					(number "AH29")
				)
				(pin bidirectional line
					(at 45.72 -29.21 180)
					(length 5.08)
					(name "SD2_RESET_B")
					(number "AJ25")
				)
				(pin bidirectional line
					(at 45.72 -39.37 180)
					(length 5.08)
					(name "SD2_VSELECT")
					(number "AJ26")
				)
				(pin bidirectional line
					(at 45.72 -44.45 180)
					(length 5.08)
					(name "SD2_DATA1")
					(number "AJ27")
				)
				(pin bidirectional line
					(at 45.72 -31.75 180)
					(length 5.08)
					(name "SD2_CLK")
					(number "AJ28")
				)
				(pin output line
					(at 45.72 -85.09 180)
					(length 5.08)
					(name "I2C1_SCL")
					(number "B20")
				)
				(pin input line
					(at 0 -78.74 0)
					(length 5.08)
					(name "UART1_RXD")
					(number "B21")
				)
				(pin input line
					(at 0 -83.82 0)
					(length 5.08)
					(name "UART2_RXD")
					(number "B22")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "PDM_BIT_STREAM1")
					(number "B24")
				)
				(pin bidirectional line
					(at 45.72 -93.98 180)
					(length 5.08)
					(name "I2C2_SDA")
					(number "C20")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PDM_CLK")
					(number "C24")
				)
				(pin bidirectional line
					(at 45.72 -87.63 180)
					(length 5.08)
					(name "I2C1_SDA")
					(number "D20")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 5.08)
					(name "PDM_BIT_STREAM0")
					(number "D24")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "ADC_IN7")
					(number "E18")
				)
				(pin output line
					(at 45.72 -91.44 180)
					(length 5.08)
					(name "I2C2_SCL")
					(number "E20")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "ADC_IN5")
					(number "F16")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "ADC_IN6")
					(number "F18")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "ADC_IN0")
					(number "F22")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 5.08)
					(name "SAI1_TXFS")
					(number "F24")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "ADC_IN3")
					(number "G18")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "ADC_IN2")
					(number "G20")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 5.08)
					(name "SAI1_TXC")
					(number "G25")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "WDOG_ANY")
					(number "G26")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "ADC_IN4")
					(number "H18")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "ADC_IN1")
					(number "H20")
				)
				(pin output line
					(at 0 -69.85 0)
					(length 5.08)
					(name "SAI1_TXD0")
					(number "J24")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "FCCU_ERR0")
					(number "J25")
				)
				(pin input line
					(at 0 -67.31 0)
					(length 5.08)
					(name "SAI1_RXD0")
					(number "J26")
				)
				(pin bidirectional line
					(at 45.72 -66.04 180)
					(length 5.08)
					(name "CCM_CLKO2")
					(number "W23")
				)
				(pin output line
					(at 45.72 -81.28 180)
					(length 5.08)
					(name "DAP_TDO_TRACESWO")
					(number "W24")
				)
				(pin bidirectional line
					(at 45.72 -63.5 180)
					(length 5.08)
					(name "CCM_CLKO1")
					(number "W25")
				)
				(pin bidirectional line
					(at 45.72 -78.74 180)
					(length 5.08)
					(name "DAP_TCLK_SWCLK")
					(number "W26")
				)
				(pin input line
					(at 45.72 -76.2 180)
					(length 5.08)
					(name "DAP_TMS_SWDIO")
					(number "W28")
				)
				(pin input line
					(at 45.72 -73.66 180)
					(length 5.08)
					(name "DAP_TDI")
					(number "W29")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 5.08)
					(name "XSPI1_DATA7")
					(number "Y28")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 5.08)
					(name "XSPI1_SS0_B")
					(number "Y29")
				)
			)
			(symbol "MIMX94398DVMMAA_6_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "GPIO_IO00")
					(number "A22")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "GPIO_IO01")
					(number "A23")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "GPIO_IO03")
					(number "A24")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "GPIO_IO05")
					(number "A25")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "GPIO_IO07")
					(number "A26")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "GPIO_IO09")
					(number "A27")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "GPIO_IO10")
					(number "A28")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "GPIO_IO02")
					(number "B23")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "GPIO_IO04")
					(number "B25")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "GPIO_IO06")
					(number "B26")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "GPIO_IO08")
					(number "B27")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "GPIO_IO11")
					(number "B28")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "GPIO_IO12")
					(number "B29")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "GPIO_IO13")
					(number "C28")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "GPIO_IO14")
					(number "C29")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "GPIO_IO15")
					(number "D28")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "GPIO_IO16")
					(number "D29")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GPIO_IO17")
					(number "E28")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "GPIO_IO18")
					(number "E29")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "GPIO_IO19")
					(number "F28")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "GPIO_IO20")
					(number "F29")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "GPIO_IO21")
					(number "G27")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "GPIO_IO22")
					(number "G28")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "GPIO_IO23")
					(number "G29")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "GPIO_IO24")
					(number "H28")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "GPIO_IO25")
					(number "H29")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "GPIO_IO26")
					(number "J28")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "GPIO_IO27")
					(number "J29")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "GPIO_IO28")
					(number "K28")
				)
				(pin bidirectional line
					(at 34.29 0 180)
					(length 5.08)
					(name "GPIO_IO29")
					(number "K29")
				)
				(pin bidirectional line
					(at 34.29 -2.54 180)
					(length 5.08)
					(name "GPIO_IO30")
					(number "L24")
				)
				(pin bidirectional line
					(at 34.29 -5.08 180)
					(length 5.08)
					(name "GPIO_IO31")
					(number "L25")
				)
				(pin bidirectional line
					(at 34.29 -7.62 180)
					(length 5.08)
					(name "GPIO_IO32")
					(number "L27")
				)
				(pin bidirectional line
					(at 34.29 -10.16 180)
					(length 5.08)
					(name "GPIO_IO33")
					(number "L28")
				)
				(pin bidirectional line
					(at 34.29 -12.7 180)
					(length 5.08)
					(name "GPIO_IO34")
					(number "L29")
				)
				(pin bidirectional line
					(at 34.29 -15.24 180)
					(length 5.08)
					(name "GPIO_IO35")
					(number "M28")
				)
				(pin bidirectional line
					(at 34.29 -17.78 180)
					(length 5.08)
					(name "GPIO_IO36")
					(number "M29")
				)
				(pin bidirectional line
					(at 34.29 -20.32 180)
					(length 5.08)
					(name "GPIO_IO37")
					(number "N23")
				)
				(pin bidirectional line
					(at 34.29 -22.86 180)
					(length 5.08)
					(name "GPIO_IO38")
					(number "N24")
				)
				(pin bidirectional line
					(at 34.29 -25.4 180)
					(length 5.08)
					(name "GPIO_IO39")
					(number "N25")
				)
				(pin bidirectional line
					(at 34.29 -27.94 180)
					(length 5.08)
					(name "GPIO_IO40")
					(number "N28")
				)
				(pin bidirectional line
					(at 34.29 -30.48 180)
					(length 5.08)
					(name "GPIO_IO41")
					(number "N29")
				)
				(pin bidirectional line
					(at 34.29 -33.02 180)
					(length 5.08)
					(name "GPIO_IO42")
					(number "P28")
				)
				(pin bidirectional line
					(at 34.29 -35.56 180)
					(length 5.08)
					(name "GPIO_IO43")
					(number "P29")
				)
				(pin bidirectional line
					(at 34.29 -38.1 180)
					(length 5.08)
					(name "GPIO_IO44")
					(number "R23")
				)
				(pin bidirectional line
					(at 34.29 -40.64 180)
					(length 5.08)
					(name "GPIO_IO45")
					(number "R24")
				)
				(pin bidirectional line
					(at 34.29 -43.18 180)
					(length 5.08)
					(name "GPIO_IO46")
					(number "R25")
				)
				(pin bidirectional line
					(at 34.29 -45.72 180)
					(length 5.08)
					(name "GPIO_IO47")
					(number "R28")
				)
				(pin bidirectional line
					(at 34.29 -48.26 180)
					(length 5.08)
					(name "GPIO_IO48")
					(number "R29")
				)
				(pin bidirectional line
					(at 34.29 -50.8 180)
					(length 5.08)
					(name "GPIO_IO49")
					(number "T28")
				)
				(pin bidirectional line
					(at 34.29 -53.34 180)
					(length 5.08)
					(name "GPIO_IO50")
					(number "T29")
				)
				(pin bidirectional line
					(at 34.29 -55.88 180)
					(length 5.08)
					(name "GPIO_IO51")
					(number "U24")
				)
				(pin bidirectional line
					(at 34.29 -58.42 180)
					(length 5.08)
					(name "GPIO_IO52")
					(number "U25")
				)
				(pin bidirectional line
					(at 34.29 -60.96 180)
					(length 5.08)
					(name "GPIO_IO53")
					(number "U26")
				)
				(pin bidirectional line
					(at 34.29 -63.5 180)
					(length 5.08)
					(name "GPIO_IO54")
					(number "U28")
				)
				(pin bidirectional line
					(at 34.29 -66.04 180)
					(length 5.08)
					(name "GPIO_IO55")
					(number "U29")
				)
				(pin bidirectional line
					(at 34.29 -71.12 180)
					(length 5.08)
					(name "GPIO_IO57")
					(number "V28")
				)
				(pin bidirectional line
					(at 34.29 -68.58 180)
					(length 5.08)
					(name "GPIO_IO56")
					(number "V29")
				)
			)
			(embedded_fonts no)
		)
)
