(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MKL02Z32V_QFN16"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MKL02Z32V_QFN16"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MKL02Z32V_QFN16"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/KL02P32M48SF0.pdf"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "48MHz Cortex-M0+ 32KB Flash Microcontroller"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MKL02Z32VFG4"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "NXP"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MICROCONTROLLER, MEMORY, FLASH, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MKL02Z32V_QFN16_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "1")
					(alternate "VREFH" power_in line)
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "VSS")
					(number "2")
					(alternate "VREFL" power_in line)
				)
				(pin bidirectional line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "PTA3")
					(number "3")
					(alternate "EXTAL0" passive line)
					(alternate "I2C0_SCL" open_collector line)
					(alternate "I2C1_SDA" open_collector line)
				)
				(pin bidirectional line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "PTA4")
					(number "4")
					(alternate "I2C0_SDA" open_collector line)
					(alternate "I2C1_SCL" open_collector line)
					(alternate "XTAL0" passive line)
				)
				(pin bidirectional line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "PTA5")
					(number "5")
					(alternate "SPI0_SS" output line)
					(alternate "TPM0_CH1" input line)
				)
				(pin bidirectional line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "PTA6")
					(number "6")
					(alternate "SPI0_MISO" input line)
					(alternate "TPM0_CH0" input line)
				)
				(pin bidirectional line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "PTA7")
					(number "7")
					(alternate "ADC0_SE7" input line)
					(alternate "IRQ_4" input line)
					(alternate "SPI0_MISO" input line)
					(alternate "SPI0_MOSI" output line)
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 2.54)
					(name "PTB0")
					(number "8")
					(alternate "ADC0_SE6" input line)
					(alternate "EXTRG_IN" input line)
					(alternate "IRQ_5" input line)
					(alternate "SPI0_SCK" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 2.54)
					(name "PTB1")
					(number "9")
					(alternate "ADC0_SE5" input line)
					(alternate "CMP0_IN3" input line)
					(alternate "IRQ_6" input line)
					(alternate "UART0_RX" input line)
					(alternate "UART0_TX" output line)
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 2.54)
					(name "PTB2")
					(number "10")
					(alternate "ADC0_SE4" input line)
					(alternate "IRQ_7" input line)
					(alternate "UART0_RX" input line)
					(alternate "UART0_TX" output line)
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 2.54)
					(name "PTB3")
					(number "11")
					(alternate "I2C0_SCL" open_collector line)
					(alternate "IRQ_10" input line)
					(alternate "UART0_TX" input line)
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "PTB4")
					(number "12")
					(alternate "I2C0_SDA" open_collector line)
					(alternate "IRQ_11" input line)
					(alternate "UART0_RX" output line)
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 2.54)
					(name "PTB5")
					(number "13")
					(alternate "ADC0_SE1" input line)
					(alternate "CMP0_IN1" input line)
					(alternate "IRQ_12" passive line)
					(alternate "TPM1_CH1" input line)
					(alternate "~{NMI}" input line)
				)
				(pin bidirectional line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "PTA0")
					(number "14")
					(alternate "ADC0_SE12" input line)
					(alternate "CMP0_IN2" input line)
					(alternate "IRQ_0" input line)
					(alternate "SWDCLK" passive line)
					(alternate "TPM1_CH0" input line)
				)
				(pin bidirectional line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "PTA1")
					(number "15")
					(alternate "IRQ_1" input line)
					(alternate "LPTMR0_ALT1" input line)
					(alternate "TPM_CLKIN0" input line)
					(alternate "~{RESET_b}" input line)
				)
				(pin bidirectional line
					(at 25.4 0 180)
					(length 2.54)
					(name "PTA2")
					(number "16")
					(alternate "CMP0_OUT" output line)
					(alternate "SWDIO" bidirectional line)
				)
			)
			(embedded_fonts no)
		)
)
