(footprint "W-PDFN-8-1EP_8x6mm_P1.27mm_EP4.3x3.4mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -0.005 -3.497 0)
		(layer "F.SilkS")
	)
	(property "Value" "W-PDFN-8-1EP_8x6mm_P1.27mm_EP4.3x3.4mm"
		(at -0.005 3.653 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -4.73 5.653 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.73 6.853 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -4.73 8.053 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.03 -1.47 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.03 -0.47 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.03 0.53 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.03 1.53 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.03 -1.47 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.03 -0.47 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.03 0.53 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.03 1.53 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.97 -1.47 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.97 -0.47 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.97 0.53 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.97 1.53 270)
		(size 0.8 0.8)
		(layers "F.Paste")
	)
	(pad "1" smd roundrect
		(at -3.905 -1.9 270)
		(size 0.45 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -3.905 -0.63 270)
		(size 0.45 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.905 0.64 270)
		(size 0.45 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.905 1.91 270)
		(size 0.45 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 3.895 1.91 270)
		(size 0.45 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 3.895 0.64 270)
		(size 0.45 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 3.895 -0.63 270)
		(size 0.45 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 3.895 -1.9 270)
		(size 0.45 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -0.005 0.005 270)
		(size 4.3 3.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0)
		(chamfer_ratio 0.1)
		(chamfer bottom_left)
	)
	(embedded_fonts no)
	(model "antmicro_mt25ql01gbbb1ew9_0sit.glb"
		(offset
			(xyz -0.755 -1.143 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 -180)
		)
	)
)
