(footprint "WDFN-8-1EP_6x5mm_P1.27mm_EP3.4x4mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -3.7 -3.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "WDFN-8-1EP_6x5mm_P1.27mm_EP3.4x4mm"
		(at -10.1 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -10.1 6 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -10.1 7.2 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -10.1 8.4 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.802 -1)
		(size 1.37 1.61)
		(layers "F.Paste")
		(roundrect_rratio 0.182482)
	)
	(pad "" smd roundrect
		(at -0.802 0.998)
		(size 1.37 1.61)
		(layers "F.Paste")
		(roundrect_rratio 0.182482)
	)
	(pad "" smd roundrect
		(at 0.8 -1)
		(size 1.37 1.61)
		(layers "F.Paste")
		(roundrect_rratio 0.182482)
	)
	(pad "" smd roundrect
		(at 0.8 0.998)
		(size 1.37 1.61)
		(layers "F.Paste")
		(roundrect_rratio 0.182482)
	)
	(pad "1" smd rect
		(at -3 -1.905 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd roundrect
		(at -3 -0.635 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3 0.633 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3 1.904 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 2.999 1.904 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 2.999 0.633 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 2.999 -0.635 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 2.999 -1.905 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd rect
		(at 0 0)
		(size 3.4 4)
		(layers "F.Cu" "F.Mask")
		(solder_paste_margin -0.1)
	)
	(embedded_fonts no)
	(model "antmicro_mt25ql256aba1ew7_0sit.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
