(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MT25QL256ABA1EW7-0SIT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 41.91 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MT25QL256ABA1EW7-0SIT"
				(at 41.91 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MT25QL256ABA1EW7-0SIT"
				(at 41.91 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.micron.com/products/nor-flash/serial-nor-flash/part-catalog/mt25ql256aba1ew7-0sit"
				(at 41.91 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Flash Memory, Serial NOR, 256 Mbit, 32M x 8bit, SPI, MLP, 8 Pins"
				(at 41.91 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MT25QL256ABA1EW7-0SIT"
				(at 41.91 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Micron Technology"
				(at 41.91 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 41.91 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 41.91 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, FLASH, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MT25QL256ABA1EW7-0SIT_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "~{CS}")
					(number "1")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "DQ1")
					(number "2")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DQ2/~{W}")
					(number "3")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DQ0")
					(number "5")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "CLK")
					(number "6")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "DQ3/~{HOLD}")
					(number "7")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
				(pin passive line
					(at 27.94 -10.16 180)
					(length 2.54)
					(name "EP")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
