(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MT25QU01GBBB8_T-PBGA-24"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MT25QU01GBBB8_T-PBGA-24"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MT25QU01GBBB8_T-PBGA-24"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/671/mict_s_a0004996076_1-2290890.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "NOR Flash SPI FLASH NOR SLC 256MX4 SOIC DDP"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MT25QU01GBBB8E12-0SIT"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Micron Technology"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, FLASH, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MT25QU01GBBB8_T-PBGA-24_1_0"
				(pin no_connect line
					(at 19.05 -11.43 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "A2")
				)
				(pin no_connect line
					(at 19.05 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "A3")
				)
				(pin no_connect line
					(at 19.05 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "A5")
				)
				(pin no_connect line
					(at 19.05 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "B1")
				)
				(pin no_connect line
					(at 19.05 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "B5")
				)
				(pin no_connect line
					(at 19.05 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "C1")
				)
				(pin no_connect line
					(at 19.05 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "C3")
				)
				(pin no_connect line
					(at 19.05 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "C5")
				)
				(pin no_connect line
					(at 19.05 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "D1")
				)
				(pin no_connect line
					(at 19.05 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "D5")
				)
				(pin no_connect line
					(at 19.05 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "E1")
				)
				(pin no_connect line
					(at 19.05 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "E2")
				)
				(pin no_connect line
					(at 19.05 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "E3")
				)
				(pin no_connect line
					(at 19.05 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "E4")
				)
				(pin no_connect line
					(at 19.05 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "E5")
				)
			)
			(symbol "MT25QU01GBBB8_T-PBGA-24_1_1"
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{RESET}")
					(number "A4")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "SCK")
					(number "B2")
				)
				(pin power_in line
					(at 21.59 -19.05 180)
					(length 2.54)
					(name "VSS")
					(number "B3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "B4")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "~{CS}")
					(number "C2")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 2.54)
					(name "~{WP}/IO2")
					(number "C4")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 2.54)
					(name "SO/IO1")
					(number "D2")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 2.54)
					(name "SI/IO0")
					(number "D3")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 2.54)
					(name "~{HOLD}/IO3")
					(number "D4")
				)
			)
			(embedded_fonts no)
		)
)
