(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MT35XU512ABA1G12-0AAT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 41.91 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MT35XU512ABA1G12-0AAT"
				(at 41.91 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MT35XU512ABA1G12-0AAT"
				(at 41.91 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.micron.com/content/dam/micron/global/secure/products/data-sheet/nor-flash/serial-nor/mt35x-xccela/die-rev-a/mt35x-qlka-u-512-aba-0.pdf"
				(at 41.91 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "NOR Flash SPI 512Mbit 8 1.8 Volts 24/25 TBGA 1 AL"
				(at 41.91 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Micron Technology"
				(at 41.91 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MT35XU512ABA1G12-0AAT"
				(at 41.91 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 41.91 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 41.91 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, DRAM, HYPERBUS, HYPERRAM, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MT35XU512ABA1G12-0AAT_1_1"
				(pin no_connect line
					(at 25.4 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "A2")
				)
				(pin passive line
					(at 27.94 -10.16 180)
					(length 2.54)
					(name "RFU")
					(number "A3")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "~{RESET}")
					(number "A4")
				)
				(pin passive line
					(at 27.94 -12.7 180)
					(length 2.54)
					(name "RFU")
					(number "A5")
				)
				(pin passive line
					(at 27.94 -15.24 180)
					(length 2.54)
					(name "RFU")
					(number "B1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "CLK")
					(number "B2")
				)
				(pin power_in line
					(at 27.94 -27.94 180)
					(length 2.54)
					(name "VSS")
					(number "B3")
				)
				(pin power_in line
					(at 27.94 0 180)
					(length 2.54)
					(name "VCC")
					(number "B4")
				)
				(pin passive line
					(at 27.94 -17.78 180)
					(length 2.54)
					(name "RFU")
					(number "B5")
				)
				(pin passive line
					(at 27.94 -27.94 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "C1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{CS}")
					(number "C2")
				)
				(pin passive line
					(at 27.94 -22.86 180)
					(length 2.54)
					(name "DQS")
					(number "C3")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "DQ2")
					(number "C4")
					(alternate "~{W}" passive line)
				)
				(pin passive line
					(at 27.94 -2.54 180)
					(length 2.54)
					(name "VPP")
					(number "C5")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "D1")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "DQ1")
					(number "D2")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DQ0")
					(number "D3")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "DQ3")
					(number "D4")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "DQ4")
					(number "D5")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "DQ7")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "DQ6")
					(number "E2")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "DQ5")
					(number "E3")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "E4")
				)
				(pin passive line
					(at 27.94 -27.94 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "E5")
				)
			)
			(embedded_fonts no)
		)
)
