(footprint "BGA-96-48_7.5x13mm_Layout9x16_P0.8mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Based on: https://www.micron.com/content/dam/micron/global/secure/products/data-sheet/dram/ddr4/8gb-auto-ddr4-dram.pdf")
	(property "Reference" "REF**"
		(at -4 -7.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-96-48_7.5x13mm_Layout9x16_P0.8mm"
		(at -4 7.85 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -4 9.05 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4 10.25 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4 11.45 0)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.5")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.9")
	)
	(pad "A1" smd circle
		(at -3.2 -6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A2" smd circle
		(at -2.4 -6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A3" smd circle
		(at -1.6 -6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A7" smd circle
		(at 1.6 -6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A8" smd circle
		(at 2.4 -6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A9" smd circle
		(at 3.2 -6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B1" smd circle
		(at -3.2 -5.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B2" smd circle
		(at -2.4 -5.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B3" smd circle
		(at -1.6 -5.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B7" smd circle
		(at 1.6 -5.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B8" smd circle
		(at 2.4 -5.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B9" smd circle
		(at 3.2 -5.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C1" smd circle
		(at -3.2 -4.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C2" smd circle
		(at -2.4 -4.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C3" smd circle
		(at -1.6 -4.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C7" smd circle
		(at 1.6 -4.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C8" smd circle
		(at 2.4 -4.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C9" smd circle
		(at 3.2 -4.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D1" smd circle
		(at -3.2 -3.6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D2" smd circle
		(at -2.4 -3.6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D3" smd circle
		(at -1.6 -3.6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D7" smd circle
		(at 1.6 -3.6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D8" smd circle
		(at 2.4 -3.6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D9" smd circle
		(at 3.2 -3.6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E1" smd circle
		(at -3.2 -2.8 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E2" smd circle
		(at -2.4 -2.8 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E3" smd circle
		(at -1.6 -2.8 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E7" smd circle
		(at 1.6 -2.8 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E8" smd circle
		(at 2.4 -2.8 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E9" smd circle
		(at 3.2 -2.8 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "F1" smd circle
		(at -3.2 -2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "F2" smd circle
		(at -2.4 -2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "F3" smd circle
		(at -1.6 -2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "F7" smd circle
		(at 1.6 -2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "F8" smd circle
		(at 2.4 -2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "F9" smd circle
		(at 3.2 -2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "G1" smd circle
		(at -3.2 -1.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "G2" smd circle
		(at -2.4 -1.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "G3" smd circle
		(at -1.6 -1.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "G7" smd circle
		(at 1.6 -1.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "G8" smd circle
		(at 2.4 -1.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "G9" smd circle
		(at 3.2 -1.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "H1" smd circle
		(at -3.2 -0.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "H2" smd circle
		(at -2.4 -0.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "H3" smd circle
		(at -1.6 -0.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "H7" smd circle
		(at 1.6 -0.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "H8" smd circle
		(at 2.4 -0.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "H9" smd circle
		(at 3.2 -0.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J1" smd circle
		(at -3.2 0.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J2" smd circle
		(at -2.4 0.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J3" smd circle
		(at -1.6 0.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J7" smd circle
		(at 1.6 0.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J8" smd circle
		(at 2.4 0.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J9" smd circle
		(at 3.2 0.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K1" smd circle
		(at -3.2 1.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K2" smd circle
		(at -2.4 1.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K3" smd circle
		(at -1.6 1.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K7" smd circle
		(at 1.6 1.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K8" smd circle
		(at 2.4 1.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K9" smd circle
		(at 3.2 1.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L1" smd circle
		(at -3.2 2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L2" smd circle
		(at -2.4 2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L3" smd circle
		(at -1.6 2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L7" smd circle
		(at 1.6 2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L8" smd circle
		(at 2.4 2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L9" smd circle
		(at 3.2 2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M1" smd circle
		(at -3.2 2.8 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M2" smd circle
		(at -2.4 2.8 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M3" smd circle
		(at -1.6 2.8 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M7" smd circle
		(at 1.6 2.8 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M8" smd circle
		(at 2.4 2.8 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M9" smd circle
		(at 3.2 2.8 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "N1" smd circle
		(at -3.2 3.6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "N2" smd circle
		(at -2.4 3.6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "N3" smd circle
		(at -1.6 3.6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "N7" smd circle
		(at 1.6 3.6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "N8" smd circle
		(at 2.4 3.6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "N9" smd circle
		(at 3.2 3.6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "P1" smd circle
		(at -3.2 4.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "P2" smd circle
		(at -2.4 4.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "P3" smd circle
		(at -1.6 4.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "P7" smd circle
		(at 1.6 4.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "P8" smd circle
		(at 2.4 4.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "P9" smd circle
		(at 3.2 4.4 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "R1" smd circle
		(at -3.2 5.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "R2" smd circle
		(at -2.4 5.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "R3" smd circle
		(at -1.6 5.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "R7" smd circle
		(at 1.6 5.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "R8" smd circle
		(at 2.4 5.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "R9" smd circle
		(at 3.2 5.2 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "T1" smd circle
		(at -3.2 6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "T2" smd circle
		(at -2.4 6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "T3" smd circle
		(at -1.6 6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "T7" smd circle
		(at 1.6 6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "T8" smd circle
		(at 2.4 6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "T9" smd circle
		(at 3.2 6 90)
		(size 0.41 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(embedded_fonts no)
	(model "antmicro_mt40a512m16td_062eaat_r.glb"
		(offset
			(xyz -0 -0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
