(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MT40A512M16TD-062EAAT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 57.912 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MT40A512M16TD-062EAAT"
				(at 57.912 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MT40A512M16TD-062EAAT"
				(at 57.912 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.micron.com/content/dam/micron/global/secure/products/data-sheet/dram/ddr4/8gb-auto-ddr4-dram.pdf"
				(at 57.912 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DDR4 SDRAM – 2Gb Memory IC, Parallel, 3200 MT/s (0.625 ns), 96-FBGA (7.5x13), 1.2V"
				(at 57.912 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Micron Technology"
				(at 57.912 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MT40A512M16TD-062EAAT:R"
				(at 57.912 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 57.912 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 57.912 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, DRAM, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MT40A512M16TD-062EAAT_1_1"
				(pin bidirectional line
					(at 40.64 -41.91 180)
					(length 5.08)
					(name "DQ8")
					(number "A3")
				)
				(pin bidirectional line
					(at 40.64 -74.93 180)
					(length 5.08)
					(name "UDQS_C")
					(number "A7")
				)
				(pin bidirectional line
					(at 40.64 -72.39 180)
					(length 5.08)
					(name "UDQS_T")
					(number "B7")
				)
				(pin bidirectional line
					(at 40.64 -44.45 180)
					(length 5.08)
					(name "DQ9")
					(number "B8")
				)
				(pin bidirectional line
					(at 40.64 -52.07 180)
					(length 5.08)
					(name "DQ12")
					(number "C2")
				)
				(pin bidirectional line
					(at 40.64 -46.99 180)
					(length 5.08)
					(name "DQ10")
					(number "C3")
				)
				(pin bidirectional line
					(at 40.64 -49.53 180)
					(length 5.08)
					(name "DQ11")
					(number "C7")
				)
				(pin bidirectional line
					(at 40.64 -54.61 180)
					(length 5.08)
					(name "DQ13")
					(number "C8")
				)
				(pin bidirectional line
					(at 40.64 -57.15 180)
					(length 5.08)
					(name "DQ14")
					(number "D3")
				)
				(pin bidirectional line
					(at 40.64 -59.69 180)
					(length 5.08)
					(name "DQ15")
					(number "D7")
				)
				(pin input line
					(at 40.64 -83.82 180)
					(length 5.08)
					(name "NF/UDM_N/_UDBI_N")
					(number "E2")
				)
				(pin input line
					(at 40.64 -81.28 180)
					(length 5.08)
					(name "NF/LDM_N/_LDBI_N")
					(number "E7")
				)
				(pin bidirectional line
					(at 40.64 -68.58 180)
					(length 5.08)
					(name "LDQS_C")
					(number "F3")
				)
				(pin bidirectional line
					(at 40.64 -24.13 180)
					(length 5.08)
					(name "DQ1")
					(number "F7")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 5.08)
					(name "ZQ")
					(number "F9")
				)
				(pin bidirectional line
					(at 40.64 -21.59 180)
					(length 5.08)
					(name "DQ0")
					(number "G2")
				)
				(pin bidirectional line
					(at 40.64 -66.04 180)
					(length 5.08)
					(name "LDQS_T")
					(number "G3")
				)
				(pin bidirectional line
					(at 40.64 -31.75 180)
					(length 5.08)
					(name "DQ4")
					(number "H2")
				)
				(pin bidirectional line
					(at 40.64 -26.67 180)
					(length 5.08)
					(name "DQ2")
					(number "H3")
				)
				(pin bidirectional line
					(at 40.64 -29.21 180)
					(length 5.08)
					(name "DQ3")
					(number "H7")
				)
				(pin bidirectional line
					(at 40.64 -34.29 180)
					(length 5.08)
					(name "DQ5")
					(number "H8")
				)
				(pin bidirectional line
					(at 40.64 -36.83 180)
					(length 5.08)
					(name "DQ6")
					(number "J3")
				)
				(pin bidirectional line
					(at 40.64 -39.37 180)
					(length 5.08)
					(name "DQ7")
					(number "J7")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "CKE")
					(number "K2")
				)
				(pin input line
					(at 0 -81.28 0)
					(length 5.08)
					(name "ODT")
					(number "K3")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "CK_T")
					(number "K7")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "CK_C")
					(number "K8")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 5.08)
					(name "WE_N/_A14")
					(number "L2")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "ACT_N")
					(number "L3")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "CS_N")
					(number "L7")
				)
				(pin input line
					(at 0 -60.96 0)
					(length 5.08)
					(name "RAS_N/_A16")
					(number "L8")
				)
				(pin input line
					(at 0 -73.66 0)
					(length 5.08)
					(name "BG0")
					(number "M2")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "A10/AP")
					(number "M3")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 5.08)
					(name "A12/BC_N")
					(number "M7")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 5.08)
					(name "CAS_N/_A15")
					(number "M8")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 5.08)
					(name "BA0")
					(number "N2")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "A4")
					(number "N3")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "A3")
					(number "N7")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 5.08)
					(name "BA1")
					(number "N8")
				)
				(pin input line
					(at 0 -83.82 0)
					(length 5.08)
					(name "TEN")
					(number "N9")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "RESET_N")
					(number "P1")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "A6")
					(number "P2")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "A0")
					(number "P3")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "A1")
					(number "P7")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "A5")
					(number "P8")
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "ALERT_N")
					(number "P9")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "A8")
					(number "R2")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "A2")
					(number "R3")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "A9")
					(number "R7")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "A7")
					(number "R8")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "A11")
					(number "T2")
				)
				(pin input line
					(at 0 -78.74 0)
					(length 5.08)
					(name "PAR")
					(number "T3")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "NF/NC")
					(number "T7")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 5.08)
					(name "A13")
					(number "T8")
				)
			)
			(symbol "MT40A512M16TD-062EAAT_2_1"
				(pin passive line
					(at 25.4 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "A1")
				)
				(pin passive line
					(at 25.4 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "VSSQ")
					(number "A2")
				)
				(pin passive line
					(at 25.4 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "VSSQ")
					(number "A8")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "A9")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VPP")
					(number "B1")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B2")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "B3")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "B9")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "C1")
				)
				(pin passive line
					(at 25.4 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "VSSQ")
					(number "C9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "D1")
				)
				(pin power_in line
					(at 25.4 -12.7 180)
					(length 5.08)
					(name "VSSQ")
					(number "D2")
				)
				(pin passive line
					(at 25.4 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "VSSQ")
					(number "D8")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "D9")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E1")
				)
				(pin passive line
					(at 25.4 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "VSSQ")
					(number "E3")
				)
				(pin passive line
					(at 25.4 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "VSSQ")
					(number "E8")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E9")
				)
				(pin passive line
					(at 25.4 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "VSSQ")
					(number "F1")
				)
				(pin power_in line
					(at 25.4 0 180)
					(length 5.08)
					(name "VDDQ")
					(number "F2")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "F8")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "G1")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "G7")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G8")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "G9")
				)
				(pin passive line
					(at 25.4 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "VSSQ")
					(number "H1")
				)
				(pin passive line
					(at 25.4 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "VSSQ")
					(number "H9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "J1")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "J2")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "J8")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "J9")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K1")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "L1")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "L9")
				)
				(pin passive line
					(at 25.4 -5.08 180)
					(length 5.08)
					(name "VREFCA")
					(number "M1")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 5.08)
					(name "VSS")
					(number "M9")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N1")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "R1")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VPP")
					(number "R9")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VDD")
					(number "T9")
				)
			)
			(embedded_fonts no)
		)
)
