(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MT41K256M16TW-107-P"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MT41K256M16TW-107-P"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MT41K256M16TW-107-P"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/6128/MT41K1G4_MT41K512M8_MT41K256M16_RevR_Sep2018.pdf"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "SDRAM - DDR3L Memory IC 4Gbit Parallel 933 MHz 20 ns 96-FBGA (8x14)"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MT41K256M16TW-107:P"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Micron Technology"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MT41K256M16TW-107-P_1_1"
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 2.54)
					(name "DQ13")
					(number "A2")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 2.54)
					(name "DQ15")
					(number "A3")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 2.54)
					(name "DQ12")
					(number "A7")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 2.54)
					(name "~{UDQS}")
					(number "B7")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 2.54)
					(name "DQ14")
					(number "B8")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 2.54)
					(name "DQ11")
					(number "C2")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 2.54)
					(name "DQ9")
					(number "C3")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 2.54)
					(name "UDQS")
					(number "C7")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 2.54)
					(name "DQ10")
					(number "C8")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 2.54)
					(name "UDM")
					(number "D3")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 2.54)
					(name "DQ8")
					(number "D7")
				)
				(pin bidirectional line
					(at 35.56 0 180)
					(length 2.54)
					(name "DQ0")
					(number "E3")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 2.54)
					(name "LDM")
					(number "E7")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 2.54)
					(name "DQ2")
					(number "F2")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 2.54)
					(name "LDQS")
					(number "F3")
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 2.54)
					(name "DQ1")
					(number "F7")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 2.54)
					(name "DQ3")
					(number "F8")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 2.54)
					(name "DQ6")
					(number "G2")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 2.54)
					(name "~{LDQS}")
					(number "G3")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 2.54)
					(name "DQ4")
					(number "H3")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 2.54)
					(name "DQ7")
					(number "H7")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 2.54)
					(name "DQ5")
					(number "H8")
				)
				(pin no_connect line
					(at 33.02 -55.88 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "J1")
				)
				(pin input line
					(at 0 -60.96 0)
					(length 2.54)
					(name "~{RAS}")
					(number "J3")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 2.54)
					(name "CK")
					(number "J7")
				)
				(pin no_connect line
					(at 33.02 -58.42 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "J9")
				)
				(pin input line
					(at 0 -71.12 0)
					(length 2.54)
					(name "ODT")
					(number "K1")
				)
				(pin input line
					(at 0 -73.66 0)
					(length 2.54)
					(name "~{CAS}")
					(number "K3")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 2.54)
					(name "~{CK}")
					(number "K7")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 2.54)
					(name "CKE")
					(number "K9")
				)
				(pin no_connect line
					(at 33.02 -60.96 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "L1")
				)
				(pin input line
					(at 0 -76.2 0)
					(length 2.54)
					(name "~{CS}")
					(number "L2")
				)
				(pin input line
					(at 0 -78.74 0)
					(length 2.54)
					(name "~{WE}")
					(number "L3")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "A10/AP")
					(number "L7")
				)
				(pin passive line
					(at 35.56 -53.34 180)
					(length 2.54)
					(name "ZQ")
					(number "L8")
				)
				(pin no_connect line
					(at 33.02 -63.5 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "L9")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "BA0")
					(number "M2")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "BA2")
					(number "M3")
				)
				(pin no_connect line
					(at 33.02 -66.04 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "M7")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "A3")
					(number "N2")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "A0")
					(number "N3")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "A12/~{BC}")
					(number "N7")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "BA1")
					(number "N8")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "A5")
					(number "P2")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "A2")
					(number "P3")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "A1")
					(number "P7")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "A4")
					(number "P8")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "A7")
					(number "R2")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "A9")
					(number "R3")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "A11")
					(number "R7")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "A6")
					(number "R8")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 2.54)
					(name "~{RESET}")
					(number "T2")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "A13")
					(number "T3")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "A14")
					(number "T7")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "A8")
					(number "T8")
				)
			)
			(symbol "MT41K256M16TW-107-P_2_1"
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDDQ")
					(number "A1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDQ")
					(number "A8")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VSS")
					(number "A9")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "VSSQ")
					(number "B1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "B2")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "B3")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "B9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDQ")
					(number "C1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDQ")
					(number "C9")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "D1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDQ")
					(number "D2")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "D8")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "D9")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "E1")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "E2")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "E8")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "E9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDQ")
					(number "F1")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "F9")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "G1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "G7")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "G8")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "G9")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VREFDQ")
					(number "H1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDQ")
					(number "H2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDQ")
					(number "H9")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "J2")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "J8")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "K2")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "K8")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "M1")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VREFCA")
					(number "M8")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "M9")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "N1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "N9")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "P1")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "P9")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "R1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "R9")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "T1")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "T9")
				)
			)
			(embedded_fonts no)
		)
)
