(footprint "FBGA-60-38_8x10mm_Layout9x11_P0.8mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -5.45 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "FBGA-60-38_8x10mm_Layout9x11_P0.8mm"
		(at -4.6 6.2 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at -4.27 -5.25 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at -4.27 -5.25 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -4.61 7.3 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.61 8.5 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -4.61 9.75 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -3.21 -4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -2.41 -4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -1.61 -4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd circle
		(at 1.59 -4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd circle
		(at 2.39 -4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at 3.19 -4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -3.21 -3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -2.41 -3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -1.61 -3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at 1.59 -3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at 2.39 -3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at 3.19 -3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -3.21 -2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -2.41 -2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -1.61 -2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C7" smd circle
		(at 1.59 -2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C8" smd circle
		(at 2.39 -2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C9" smd circle
		(at 3.19 -2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -3.21 -1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -2.41 -1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at -1.61 -1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D7" smd circle
		(at 1.59 -1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D8" smd circle
		(at 2.39 -1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D9" smd circle
		(at 3.19 -1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -3.21 -0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -2.41 -0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -1.61 -0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E7" smd circle
		(at 1.59 -0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E8" smd circle
		(at 2.39 -0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E9" smd circle
		(at 3.19 -0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -2.41 0)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at -1.61 0)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F7" smd circle
		(at 1.59 0)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F8" smd circle
		(at 2.39 0)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F9" smd circle
		(at 3.19 0)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -3.21 0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -2.41 0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G3" smd circle
		(at -1.61 0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G7" smd circle
		(at 1.59 0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G8" smd circle
		(at 2.39 0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -2.41 1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at -1.61 1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H7" smd circle
		(at 1.59 1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H8" smd circle
		(at 2.39 1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H9" smd circle
		(at 3.19 1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at -3.21 2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at -2.41 2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J3" smd circle
		(at -1.61 2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J7" smd circle
		(at 1.59 2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J8" smd circle
		(at 2.39 2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -2.41 3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K3" smd circle
		(at -1.61 3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K7" smd circle
		(at 1.59 3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K8" smd circle
		(at 2.39 3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K9" smd circle
		(at 3.19 3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L1" smd circle
		(at -3.21 4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L2" smd circle
		(at -2.41 4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L3" smd circle
		(at -1.61 4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L7" smd circle
		(at 1.59 4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L8" smd circle
		(at 2.39 4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_mt47h128m8cf_25_h.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
