(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MT47H128M8CF-25_H"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MT47H128M8CF-25_H"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MT47H128M8CF-25_H"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://octopart.com/datasheet/mt47h128m8cf-25%3Ah-micron-12414390"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DDR2 SDRAM, 16 Meg x 8 x 8 banks, VDD = +1.8V ±0.1V, VDDQ = +1.8V ±0.1V, 60-ball FBGA (8mmx10mm))"
				(at 38.1 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MT47H128M8CF-25_H"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Micron Technology"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SDRAM, MEMORY, BGA"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MT47H128M8CF-25_H_1_1"
				(pin power_in line
					(at 25.4 -55.88 180)
					(length 2.54)
					(name "V_{DD}")
					(number "A1")
				)
				(pin power_in line
					(at 25.4 -58.42 180)
					(length 2.54)
					(name "RDQS")
					(number "A2")
				)
				(pin power_in line
					(at 25.4 -60.96 180)
					(length 2.54)
					(name "V_{SS}")
					(number "A3")
				)
				(pin power_in line
					(at 25.4 -63.5 180)
					(length 2.54)
					(name "V_{SSQ}")
					(number "A7")
				)
				(pin bidirectional line
					(at 25.4 -27.94 180)
					(length 2.54)
					(name "~{DQS}")
					(number "A8")
				)
				(pin power_in line
					(at 25.4 -66.04 180)
					(length 2.54)
					(name "V_{DDQ}")
					(number "A9")
				)
				(pin bidirectional line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "DQ6")
					(number "B1")
				)
				(pin passive line
					(at 25.4 -63.5 180)
					(length 2.54)
					(hide yes)
					(name "V_{SSQ}")
					(number "B2")
				)
				(pin bidirectional line
					(at 25.4 -35.56 180)
					(length 2.54)
					(name "DM")
					(number "B3")
					(alternate "RDQS" passive line)
				)
				(pin bidirectional line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "DQS")
					(number "B7")
				)
				(pin passive line
					(at 25.4 -63.5 180)
					(length 2.54)
					(hide yes)
					(name "V_{SSQ}")
					(number "B8")
				)
				(pin bidirectional line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "DQ7")
					(number "B9")
				)
				(pin passive line
					(at 25.4 -66.04 180)
					(length 2.54)
					(hide yes)
					(name "V_{DDQ}")
					(number "C1")
				)
				(pin bidirectional line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "DQ1")
					(number "C2")
				)
				(pin passive line
					(at 25.4 -66.04 180)
					(length 2.54)
					(hide yes)
					(name "V_{DDQ}")
					(number "C3")
				)
				(pin passive line
					(at 25.4 -66.04 180)
					(length 2.54)
					(hide yes)
					(name "V_{DDQ}")
					(number "C7")
				)
				(pin bidirectional line
					(at 25.4 0 180)
					(length 2.54)
					(name "DQ0")
					(number "C8")
				)
				(pin passive line
					(at 25.4 -66.04 180)
					(length 2.54)
					(hide yes)
					(name "V_{DDQ}")
					(number "C9")
				)
				(pin bidirectional line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "DQ4")
					(number "D1")
				)
				(pin passive line
					(at 25.4 -63.5 180)
					(length 2.54)
					(hide yes)
					(name "V_{SSQ}")
					(number "D2")
				)
				(pin bidirectional line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "DQ3")
					(number "D3")
				)
				(pin bidirectional line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "DQ2")
					(number "D7")
				)
				(pin passive line
					(at 25.4 -63.5 180)
					(length 2.54)
					(hide yes)
					(name "V_{SSQ}")
					(number "D8")
				)
				(pin bidirectional line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "DQ5")
					(number "D9")
				)
				(pin power_in line
					(at 25.4 -53.34 180)
					(length 2.54)
					(name "V_{DDL}")
					(number "E1")
				)
				(pin power_in line
					(at 25.4 -50.8 180)
					(length 2.54)
					(name "V_{REF}")
					(number "E2")
				)
				(pin passive line
					(at 25.4 -60.96 180)
					(length 2.54)
					(hide yes)
					(name "V_{SS}")
					(number "E3")
				)
				(pin power_in line
					(at 25.4 -68.58 180)
					(length 2.54)
					(name "V_{SSDL}")
					(number "E7")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 2.54)
					(name "CK")
					(number "E8")
				)
				(pin passive line
					(at 25.4 -55.88 180)
					(length 2.54)
					(hide yes)
					(name "V_{DD}")
					(number "E9")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 2.54)
					(name "CKE")
					(number "F2")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 2.54)
					(name "~{WE}")
					(number "F3")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 2.54)
					(name "~{RAS}")
					(number "F7")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 2.54)
					(name "~{CK}")
					(number "F8")
				)
				(pin input line
					(at 0 -60.96 0)
					(length 2.54)
					(name "ODT")
					(number "F9")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 2.54)
					(name "BA2")
					(number "G1")
				)
				(pin input line
					(at 0 -41.91 0)
					(length 2.54)
					(name "BA0")
					(number "G2")
				)
				(pin input line
					(at 0 -44.45 0)
					(length 2.54)
					(name "BA1")
					(number "G3")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 2.54)
					(name "~{CAS}")
					(number "G7")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 2.54)
					(name "~{CS}")
					(number "G8")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "A10")
					(number "H2")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "A1")
					(number "H3")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "A2")
					(number "H7")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "A0")
					(number "H8")
				)
				(pin passive line
					(at 25.4 -55.88 180)
					(length 2.54)
					(hide yes)
					(name "V_{DD}")
					(number "H9")
				)
				(pin passive line
					(at 25.4 -60.96 180)
					(length 2.54)
					(hide yes)
					(name "V_{SS}")
					(number "J1")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "A3")
					(number "J2")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "A5")
					(number "J3")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "A6")
					(number "J7")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "A4")
					(number "J8")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "A7")
					(number "K2")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "A9")
					(number "K3")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "A11")
					(number "K7")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "A8")
					(number "K8")
				)
				(pin passive line
					(at 25.4 -60.96 180)
					(length 2.54)
					(hide yes)
					(name "V_{SS}")
					(number "K9")
				)
				(pin passive line
					(at 25.4 -55.88 180)
					(length 2.54)
					(hide yes)
					(name "V_{DD}")
					(number "L1")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "A12")
					(number "L2")
				)
				(pin passive line
					(at 25.4 -40.64 180)
					(length 2.54)
					(name "RFU")
					(number "L3")
				)
				(pin passive line
					(at 25.4 -43.18 180)
					(length 2.54)
					(name "RFU")
					(number "L7")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "A13")
					(number "L8")
				)
			)
			(embedded_fonts no)
		)
)
