(footprint "BGA-82_11x9mm_Layout13x11_P0.8mm_DDR5_MO-210-AN"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -6.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-82_11x9mm_Layout13x11_P0.8mm_DDR5_MO-210-AN"
		(at -14.94 6.93 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "."
		(at -4.54 -5.83 0)
		(layer "F.SilkS")
	)
	(fp_text user "Author: Antmicro"
		(at -4.622 8.699 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -4.622 9.899 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.622 11.099 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -4 -4.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -3.202 -4.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -2.4 -4.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at -1.601 -4.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd circle
		(at 1.6 -4.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at 2.398 -4.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd circle
		(at 3.2 -4.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd circle
		(at 3.999 -4.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -3.202 -4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -2.4 -4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at -1.601 -4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at 1.6 -4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at 2.398 -4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd circle
		(at 3.2 -4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -3.202 -3.202)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -2.4 -3.202)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at -1.601 -3.202)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C8" smd circle
		(at 1.6 -3.202)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C9" smd circle
		(at 2.398 -3.202)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C10" smd circle
		(at 3.2 -3.202)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -3.202 -2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at -2.4 -2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at -1.601 -2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D8" smd circle
		(at 1.6 -2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D9" smd circle
		(at 2.398 -2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D10" smd circle
		(at 3.2 -2.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -3.202 -1.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -2.4 -1.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at -1.601 -1.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E8" smd circle
		(at 1.6 -1.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E9" smd circle
		(at 2.398 -1.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E10" smd circle
		(at 3.2 -1.601)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -3.202 -0.804)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at -2.4 -0.804)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at -1.601 -0.804)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F8" smd circle
		(at 1.6 -0.804)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F9" smd circle
		(at 2.398 -0.804)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F10" smd circle
		(at 3.2 -0.804)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -3.202 0)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G3" smd circle
		(at -2.4 0)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G4" smd circle
		(at -1.601 0)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G8" smd circle
		(at 1.6 0)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G9" smd circle
		(at 2.398 0)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G10" smd circle
		(at 3.2 0)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -3.202 0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at -2.4 0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at -1.601 0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H8" smd circle
		(at 1.6 0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H9" smd circle
		(at 2.398 0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H10" smd circle
		(at 3.2 0.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at -3.202 1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J3" smd circle
		(at -2.4 1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J4" smd circle
		(at -1.601 1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J8" smd circle
		(at 1.6 1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J9" smd circle
		(at 2.398 1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J10" smd circle
		(at 3.2 1.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -3.202 2.398)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K3" smd circle
		(at -2.4 2.398)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K4" smd circle
		(at -1.601 2.398)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K8" smd circle
		(at 1.6 2.398)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K9" smd circle
		(at 2.398 2.398)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K10" smd circle
		(at 3.2 2.398)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L2" smd circle
		(at -3.202 3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L3" smd circle
		(at -2.4 3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L4" smd circle
		(at -1.601 3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L8" smd circle
		(at 1.6 3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L9" smd circle
		(at 2.398 3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L10" smd circle
		(at 3.2 3.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M2" smd circle
		(at -3.202 3.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M3" smd circle
		(at -2.4 3.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M4" smd circle
		(at -1.601 3.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M8" smd circle
		(at 1.6 3.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M9" smd circle
		(at 2.398 3.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M10" smd circle
		(at 3.2 3.999)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N1" smd circle
		(at -4 4.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N2" smd circle
		(at -3.202 4.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N3" smd circle
		(at -2.4 4.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N4" smd circle
		(at -1.601 4.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N8" smd circle
		(at 1.6 4.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N9" smd circle
		(at 2.398 4.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N10" smd circle
		(at 3.2 4.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N11" smd circle
		(at 3.999 4.799)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_mt60b2g8hb_48b_a.glb"
		(offset
			(xyz -4.5 5.5 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 90)
		)
	)
)
